{"text_format":"1","workbook":"xlsx","n_sheets":9,"sheets":["Content","Lens","IP Cameras & NVR","Analog Cameras & DVR","Monitors","Thermal & Low Light","Raytec","Videotec","NVT"],"not_rendered":{"charts":0,"images":82,"macros":1,"external_links":0,"defined_names":10,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Content","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[[0,0,0,4],[3,2,3,4],[4,2,4,4],[41,1,41,3],[9,1,9,3],[11,1,11,3],[25,1,25,3],[17,1,17,3],[28,2,28,5]]}
[]
[]
[]
[null,null,"Gültig ab 01.02.2017 v1.0",null,null,null,"Rabatt:",0]
[null,null,"Änderungen und Irrtümer vorbehalten."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"NEUE PRODUKTE / PREIS markiert"]
[]
[null,"Diese Preisliste ist gültig ab 01.02.2017. Alle vorherigen Preislisten verlieren ihre Gültigkeit."]
[null,"Alle Preisangaben sind unverbindliche Endverbraucherpreise in EUR zzgl. der gesetzlichen  MwSt. "]
[null,"Alle Rechtsgeschäfte basieren auf den CBC (Europe) GmbH \"Allgemeinen Leistungs- und Lieferbedingungen\"."]

{"sheet":"Lens","index":1,"n_rows":312,"n_cols":8,"rows_kept":312,"cut":false,"hidden":false,"merged":[[255,0,255,2]]}
["Objektive",null,"     ",null,null,null,"     "]
[]
[]
[null,"Modell","Beschreibung","EURO"]
["CCTV"]
["Megapixelobjektive"]
["Manuelle Blende",null,"     "]
[null,"A3Z2812CS-MPWIR"," 2,8 - 8,5mm, 1.2, 1/2.7\",  CS, IR, 5 Megapixel",180]
[null,"A4Z1214CS-MPIR"," 12,5 - 50mm, 1.4 - 16C, 1/2.7\",  CS, IR, 3 Megapixel",240]
[null,"A4Z2812CS-MPIR","2,8 - 10,0mm, 1.2, 1/2.7\", CS, IR, 3 Megapixel",140]
[null,"A6Z8516CS-MP","8,5 - 50mm, F1,6 - F16C, 1/2.7\", CS, 3 Megapixel",130]
[null,"E3Z4518CS-MPIR","4.5 mm - 13.2, 1.8 - 16C, 1/1.8\", CS, IR, 5 Megapixel",350]
[null,"H2Z0414C-MP"," 4,0 – 8,0 mm, 1,4 – 16C, 1/2'’, C, Megapixel",150]
[null,"H5Z2518C-MP"," 25,0 - 135 mm, 1,8 - 16C, 1/2\", C, 3 Megapixel",440]
[null,"M3Z1228С-MP"," 12,0 - 36,0 mm, 2,8 – 16C, 2/3\", C, Megapixel",280]
["DC-Blende",null,"     "]
[null,"AG3Z2812FCS-MPWIR"," 2,8 - 8,5mm, 1.2, 1/2.7\",  CS, IR, 5 Megapixel",160]
[null,"AG4Z1214FCS-MPIR","12,5 - 50 mm, 1.4 - 360C, 1/2.7\", CS, IR-corrected, 3 Megapixel",240]
[null,"AG4Z2812FCS-MPIR","2,8 - 10,0mm, 1.2, 1/2.7\", CS, IR-corrected, 3 Megapixel",110]
[null,"AG6Z8516FCS-MP","8,5 - 50mm, F1,6 - F16C, 1/2.7\", CS, 3 Megapixel",130]
[null,"HG2Z0414FC-MP"," 4.0 - 8.0mm, F1.4 Megapixel, CS",170]
[null,"HG5Z2518FC-MP","25,0 - 135 mm, 1,8 - 360C, 1/2\", C, 3 Megapixel",450]
[null,"MG3Z1228FC-MP","12,0 - 36,0 mm, 2,8 - 360C, 2/3\", C, Megapixel",340]
[null,"MG1616FC-MP","16mm,  F1.6, 2/3\", C, 5 Megapixel",470]
[null,"MG2514FC-MP","25,0mm, F1.4, DC-iris, 2/3\", C, 5 Megapixel",470]
[null,"MG2514FC-MPIR","25,0mm, 2/3\", C, F1.4, DC-iris, IR-corrected, 5 Megapixel",700]
[null,"MG3518FC-MPIR","35,0 mm, 1,8, 2/3\", C, IR-corrected, 5 Megapixel",690]
[null,"MG5020FC-MPIR","50,0 mm, 2,0, 2/3\", C, IR-corrected, 5 Megapixel",710]
["P-Iris",null,"     "]
[null,"AG3Z2812KCS-MPWIR"," 2,8 - 8,5mm, 1.2, 1/2.7\",  P-Iris, CS, IR, 5 Megapixel",200]
[null,"AG4Z1214KCS-MPIR","12,5 - 50,0 mm, F1,4 - 16C, P-Iris, 1/2.7\", CS, IR-corrected, 3 Megapixel",270]
[null,"AG4Z2812KCS-MPIR","2,8 - 10mm, F1,4 - F16C, P-Iris,  1/2.7\", CS, IR-corrected, 3 Megapixel",180]
[null,"AG6Z8516KCS-MP","8,5 - 50mm, F1,6 - F16C, P-Iris, 1/2.7\", CS, 3 Megapixel",160]
[null,"MG2514KC-MPIR-V31","25,0mm, 2/3\", C, F1.4, P-iris, IR-corrected, 5 Megapixel",740]
[null,"MG3518KC-MPIR-V31","35,0mm, 2/3\", C, F1.8, P-iris, IR-corrected, 5 Megapixel",730]
[null,"MG5020KC-MPIR-V31","50,0mm, 2/3\", C, F2.0, P-iris, IR-corrected, 5 Megapixel",750]
["Standard\nManuelle Blende",null,null,null,null,null,"     "]
[null,"T2314FICS"," 2.3 mm 1.4 – 16C 1/3\" CS ",160,null,"T2314FICS"," 2,3 mm, 1,4 – 16C 1/3\", CS ",160]
[null,"T2616FICS"," 2.6 mm 1.6 – 11C 1/3\" CS ",104,null,"T2616FICS"," 2,6 mm, 1,6 – 11C 1/3\", CS ",104]
[null,"T2625CS-P"," 2.6 mm 2.5 – 32C 1/3\" CS, Pinhole",368,null,"T2625CS-P"," 2,6 mm, 2,5 – 32C 1/3\" , CS, P",368]
[null,"T0412FICS"," 4.0 mm 1.2 – 16C 1/3\" CS ",55,null,"T0412FICS"," 4,0 mm, 1,2 – 16C 1/3\", CS ",55]
[null,"T0812FICS"," 8.0 mm 1.2 – 16C 1/3\" CS ",53,null,"T0812FICS"," 8,0 mm, 1,2 – 16C 1/3\", CS ",53]
[null,"H1214FICS"," 12.0 mm 1.4 – 16C 1/2\" CS ",74,null,"H1214FICS"," 12,0 mm, 1,4 – 16C 1/2\", CS ",74]
["DC-Blende",null,"     "]
[null,"TG2314FCS"," 2.3 mm 1.4 – 360C 1/3\" CS ",191,null,"TG2314FCS"," 2,3 mm, 1,4 – 360C, 1/3\", CS ",191]
[null,"TG2616FCS"," 2.6 mm 1.6 – 360C 1/3\" CS ",144,null,"TG2616FCS"," 2,6 mm, 1,6 – 360C, 1/3\", CS ",144]
[null,"TG2625FCS-P"," 2.6 mm 2.5 – 360C 1/3\" CS, Pinhole",518,null,"TG2625FCS-P"," 2,6 mm, 2,5 – 360C, 1/3\", CS, P",518]
[null,"TG0412FCS"," 4.0 mm 1.2 – 360C 1/3\" CS ",99,null,"TG0412FCS"," 4,0 mm, 1,2 – 360C, 1/3\", CS ",99]
[null,"TG0812FCS"," 8.0 mm 1.2 – 360C 1/3\" CS ",92,null,"TG0812FCS"," 8,0 mm, 1,2 – 360C, 1/3\", CS ",92]
[null,"HG1214FCS"," 12.0 mm 1.4 – 360C 1/2\" CS ",116,null,"HG1214FCS"," 12,0 mm, 1,4 – 360C, 1/2\", CS ",116]
["Video-Blende",null,"     ",null,null,null,"     "]
[null,"TG2314AFCS"," 2.3 mm 1.4 – 360C 1/3\" CS ",227,null,"TG2314AFCS"," 2,3 mm, 1,4 – 360C, 1/3\", CS ",227]
[null,"TG2616AFCS"," 2.6 mm 1.6 – 360C 1/3\" CS ",174,null,"TG2616AFCS"," 2,6 mm, 1,6 – 360C, 1/3\", CS ",174]
[null,"TG2625AFCS-P"," 2.6 mm 2.5 – 360C 1/3\" CS, Pinhole",553,null,"TG2625AFCS-P"," 2,6 mm, 2,5 – 360C, 1/3\", CS, P",553]
[null,"HG1214AFCS"," 12.0 mm 1.4 – 360C 1/2\" CS ",139,null,"HG1214AFCS"," 12,0 mm, 1,4 – 360C, 1/2\", CS ",139]
["Manuelle Vario-Objektive",null,"     ",null,null,null,"     "]
[null,"T2Z1816CS"," 1,8 - 3,6 mm 1,6 – 16C 1/3\" CS ",212,null,"T2Z1816CS"," 1,8 - 3,6 mm, 1,6 – 16C, 1/3\", CS ",212]
[null,"T3Z2910CS"," 2,9 – 8,2 mm 1,0 – 16C 1/3’’ CS ASP",50,null,"T3Z2910CS"," 2,9 – 8,2 mm, 1,0 – 16C, 1/3’’, CS, ASP",50]
[null,"T3Z2910CS-IR"," 2,9 – 8,2 mm 1,0 – 16C 1/3’’ CS IR ASP",60,null,"T3Z2910CS-IR"," 2,9 – 8,2 mm, 1,0 – 16C, 1/3’’, CS, IR, ASP",60]
[null,"T3Z3510CS"," 3,5 - 10,5 mm 1,0 – 16C 1/3\" CS ASP",87,null,"T3Z3510CS"," 3,5 - 10,5 mm, 1,0 – 16C, 1/3\", CS, ASP",87]
[null,"T3Z3510CS-IR"," 3,5 - 10,5 mm 1,0 – 16C 1/3\" CS IR, ASP",107,null,"T3Z3510CS-IR"," 3,5 - 10,5 mm, 1,0 – 16C, 1/3\", CS, IR, ASP",107]
[null,"T4Z2813CS-IR"," 2,8 – 12,0 mm 1,3 – 16C 1/3’’ CS IR, ASP",70,null,"T4Z2813CS-IR"," 2,8 – 12,0 mm, 1,3 – 16C, 1/3’’, CS, IR, ASP",70]
[null,"T5Z8513CS-IR"," 8,5 - 40,0 mm 1,3 – 16C 1/3\" CS IR, ASP",158,null,"T5Z8513CS-IR"," 8,5 - 40,0 mm, 1,3 – 16C, 1/3\", CS, IR, ASP",158]
[null,"T10Z0513CS"," 5,0 - 50,0 mm 1,3 – 16C 1/3\" CS ASP",98,null,"T10Z0513CS"," 5,0 - 50,0 mm, 1,3 – 16C, 1/3\", CS, ASP",98]
[null,"H2Z4516CS"," 4,5 - 10,0 mm 1,6 – 16C 1/2\" CS ",99,null,"H2Z4516CS"," 4,5 - 10,0 mm, 1,6 – 16C, 1/2\", CS ",99]
[null,"H3Z4512CS-IR"," 4,5 - 12,5 mm 1,2 – 16C 1/2\" CS IR, ASP",138,null,"H3Z4512CS-IR"," 4,5 - 12,5 mm, 1,2 – 16C, 1/2\", CS, IR, ASP",138]
[null,"H3Z1014CS"," 10,0 - 30,0 mm 1,4 – 16C 1/2\" CS Flat, ASP",211,null,"H3Z1014CS"," 10,0 - 30,0 mm, 1,4 – 16C, 1/2\", CS, Flat, ASP",211]
["Manuelle Objektive mit DC-Blende",null,"     "]
[null,"TG2Z1816FCS"," 1.8 – 3.6 mm 1.6 – 360C 1/3\" CS ",261,null,"TG2Z1816FCS"," 1,8 - 3,6 mm, 1,6 – 360C, 1/3\", CS ",261]
[null,"TG3Z2910FCS"," 2.9 – 8.2 mm 1.0 – 360C 1/3’’ CS ASP",55,null,"TG3Z2910FCS"," 2,9 – 8,2 mm, 1,0 – 360C, 1/3’’, CS, ASP",55]
[null,"TG3Z2910FCS-IR"," 2.9 – 8.2 mm 1.0 – 360C 1/3’’ CS IR, ASP",65,null,"TG3Z2910FCS-IR"," 2,9 – 8,2 mm, 1,0 – 360C 1/3’’ CS, IR, ASP",65]
[null,"TG3Z3510FCS "," 3.5 – 10.5 mm 1.0 – 360C 1/3\" CS ",98,null,"TG3Z3510FCS "," 3,5 - 10,5 mm, 1,0 – 360C, 1/3\", CS ",98]
[null,"TG3Z3510FCS-IR"," 3.5 – 10.5 mm 1.0 – 360C 1/3\" CS IR, ASP",118,null,"TG3Z3510FCS-IR"," 3,5 - 10,5 mm, 1,0 – 360C, 1/3\", CS, IR, ASP",118]
[null,"TG4Z2813FCS-IR"," 2.8 – 12.0 mm 1.3 – 360C 1/3’’ CS IR, ASP",85,null,"TG4Z2813FCS-IR"," 2,8 – 12,0 mm, 1,3 – 360C, 1/3’’, CS, IR, ASP",85]
[null,"TG5Z8513FCS-IR "," 8.5 – 40.0 mm 1.3 – 360 1/3\" CS IR, ASP",158,null,"TG5Z8513FCS-IR "," 8,5 - 40,0 mm, 1,3 – 360, 1/3\", CS, IR, ASP",158]
[null,"TG10Z0513FCS"," 5.0 – 50.0 mm 1.3 – 360C 1/3\" CS ASP",100,null,"TG10Z0513FCS"," 5,0 - 50,0 mm, 1,3 – 360C, 1/3\", CS, ASP",100]
[null,"HG2Z4516FCS"," 4.5 – 10.0 mm 1.6 – 360C 1/2\" CS ",138,null,"HG2Z4516FCS"," 4,5 - 10,0 mm, 1,6 – 360C, 1/2\", CS ",138]
[null,"HG3Z4512FCS-IR"," 4.5 – 12.5 mm 1.2 – 360 1/2\" CS IR, ASP",175,null,"HG3Z4512FCS-IR"," 4,5 - 12,5 mm, 1,2 – 360, 1/2\", CS, IR, ASP",175]
[null,"HG3Z1014FCS"," 10.0 – 30.0 mm 1.4 – 360C 1/2\" CS Flat ASP",272,null,"HG3Z1014FCS"," 10,0 - 30,0 mm, 1,4 – 360C, 1/2\", CS, Flat, ASP",272]
["Manuelle Objektive mit Video-Blende",null,"     "]
[null,"TG2Z1816AFCS"," 1.8 – 3.6 mm 1.6 – 360C 1/3\" CS ",275,null,"TG2Z1816AFCS"," 1,8 - 3,6 mm, 1,6 – 360C, 1/3\", CS ",275]
[null,"TG3Z2910AFCS"," 2.9 – 8.2 mm 1.0 – 360C 1/3’’ CS ASP",78,null,"TG3Z2910AFCS"," 2,9 – 8,2 mm, 1,0 – 360C, 1/3’’, CS, ASP",78]
[null,"TG3Z2910AFCS-IR"," 2.9 – 8.2 mm 1.0 – 360C 1/3’’ CS IR, ASP",88,null,"TG3Z2910AFCS-IR"," 2,9 – 8,2 mm, 1,0 – 360C, 1/3’’, CS, IR, ASP",88]
[null,"TG3Z3510AFCS"," 3.5 – 10.5 mm 1.0 – 360C 1/3\" CS ASP",131,null,"TG3Z3510AFCS"," 3,5 - 10,5 mm, 1,0 – 360C, 1/3\", CS, ASP",131]
[null,"TG3Z3510AFCS-IR"," 3.5 – 10.5 mm 1.0 – 360C 1/3\" CS IR, ASP",151,null,"TG3Z3510AFCS-IR"," 3,5 - 10,5 mm, 1,0 – 360C, 1/3\", CS, IR, ASP",151]
[null,"TG4Z2813AFCS-IR"," 2.8 – 12.0 mm 1.3 – 360C 1/3’’ CS IR, ASP",118,null,"TG4Z2813AFCS-IR"," 2,8 – 12,0 mm, 1,3 – 360C, 1/3’’, CS, IR, ASP",118]
[null,"TG5Z8513AFCS-IR"," 8.5 – 40.0 mm 1.3 – 360 1/3\" CS IR, ASP",228,null,"TG5Z8513AFCS-IR"," 8,5 - 40,0 mm, 1,3 – 360, 1/3\", CS, IR, ASP",228]
[null,"TG10Z0513AFCS"," 5.0 – 50.0 mm 1.3 – 360C 1/3\" CS ASP",131,null,"TG10Z0513AFCS"," 5,0 - 50,0 mm, 1,3 – 360C, 1/3\", CS, ASP",131]
[null,"HG2Z4516AFCS"," 4.5 – 10.0 mm 1.6 – 360C 1/2\" CS ",154,null,"HG2Z4516AFCS"," 4,5 - 10,0 mm, 1,6 – 360C, 1/2\", CS ",154]
[null,"HG3Z4512AFCS-IR"," 4.5 – 12.5 mm 1.2 – 360 1/2\" CS IR, ASP",187,null,"HG3Z4512AFCS-IR"," 4,5 - 12,5 mm, 1,2 – 360, 1/2\", CS, IR, ASP",187]
[null,"HG3Z1014AFCS"," 10.0 - 30.0 mm 1.4 – 360C 1/2\" CS Flat ASP",284,null,"HG3Z1014AFCS"," 10,0 - 30,0 mm, 1,4 – 360C, 1/2\", CS, Flat, ASP",284]
["Manuelle Zoom-Objektive",null,"     ",null,null,null,"     "]
[null,"H6Z0812"," 8.0 – 48.0 mm 1.2 – 16C 1/2\" C ",432,null,"H6Z0812"," 8,0 - 48,0 mm, 1,2 – 16C, 1/2\", C ",432]
[null,"M6Z1212"," 12.5 – 75.0 mm 1.2 – 16C 2/3\" C ",432,null,"M6Z1212"," 12,5 - 75,0 mm, 1,2 – 16C, 2/3\", C ",432]
["Zoom-Objektive mit DC-Blende",null,"     "]
[null,"T6Z5710AIDC-CS"," 5.7 – 34.2 mm 1.0 – 360C 1/3\" CS ",480,null,"T6Z5710AIDC-CS"," 5,7 - 34,2 mm, 1,0 – 360C, 1/3\", CS ",480]
[null,"H6Z0812AIDC"," 8.0 – 48.0 mm 1.2 – 560C 1/2\" C  ",456,null,"H6Z0812AIDC"," 8,0 - 48,0 mm, 1,2 – 560C, 1/2\", C  ",456]
["Zoom-Objektive mit Video-Blende",null,"     ",null,null,"T6Z5710AIVD-CS"," 5,7 - 34,2 mm, 1,0 – 360C, 1/3\", CS ",528]
[null,"T6Z5710AIVD-CS"," 5.7 – 34.2 mm 1.0 – 360C 1/3\" CS ",528,null,"H6Z0812AIVD"," 8,0 - 48,0 mm, 1,2 – 560C, 1/2\", C  ",504]
[null,"H6Z0812AIVD"," 8.0 – 48.0 mm 1.2 – 560C 1/2\" C  ",504,null,null,"     "]
["Motorisierte Zoom-Objektive",null,"     ",null,null,"T6Z5710M-CS"," 5,7 - 34,2 mm, 1,0 – 16C, 1/3\", CS ",612]
[null,"T6Z5710M-CS"," 5,7 - 34,2 mm, 1,0 – 16C, 1/3\", CS ",612,null,"T6Z5710MS-CS"," 5,7 - 34,2 mm, 1,0 – 360C, 1/3\", CS ",636]
[null,"T6Z5710MS-CS"," 5,7 - 34,2 mm, 1,0 – 360C, 1/3\", Spot Filter, CS ",636,null,"T6Z5710MP-CS"," 5,7 - 34,2 mm, 1,0 – 16C, 1/3\", CS ",804]
[null,"T6Z5710MP-CS"," 5,7 - 34,2 mm, 1,0 – 16C, 1/3\", Preset, CS ",804,null,"T6Z5710MSP-CS"," 5,7 - 34,2 mm, 1,0 – 360C, 1/3\", CS ",828]
[null,"T6Z5710MSP-CS"," 5,7 - 34,2 mm, 1,0 – 360C, 1/3\", Spot Filter, Preset, CS ",828,null,"T6Z5710AMS-CS"," 5,7 - 34,2 mm, 1,0 – 360C, 1/3\", CS ",660]
[null,"T6Z5710AMS-CS"," 5,7 - 34,2 mm, 1,0 – 360C, 1/3\", Spot Filter, CS ",660,null,"T6Z5710AMSP-CS"," 5,7 - 34,2 mm, 1,0 – 360C, 1/3\", CS ",864]
[null,"T6Z5710AMSP-CS"," 5,7 - 34,2 mm, 1,0 – 360C, 1/3\", Video Auto Iris, Spot Filter, Prest, CS ",864,null,"T6Z5710DC-CS"," 5,7 - 34,2 mm, 1,0 – 360C, 1/3\", CS ",624]
[null,"T6Z5710DC-CS"," 5,7 - 34,2 mm, 1,0 – 360C, 1/3\", DC Auto Iris, CS ",624,null,"T6Z5710PDC-CS"," 5,7 - 34,2 mm, 1,0 – 360C, 1/3\", CS ",740]
[null,"T6Z5710PDC-CS"," 5,7 - 34,2 mm, 1,0 – 360C, 1/3\", Preset, DC Auto Iris, CS ",740,null,"T10Z5712M-CS"," 5,7 - 57,0 mm, 1,2 – 22C, 1/3\", CS ",732]
[null,"T10Z5712M-CS"," 5,7 - 57,0 mm, 1,2 – 22C, 1/3\", CS ",732,null,"T10Z5712MS-CS"," 5,7 - 57,0 mm, 1,2 – 560C, 1/3\", CS ",768]
[null,"T10Z5712MS-CS"," 5,7 - 57,0 mm, 1,2 – 560C, 1/3\", Spot Filter, CS ",768,null,"T10Z5712MP-CS"," 5,7 - 57,0 mm, 1,2 – 22C, 1/3\", CS ",972]
[null,"T10Z5712MP-CS"," 5,7 - 57,0 mm, 1,2 – 22C, 1/3\", Preset, CS ",972,null,"T10Z5712MSP-CS"," 5,7 - 57,0 mm, 1,2 – 560C, 1/3\", CS ",1008]
[null,"T10Z5712MSP-CS"," 5,7 - 57,0 mm, 1,2 – 560C, 1/3\", Spot Filter, Preset, CS ",1008,null,"T10Z5712AMS-CS"," 5,7 - 57,0 mm, 1,2 – 560C,  1/3\", CS ",792]
[null,"T10Z5712AMS-CS"," 5,7 - 57,0 mm, 1,2 – 560C,  1/3\", Video Auto Iris, Spot Filter, CS ",792,null,"T10Z5712AMSP-CS"," 5,7 - 57,0 mm, 1,2 – 560C, 1/3\", CS ",1032]
[null,"T10Z5712AMSP-CS"," 5,7 - 57,0 mm, 1,2 – 560C, 1/3\", Video Auto Iris, Spot Filter, Preset, CS ",1032,null,"T10Z5712DC-CS"," 5,7 - 57,0 mm, 1,2 – 560C, 1/3\", CS ",726]
[null,"T10Z5712DC-CS"," 5,7 - 57,0 mm, 1,2 – 560C, 1/3\", DC Auto Iris, CS ",650,null,"T10Z5712PDC-CS"," 5,7 - 57,0 mm, 1,2 – 560C, 1/3\", CS ",907]
[null,"T10Z5712PDC-CS"," 5,7 - 57,0 mm, 1,2 – 560C, 1/3\", Preset, DC Auto Iris, CS ",800,null,"T21Z5816M-CS"," 5,8 - 121,8 mm, 1,6 – 22C, 1/3\", CS ",1248]
[null,"T21Z5816M-CS"," 5,8 - 121,8 mm, 1,6 – 22C, 1/3\", CS ",1248,null,"T21Z5816MS-CS"," 5,8 - 121,8 mm, 1,6 – 560C, 1/3\", CS ",1272]
[null,"T21Z5816MS-CS"," 5,8 - 121,8 mm, 1,6 – 560C, 1/3\", Spot Filter, CS ",1272,null,"T21Z5816MP-CS"," 5,8 - 121,8 mm, 1,6 – 22C, 1/3\", CS ",1464]
[null,"T21Z5816MP-CS"," 5,8 - 121,8 mm, 1,6 – 22C, 1/3\", Preset, CS ",1464,null,"T21Z5816MSP-CS"," 5,8 - 121,8 mm, 1,6 – 560C, 1/3\", CS ",1500]
[null,"T21Z5816MSP-CS"," 5,8 - 121,8 mm, 1,6 – 560C, 1/3\", Spot Filter, Preset, CS ",1500,null,"T21Z5816AMS-CS"," 5,8 - 121,8 mm, 1,6 – 560C, 1/3\", CS ",1260]
[null,"T21Z5816AMS-CS"," 5,8 - 121,8 mm, 1,6 – 560C, 1/3\", Video Auto Iris, CS ",1260,null,"T21Z5816AMSP-CS"," 5,8 - 121,8 mm, 1,6 – 560C, 1/3\", CS ",1524]
[null,"T21Z5816AMSP-CS"," 5,8 - 121,8 mm, 1,6 – 560C, 1/3\", Video Auto Iris, Spot Filter, Preset, CS ",1524,null,"T21Z5816DC-CS"," 5,8 - 121,8 mm, 1,6 – 560C, 1/3\", CS ",1224]
[null,"T21Z5816DC-CS"," 5,8 - 121,8 mm, 1,6 – 560C, 1/3\", DC Auto Iris, CS ",1200,null,"T21Z5816PDC-CS"," 5,8 - 121,8 mm, 1,6 – 560C, 1/3\", CS ",1488]
[null,"T21Z5816PDC-CS"," 5,8 - 121,8 mm, 1,6 – 560C, 1/3\", Preset, DC Auto Iris, CS ",1350,null,"T34Z5518AMS-CS"," 5,5 - 187,0 mm, 1,8 – 560C, 1/3\", CS ",1704]
[null,"T34Z5518AMS-CS"," 5,5 - 187,0 mm, 1,8 – 560C, 1/3\", Video Auto Iris, Spot Filter, CS ",1704,null,"T34Z5518AMSP-CS"," 5,5 - 187,0 mm, 1,8 – 560C, 1/3\", CS ",1932]
[null,"T34Z5518AMSP-CS"," 5,5 - 187,0 mm, 1,8 – 560C, 1/3\", Video Auto Iris, Spot Filter, Preset, CS ",1932,null,"T34Z5518AMSR-CS"," 5,5 - 187,0 mm, 1,8 – 560C, 1/3\", CS ",1812]
[null,"T34Z5518AMSR-CS"," 5,5 - 187,0 mm, 1,8 – 560C, 1/3\", Video Auto Iris / manual Override, Spot Filter, CS ",1812,null,"T34Z5518AMSPR-CS"," 5,5 - 187,0 mm, 1,8 – 560C, 1/3\", CS ",2028]
[null,"T34Z5518AMSPR-CS"," 5,5 - 187,0 mm, 1,8 – 560C, 1/3\", Video Auto Iris / manual Override, Spot Filter, Preset, CS ",2028,null,"T34Z5518DC-CS"," 5,5 - 187,0 mm, 1,8 – 560C, 1/3\", CS ",1692]
[null,"T34Z5518DC-CS"," 5,5 - 187,0 mm, 1,8 – 560C, 1/3\", DC Auto Iris, CS ",1692,null,"T34Z5518PDC-CS"," 5,5 - 187,0 mm,1,8 – 560C, 1/3\", CS ",1920]
[null,"T34Z5518PDC-CS"," 5,5 - 187,0 mm,1,8 – 560C, 1/3\", Preset, DC Auto Iris, CS ",1920,null,"H6Z0812M"," 8,0 - 48,0 mm, 1,2 - 16C, 1/2\", C ",564]
[null,"H6Z0812M"," 8,0 - 48,0 mm, 1,2 - 16C, 1/2\", C ",564,null,"H6Z0812MS"," 8,0 - 48,0 mm, 1,2 – 560C, 1/2\", C ",612]
[null,"H6Z0812MS"," 8,0 - 48,0 mm, 1,2 – 560C, 1/2\", Spot Filter, C ",612,null,"H6Z0812MP"," 8,0 - 48,0 mm, 1,2 - 16C, 1/2\" C ",780]
[null,"H6Z0812MP"," 8,0 - 48,0 mm, 1,2 - 16C, 1/2\", C ",780,null,"H6Z0812MSP"," 8,0 - 48,0 mm, 1,2 – 560C, 1/2\", C ",804]
[null,"H6Z0812MSP"," 8,0 - 48,0 mm, 1,2 – 560C, 1/2\", Spot Filter, Preset, C ",804,null,"H6Z0812AMS"," 8,0 - 48,0 mm, 1,2 – 560C, 1/2\", C ",648]
[null,"H6Z0812AMS"," 8,0 - 48,0 mm, 1,2 – 560C, 1/2\", Spot Filter, C ",648,null,"H6Z0812AMSP"," 8,0 - 48,0 mm, 1,2 – 560C, 1/2\", C ",840]
[null,"H6Z0812AMSP"," 8,0 - 48,0 mm, 1,2 – 560C, 1/2\", Spot Filter, Preset, C ",840,null,"H10Z0812M"," 8,0 - 80,0 mm, 1,2 – 22C, 1/2\", C ",864]
[null,"H10Z0812M"," 8,0 - 80,0 mm, 1,2 – 22C, 1/2\", C ",864,null,"H10Z0812MS"," 8,0 - 80,0 mm, 1,2 – 560C, 1/2\", C ",924]
[null,"H10Z0812MS"," 8,0 - 80,0 mm, 1,2 – 560C, 1/2\", Spot Filter, C ",924,null,"H10Z0812MP"," 8,0 - 80,0 mm, 1,2 – 22C, 1/2\", C ",1068]
[null,"H10Z0812MP"," 8,0 - 80,0 mm, 1,2 – 22C, 1/2\", Preset, C ",1068,null,"H10Z0812MSP"," 8,0 - 80,0 mm, 1,2 – 560C, 1/2\", C ",1128]
[null,"H10Z0812MSP"," 8,0 - 80,0 mm, 1,2 – 560C, 1/2\", Spot Filter, Preset, C ",1128,null,"H10Z0812AMS"," 8,0 - 80,0 mm, 1,2 – 560C, 1/2\", C ",1008]
[null,"H10Z0812AMS"," 8,0 - 80,0 mm, 1,2 – 560C, 1/2\", Video Auto Iris, Spot Filter, C ",800,null,"H10Z0812AMSP"," 8,0 - 80,0 mm, 1,2 – 560C, 1/2\", C ",1236]
[null,"H10Z0812AMSP"," 8,0 - 80,0 mm, 1,2 – 560C, 1/2\", Video Auto Iris, Spot Filter, Preset, C ",950,null,"H10Z1218M"," 12,0 - 120,0 mm, 1,8 – 22C, 1/2\", C ",924]
["2MP","H10Z0819PDC-MP"," 8,0 - 80,0 mm, 1,9, 1/2\", C, Preset, DC Auto Iris, 1 Megapixel ",690]
["2MP","H10Z0819DC-MP"," 8,0 - 80,0 mm, 1,9, 1/2\", C, DC Auto Iris, 1 Megapixel ",640]
["2MP","H10Z0819AMSP-MP"," 8,0 - 80,0 mm, 1,9, 1/2\", C, Preset, Video Auto Iris, 1 Megapixel ",690]
["2MP","H10Z0819AMS-MP"," 8,0 - 80,0 mm, 1,9, 1/2\", C, Video Auto Iris, 1 Megapixel ",640]
[null,"H10Z1218M"," 12,0 - 120,0 mm, 1,8 – 22C, 1/2\", C ",924,null,"H10Z1218MS"," 12,0 - 120,0 mm, 1,8 – 560C, 1/2\", C ",984]
[null,"H10Z1218MS"," 12,0 - 120,0 mm, 1,8 – 560C, 1/2\", Spot Filter, C ",984,null,"H10Z1218MP"," 12,0 - 120,0 mm, 1,8 – 22C, 1/2\", C ",1140]
[null,"H10Z1218MP"," 12,0 - 120,0 mm, 1,8 – 22C, 1/2\", Preset, C ",1140,null,"H10Z1218MSP"," 12,0 - 120,0 mm, 1,8 – 560C, 1/2\", C ",1200]
[null,"H10Z1218MSP"," 12,0 - 120,0 mm, 1,8 – 560C, 1/2\", Spot Filter, Preset, C ",1200,null,"H10Z1218AMS-2"," 12,0 - 120,0 mm, 1,8 – 560C, 1/2\", C ",1044]
[null,"H10Z1218AMS-2"," 12,0 - 120,0 mm, 1,8 – 560C, 1/2\", Video Auto Iris, Spot Filter, C ",1044,null,"H10Z1218AMSP-2"," 12,0 - 120,0 mm, 1,8 – 560C, 1/2\", C ",1284]
[null,"H10Z1218AMSP-2"," 12,0 - 120,0 mm, 1,8 – 560C, 1/2\", Video Auto Iris, Spot Filter, Preset, C ",1284,null,"H10Z1218DC"," 12,0 - 120,0 mm, 1,8 – 560C, 1/2\", C ",888]
[null,"H10Z1218DC"," 12,0 - 120,0 mm, 1,8 – 560C, 1/2\", DC Auto Iris, C ",888,null,"H10Z1218PDC"," 12,0 - 120,0 mm, 1,8 – 560C, 1/2\", C ",1116]
[null,"H10Z1218PDC"," 12,0 - 120,0 mm, 1,8 – 560C, 1/2\", Preset, DC Auto Iris, C ",1116,null,"H16Z7516AMS"," 7,5 - 120,0 mm, 1,6 – 560C, 1/2\", C ",1224]
[null,"H16Z7516AMS"," 7,5 - 120,0 mm, 1,6 – 560C, 1/2\", Video Auto Iris, Spot Filter, C ",1224,null,"H16Z7516AMSP"," 7,5 - 120,0 mm, 1,6 – 560C, 1/2\", C ",1464]
[null,"H16Z7516AMSP"," 7,5 - 120,0 mm, 1,6 – 560C, 1/2\", Video Auto Iris, Spot Filter, Preset, C ",1464,null,"H16Z7516AMSR"," 7,5 - 120,0 mm, 1,6 – 560C, 1/2\", C ",1308]
[null,"H16Z7516AMSR"," 7,5 - 120,0 mm, 1,6 – 560C, 1/2\", Video Auto Iris / manual Override, Spot Filter, C ",1308,null,"H16Z7516AMSPR"," 7,5 - 120,0 mm, 1,6 – 560C, 1/2\", C ",1668]
[null,"H16Z7516AMSPR"," 7,5 - 120,0 mm, 1,6 – 560C, 1/2\", Video Auto Iris / manual Override, Spot Filter, Preset, C ",1668,null,"H16Z7516DC"," 7,5 - 120,0 mm, 1,6 – 560C, 1/2\", C ",1092]
[null,"H16Z7516DC"," 7,5 - 120,0 mm, 1,6 – 560C, 1/2\", DC Auto Iris, C ",1092,null,"H16Z7516PDC"," 7,5 - 120,0 mm, 1,6 – 560C, 1/2\", C ",1416]
[null,"H16Z7516PDC"," 7,5 - 120,0 mm, 1,6 – 560C, 1/2\", Preset, DC Auto Iris, C ",1416,null,"H16Z7516AMS-IR"," 7,5 - 120,0 mm, 1,6 – 560C, 1/2\", C, IR",4044]
[null,"H16Z7516AMS-IR"," 7,5 - 120,0 mm, 1,6 – 560C, 1/2\", Video Auto Iris, Spot Filter, C, IR",2340,null,"H16Z7516AMSP-IR"," 7,5 - 120,0 mm, 1,6 – 560C, 1/2\", C, IR",4440]
[null,"H16Z7516AMSP-IR"," 7,5 - 120,0 mm, 1,6 – 560C, 1/2\", Video Auto Iris, Spot Filter, Preset, C, IR",2480,null,"H16Z7516AMSR-IR"," 7,5 - 120,0 mm, 1,6 – 560C, 1/2\", C, IR",4620]
[null,"H16Z7516AMSR-IR"," 7,5 - 120,0 mm, 1,6 – 560C, 1/2\", Video Auto Iris / manual Override, Spot Filter, C, IR",2430,null,"H16Z7516AMSPR-IR"," 7,5 - 120,0 mm, 1,6 – 560C, 1/2\", C, IR",5040]
[null,"H16Z7516AMSPR-IR"," 7,5 - 120,0 mm, 1,6 – 560C, 1/2\", Video Auto Iris, / manual Override, Spot Filter, Preset, C, IR",2570,null,"H21Z1015AMS"," 10,0 - 210,0 mm, 1,5 - 1000, 1/2\",  C, Lieferzeit auf Anfrage ",1680]
["2MP","H21Z1016AMS-MP","10.0mm - 210mm, 1.6 - 1000, 1/2\", Video Auto Iris, C, 2 Megapixel",1860]
["2MP","H21Z1016AMSP-MP","10.0mm - 210mm, 1.6 - 1000, 1/2\", Video Auto Iris, Preset, C, 2 Megapixel",2040]
["3MP","H21Z1016DC-MP","10.0mm - 210mm, 1.6 - 1000, 1/2\", DC Auto Iris, C, 2 Megapixel",1860]
["3MP","H21Z1016PDC-MP","10.0mm - 210mm, 1.6 - 1000, 1/2\", DC Auto Iris, Preset, C, 2 Megapixel",2040]
["3MP","E24Z1018M-MP","10.0mm - 240mm, 1.8 - 500C, 1/1.8\", C, 3 Megapixel",3120]
["3MP","E24Z1018M-MPIR","10.0mm - 240mm, 1.8 - 500C, 1/1.8\", C, 3 Megapixel, IR",4020]
["3MP","E24Z1018MS-MP","10.0mm - 240mm, 1.8 - 500C, 1/1.8\", C, Spotfilter, 3 Megapixel",3240]
["3MP","E24Z1018MS-MPIR","10.0mm - 240mm, 1.8 - 500C, 1/1.8\",C, Spotfilter, 3 Megapixel, IR",4140]
["3MP","E24Z1018MP-MP","10.0mm - 240mm, 1.8 - 500C, 1/1.8\", C, 3 Megapixel",3240]
["3MP","E24Z1018MP-MPIR","10.0mm - 240mm, 1.8 - 500C, 1/1.8\", C, Preset, 3 Megapixel",4140,null,"H30Z1015AMS"," 10,0 - 300,0 mm, 1,5 – 560C, 1/2\", C ",3600]
["3MP","E24Z1018MSP-MP","10.0mm - 240mm, 1.8 - 500C, 1/1.8\", C, Spotfilter, Preset, 3 Megapixel",3300,null,"H30Z1015AMSP"," 10,0 - 300,0 mm, 1,5 – 560C, 1/2\", C ",3900]
["3MP","E24Z1018MSP-MPIR","10.0mm - 240mm, 1.8 - 500C, 1/1.8\", C, , Spotfilter, Preset, 3 Megapixel",4200,null,"H30Z1015AMSR"," 10,0 - 300,0 mm, 1,5 – 560C, 1/2\", C ",4116]
["3MP","E24Z1018AMS-MP","10.0mm - 240mm, 1.8 - 500C, 1/1.8\", Video Auto Iris, C, Spotfilter, 3 Megapixel",2880,null,"H30Z1015AMSPR"," 10,0 - 300,0 mm, 1,5 – 560C, 1/2\", C ",4452]
["3MP","E24Z1018AMS-MPIR","10.0mm - 240mm, 1.8 - 500C, 1/1.8\", Video Auto Iris, C, Spotfilter, Preset, 3 Megapixel, IR",3780]
["3MP","E24Z1018AMSP-MP","10.0mm - 240mm, 1.8 - 500C, 1/1.8\", Video Auto Iris, C, Spotfilter, Preset, 3 Megapixel",2970]
["3MP","E24Z1018AMSP-MPIR","10.0mm - 240mm, 1.8 - 500C, 1/1.8\", Video Auto Iris, C, Spotfilter, Preset, 3 Megapixel, IR",3900]
["3MP","E24Z1018DC-MP","10.0mm - 240mm, 1.8 - 500C, 1/1.8\", DC Auto Iris, C, 3 Megapixel",2880]
["3MP","E24Z1018DC-MPIR","10.0mm - 240mm, 1.8 - 500C, 1/1.8\", DC Auto Iris, C, 3 Megapixel, IR",3780,null,"H60Z1238A"," 12,5 - 1500 mm, 3.8 - 3000, 1/2\", C, 2xExtender",20000]
["3MP","E24Z1018PDC-MP","10.0mm - 240mm, 1.8 - 500C, 1/1.8\", DC Auto Iris, C, Preset, 3 Megapixel",2970,null,"H60Z1238A-IR"," 12,5 - 1500 mm, 3.8 - 3000, 1/2\", C,IR,2xExtender",23000]
["3MP","E24Z1018PDC-MPIR","10.0mm - 240mm, 1.8 - 500C, 1/1.8\", DC Auto Iris, C, Preset, 3 Megapixel, IR",3900,null,"H60Z1238A-IRF"," 12,5 - 1500 mm, 3.8 - 3000, 1/2\", C, IR, 2xExtender, AntiFog Funktion",25000]
["2MP","M24Z1527PDC-MP","2/3\" f15.0-360mm 2.7 DC 2MP 24X Preset Spot Filter C",5400]
["2MP","M24Z2138PDC-MP","2/3\" 21.0-500mm 3.8 DC 2MP 24X Preset Sport Filter. C",6600]
["1.3MP","H27Z9535AM-MP","9,5 - 256,5 mm, 3,5, 1/2\", Video Auto Iris, C, 1.3 Megapixel",3300,null,"H62Z1235AMS-MP","12,5 - 775,0 mm, 3.5, 1/2\" C, Megapixel, NEU",14800]
["1.3MP","H27Z9535AMP-MP","9,5 - 256,5 mm, 3,5, 1/2\", Video Auto Iris, Preset, C, 1.3 Megapixel",3500,null,"H62Z1235AMSP-MP","12,5 - 775,0 mm, 3.5 1/2\", C, Megapixel, NEU",15500]
["1.3MP","H27Z9535DC-MP","9,5 - 256,5 mm, 3,5, 1/2\", DC Auto Iris, C, 1.3 Megapixel",3300]
["1.3MP","H27Z9535PDC-MP","9,5 - 256,5 mm, 3,5, 1/2\", DC Auto Iris, Preset, C, 1.3 Megapixel",3500]
[null,"H30Z1015AMS"," 10,0 - 300,0 mm, 1,5 – 560C, 1/2\", Video Auto Iris, C ",3600]
[null,"H30Z1015AMSP"," 10,0 - 300,0 mm, 1,5 – 560C, 1/2\", Video Auto Iris, Spot Filter, Preset, C ",3900]
[null,"H30Z1015AMSR"," 10,0 - 300,0 mm, 1,5 – 560C, 1/2\", Video Auto Iris / manual Override, Spot Filter, C ",4116]
[null,"H30Z1015AMSPR"," 10,0 - 300,0 mm, 1,5 – 560C, 1/2\", Video Auto Iris / manual Override, Spot Filter, Preset, C ",4452]
["2MP","H35Z1015AMS-MP","10,0 - 350 mm, 1,5, 1/2\", Video Auto Iris, Spot Filter, C, 2 Megapixel",4800]
["2MP","H35Z1015AMSP-MP","10,0 - 350 mm, 1,5, 1/2\", Video Auto Iris, Spot Filter, Preset, 2 Megapixel",5100]
["2MP","H35Z1015DC-MP","10,0 - 350 mm, 1,5, 1/2\", DC Auto Iris, C, 2 Megapixel",4800]
["2MP","H35Z1015PDC-MP","10,0 - 350 mm, 1,5, 1/2\", DC Auto Iris, Preset, C, 2 Megapixel",5100]
[null,"H60Z1238A"," 12,5 - 1500 mm, 3.8 - 3000, 1/2\", Video Auto Iris, C, 2x Extender",14400]
[null,"H60Z1238A-IR"," 12,5 - 1500 mm, 3.8 - 3000, 1/2\", Video Auto Iris, IR, C, 2xExtender",15800]
[null,"H60Z1238A-IRF"," 12,5 - 1500 mm, 3.8 - 3000, 1/2\", Video Auto Iris, IR, 2x Extender, C, AntiFog Funktion",16300]
["2MP","H62Z1235AM-MP","12,5 - 775,0 mm, 3.5, 1/2\", Video Auto Iris,C, 2 Megapixel",10300]
["2MP","H62Z1235AMP-MP","12,5 - 775,0 mm, 3.5, 1/2\", Video Auto Iris, Preset, C, 2 Megapixel",11100]
["2MP","H62Z1235AM-MP-EX","25 - 1550 mm, 3.5, 1/2\", Video Auto Iris, 2 Megapixel, 2x Extender",13200]
["2MP","H62Z1235AMP-MP-EX","25 - 1550 mm, 3.5, 1/2\", Video Auto Iris, Preset, 2 Megapixel, 2x Extender",14200]
["2MP","H62Z1235AMP-MPIR","12,5 - 775,0 mm, 3.5, 1/2\", Video Auto Iris, Preset, C, 2 Megapixel, IR",15000]
["2MP","H62Z1235AMP-MPIR-EX","25 - 1550 mm, 3.5, 1/2\", Video Auto Iris, Preset, 2 Megapixel, IR, 2x Extender",18000]
["2MP","H62Z1235DC-MP","12,5 - 775,0 mm, 3.5, 1/2\", DC Auto Iris, C, 2 Megapixel",10300]
["2MP","H62Z1235PDC-MP","12,5 - 775,0 mm, 3.5, 1/2\", DC Auto Iris, Preset, C, 2 Megapixel",11100]
["2MP","H62Z1235DC-MP-EX","25 - 1550 mm, 3.5, 1/2\", DC Auto Iris, 2 Megapixel, C, 2x Extender",13200]
["2MP","H62Z1235PDC-MP-EX","25 - 1550 mm, 3.5, 1/2\", DC Auto Iris, Preset, 2 Megapixel, 2x Extender",14200]
["2MP","H62Z1235PDC-MPIR","12,5 - 775,0 mm, 3.5, 1/2\", DC Auto Iris, Preset, 2 Megapixel, IR",15000]
["2MP","H62Z1235PDC-MPIR-EX","25 - 1550 mm, 3.5, 1/2\", DC Auto Iris, Preset, 2 Megapixel, IR, 2x Extender",18000]
["Nadelöhrobjektive",null,"     ",null,null,"T2625CS-P"," 2,6 mm 2,5 - 32C 1/3\" CS, M",368]
[null,"T2625CS-P"," 2.6 mm 2.5 – 32C 1/3\" CS M",368,null,"TG2625FCS-P"," 2,6 mm 2,5 - 360C, 1/3\", CS, D9",518]
[null,"TG2625FCS-P"," 2.6 mm 2.5 – 360C 1/3\" CS D9",518,null,"TG2625FCS-P"," 2,6 mm, 2,5 - 360C, 1/3\", CS, D31",{"$error":"#N/A"}]
[null,"TG2625FCS-P31"," 2.6 mm 2.5 – 360C 1/3\" CS D31",518,null,"TG2625AFCS-P"," 2,6 mm, 2,5 - 360C, 1/3\", CS, V",553]
[null,"TG2625AFCS-P"," 2.6 mm 2.5 – 360C 1/3\" CS V",553,null,null,"     "]
["Machine Vision"]
["Image Processing",null,null,null,null,"M1214MP2"," 12,0 mm, 1,4 – 16C, 2/3\", C, Megapixel",180]
[null,"H0514-MP2"," 5,0 mm, 1,4 - 16C, 1/2’’, C, Megapixel",252,null,"M1614MP2"," 16,0 mm, 1,4 – 16C, 2/3\", C, Megapixel",156]
[null,"M0814-MP2"," 8,0 mm, 1,4 – 16C, 2/3\", C, 1.5 Megapixel",180,null,"M2514MP2"," 25,0 mm, 1,4 – 16C, 2/3\", C, Megapixel",168]
[null,"M1214-MP2"," 12,0 mm, 1,4 – 16C, 2/3\", C, 1.5 Megapixel",180,null,"M3514MP"," 35,0 mm, 1,4 – 16C, 2/3\", C, Megapixel",216]
[null,"M1614-MP2"," 16,0 mm, 1,4 – 16C, 2/3\", C, 1.5 Megapixel",156,null,"M5018MP2"," 50,0 mm, 1,8 – 16C, 2/3\" ,C, Megapixel",180]
[null,"M2514-MP2"," 25,0 mm, 1,4 – 16C, 2/3\", C, 1.5 Megapixel",168,null,"M7528MP"," 75,0 mm, 2,8 – 16C, 2/3\", C,  Megapixel",276]
[null,"M3514-MP"," 35,0 mm, 1,4 – 16C, 2/3\", C, 1.5 Megapixel",216,null,"M2518-MPW"," 25,0 mm, 1,8 - 16, 2/3\", C, 5 Megapixel",890]
[null,"M5018-MP2"," 50,0 mm, 1,8 – 16C, 2/3\" ,C, 1.5 Megapixel",180]
[null,"M7528-MP"," 75,0 mm, 2,8 – 16C, 2/3\", C,  1.5 Megapixel",276]
[null,"M0824-MPW2"," 8,0 mm, 2,4 – 16C, 2/3\", C, 5 Megapixel",380]
[null,"M1224-MPW2"," 12,0 mm, 2,4 – 16C, 2/3\", C, 5 Megapixel",340]
[null,"M1620-MPW2","16,0 mm, 2,0, 2/3\", C, 5 Megapixel",300]
[null,"M2518-MPW2","25,0 mm, 1,8, 2/3\", C, 5 Megapixel",300]
[null,"M3520-MPW2","35,0 mm, 2,0, 2/3\", C, 5 Megapixel",300]
[null,"M5028-MPW2","50,0 mm, 2,8, 2/3\", C, 5 Megapixel",300]
[null,"M2514FIC-MPIR","25,0 mm, 2/3\", C, F1.4, IR-corrected, 5 Megapixel",680]
[null,"M3518FIC-MPIR","35,0 mm, 1,8, 2/3\", C, IR-corrected, 5 Megapixel",670]
[null,"M5020FIC-MPIR","50,0 mm, 2,0, 2/3\", C, IR-corrected, 5 Megapixel",690,null,null,"     "]
["1\""]
["Neu","V0814-MP","8mm, 1\", F1.4, C, 2MP",430,null,"T1318C-WA"," 1,28 mm, 1,8 - 16C, 1/3\" ,C, Weitwinkel, Megapixel",1560]
["Neu","V1214-MP","12mm, 1\", F1.4, C, 2MP",400,null,"H0514-MP"," 5,0 mm, 1,4 - 16C, 1/2’’, C, Megapixel",252]
["Neu","V1614-MP","16mm, 1\", F1.4, C, 2MP",400,null,"MLH10XC"," 13,0 – 130 mm, 5,6 – 32C, 1/2'’, C, Macro",438]
["Neu","V2514-MP","25mm, 1\", F1.4, C, 2MP",400,null,"TEC-V7X"," 47,65 - 106,26 mm, 4,3 - 32, 1,1\", C, Telec. Macro, 5 Megapixel",3500]
["Neu","V5014-MP","50mm, 1\", F1.4, C, 2MP",430]
["1.1\""]
["Neu","V0828-MPY","8mm, 1.1\", F2.8, C, 12MP",930]
["Neu","V1228-MPY","12mm, 1.1\", F2.8, C, 12MP",860]
["Neu","V1628-MPY","16mm, 1.1\", F2.8, C, 12MP",810]
["Neu","V2528-MPY","25mm, 1.1\", F2.8, C, 12MP",810]
["Neu","V3528-MPY","35mm, 1.1\", F2.8, C, 12MP",810]
["Neu","V5028-MPY","50mm, 1.1\", F2.8, C, 12MP",810]
["Makro",null,"     "]
[null,"T1318C-WA"," 1,28 mm 1,8 - 16C 1/3\" C",800]
[null,"MLH10XC"," 13,0 – 130 mm 5,6 – 32C 1/2'’ C Macro",438]
[null,"MLM-3XMP"," 27.0 - 91.0 mm 4.5 – 22C 2/3\" C Macro, Megapixel",540]
["Megapixel-Objektive mit M12 x 0,5 Mount"]
[null,"E1220KV"," 12 mm, 2.01/1.8\"  ",140]
[null,"E1620KV"," 16 mm, 2.0 1/1.8\"  ",120]
[null,"E2520KV"," 25 mm, 2.0 1/1.8\" ",120]
["Neu","E3828KRW","3.8mm, 8MP, 1/1.8\"",160]
["Neu","E5228KRW","5.2mm, 8MP, 1/1.8\"",140]
[null,"H1328KP"," 1,27 mm, 2,8, 1/2\", Megapixel, Fish-Eye",150]
[null,"H0320KP"," 3 mm, 2 1/2\"  Megapixel",98]
[null,"H0624KP"," 6 mm, 2,4, 1/2\", Megapixel",88]
[null,"H0924KP"," 9 mm, 2,4, 1/2\", Megapixel",88]
[null,"H1620KP"," 16 mm, 2 1/2\", Megapixel",88]
[null,"H2520KP"," 25 mm 2, 1/2\", Megapixel",88]
[null,"M12*P0.5 Mount Adapter","Adapter CS-Mount / M12 ","auf Anfrage"]
["SWIR"]
[null,"M1614-SW","16mm, C, F1.4",580]
[null,"M2514-SW","25mm, C, F1.4",580]
[null,"M3514-SW","35mm, C, F1.4",580]
[null,"M5018-SW","50mm, C, F1.8",580]
["Telezentrische Objektive"]
[null,"TEC-V7X"," 47,65 - 106,26 mm 4,3 - 32 1,1\", C, Telec. Macro, 5 Megapixel",1999]
[null,"TECM55"," 55.0 mm 2.8 – 32C 2/3’’ C Telec.",604]
[null,"TECM55-20","Brennweitenkonverter für TECM55, 2x     ",173]
[null,"TECM55-75","Brennweitenkonverter für TECM55, 0.75x     ",172]
[null,"TEC-M55MPW"," 55,0 mm, 3.0 – 22C, 2/3’’, C, Telez., 5 Megapixel",720]
[null,"TEC-M0565MPC","0.5x, Coaxial, 2/3\", C, 65mm WD",1000]
[null,"TEC-M0565MP","0.5x, 2/3\", C, 65mm WD",850]
[null,"TEC-M0865MPC","0.8x, Coaxial, 2/3\", C, 65mm WD",920]
[null,"TEC-M0865MP","0.8x, 2/3\", C, 65mm WD",800]
[null,"TEC-M1065MPC","1.0x, Coaxial, 2/3\", C, 65mm WD",920]
[null,"TEC-M1065MP","1.0x, 2/3\", C, 65mm WD",800]
[null,"TEC-M2065MPC","2.0x, Coaxial, 2/3\", C, 65mm WD",930]
[null,"TEC-M2065MP","2.0x, 2/3\", C, 65mm WD",800]
[null,"TEC-M03110MPC","0.3x, Coaxial, 2/3\", C, 110mm WD",1900]
[null,"TEC-M03110MP","0.3x, 2/3\", C, 110mm WD",1700]
[null,"TEC-M05110MPC","0.5x, Coaxial, 2/3\", C, 110mm WD",1150]
[null,"TEC-M05110MP","0.5x, 2/3\", C, 110mm WD",990]
[null,"TEC-M08110MPC","0.8x, Coaxial, 2/3\", C, 110mm WD",1050]
[null,"TEC-M08110MP","0.8x, 2/3\", C, 110mm WD",960]
[null,"TEC-M10110MPC","1.0x, Coaxial, 2/3\", C, 110mm WD",1050]
[null,"TEC-M10110MP","1.0x, 2/3\", C, 110mm WD",960]
[null,"TEC-M15110MPC","1.5x, Coaxial, 2/3\", C, 110mm WD",1050]
[null,"TEC-M15110MP","1.5x, 2/3\", C, 110mm WD",960]
[null,"TEC-M20110MPC","2.0x, Coaxial, 2/3\", C, 110mm WD",1050]
[null,"TEC-M20110MP","2.0x, 2/3\", C, 110mm WD",960]
["Telezentrische Objektive mit 5MP"]
[null,"TEC-V0565MPW","0.5x, 1\", C, 65mm WD",1880]
[null,"TEC-V1065MPW","1.0x, 1\", C, 65mm WD",1900]
[null,"TEC-V05110MPW","0.5x, 1\", C, 110mm WD",1880]
[null,"TEC-V10110MPW","1.0x, 1\", C, 110mm WD",1900]
["Zubehör",null,"     ",null,null,"HM0924KP"," 9 mm, 2.4 - 22, 1/2\", Megapixel","auf Anfrage"]
[null,"VM100","Zwischenringsatz (0,5, 1, 5, 10, 20, 40 mm)     ",56,null,"HM1620KP"," 16 mm, 2.0 - 32, 1/2\", Megapixel","auf Anfrage"]
[null,"VM400","Adapterring C-/CS-Mount, 5 mm     ",8,null,"M12*P0.5 Mount Adapter","Adapter zwischen einem CS-Mount Gewinde und dem M12 Gewinde     ","auf Anfrage"]
[null,"EX1.5CS","Brennweitenkonverter, 1,5-fach, CS     ",67,null,null,"     "]
[null,"EX1.5C","Brennweitenkonverter, 1,5-fach, C     ",66]
[null,"EX2.0CS","Brennweitenkonverter, 2-fach, CS     ",82,null,"THH5000"," 1,9 mm,  2 1/4\"  ",37]
[null,"EX2.0C","Brennweitenkonverter, 2-fach, C     ",91,null,"TER5000"," 2,5 mm,  2 1/3\"  ",24]
[null,"LP1","4-poliger Stecker für Autoiris-Objektive     ",4,null,"TEH5000"," 2,9 mm,  2 1/3\"  ",24]

{"sheet":"IP Cameras & NVR","index":2,"n_rows":175,"n_cols":5,"rows_kept":175,"cut":false,"hidden":false,"merged":[[138,0,138,2],[4,0,4,4],[28,0,31,1],[103,0,103,2],[119,0,119,1]]}
["IP-Kameras & NVR",null,null,"     "]
[]
[]
[null,null,"Modell","Beschreibung"," EURO"]
["Ganz GenSTAR"]
[null,"CS-Mount"]
[null,null,"ZN8-CAN","H.264 4 Megapixel, CS-Mount, 1/3\" CMOS, mechanische Tag/Nachtumschaltung, max. 30bps, DWDR, AGC, 2/3DNR, 24VAC / 12VDC / PoE, 142mm (W) x 65mm (H) x 78mm (D), 360g",395]
[null,"Bulletkamera"]
[null,null,"ZN8-B4NMZ59 ","H.264 2 Megapixel, 3.0mm - 12mm, motorisierter Zoom Fokus, mechanische Tag/Nacht Umschaltung, max. 30bps, IRLEDs 30-40m, DWDR, AGC, DIS, POI, 3DNR, 12VDC / PoE, 377mm (H) x 110mm (Ø), 780g",450]
[null,null,"ZN8-BANVF59","H.264 4 Megapixel, 3.0mm - 12mm, mechanische Tag/Nachtumschaltung, max. 30bps, IR-LEDs 20-25m, DWDR, AGC, DIS, POI, 2/3DNR, 12VDC / PoE, 264.5mm (H) x 80.3mm (Ø), 780g\"",383]
[null,null,"ZN8-NANFN4","H.264 4 Megapixel, 3.6mm, mechanische Tag/Nachtumschaltung, max. 30bps, IR-LEDs 20-30m, DWDR, AGC, DIS, POI, 12VDC / PoE, 169(B) ×70(H) ×60(T), 631g",258]
[null,null,"ZN8-N4NFN4","1/3“ 2 Megapixel CMOS Bulletkamera, 3.6mm Lens, TDN, DNR, DWDR, IR-LEDs 20 ~ 30m, IP66, 12vdc/POE",248]
[null,null,"ZN8-B4NVF56","1/3“ 2 Megapixel CMOS Bulletkamera,  2.8 ~ 12mm Lens, TDN, DNR, DWDR, IR-LEDs 40 ~ 50m, IP66, 12vdc/POE",373]
[null,"Fisheye"]
[null,null,"ZN8-F7NTFN10L","H.264 6 Megapixel Dome Fisheye, 1.6mm, 360° FoV, mechanische Tag/Nachtumschaltung, max. 30bps, IR-LEDs 10m, DWDR, AGC, DIS, POI, 12VDC / 24VAC / PoE, 46.8mm (H) x 160mm (D), 700g",866]
[null,"PTZ"]
[null,null,"ZN8-P4NTAF60L","H.264 2 Megapixel PTZ Dome, 4.7mm - 103mm, 1/2.8\" CMOS, Farbe 0.02 lux / s/w\n0.002 lux, 0 lux (IR an), 3DNR, DWDR, IR-LEDs 100m, 24VAC, 332mm (H) x 205mm (D), 4.3kg, inkl. Wandarm und Netzteil 24VAC",1560]
[null,null,"ZN8-P5NTAF62L ","H.264 3 Megapixel PTZ Dome, 4.7mm - 56.4mm, 1/2.8\" CMOS, Farbe 0.01 lux / s/w\n0.001 lux, 0 lux (IR an), 3DNR, DWDR, IR-LEDs 100m, 12VDC/PoE+, 321mm (H) x 222mm x 146, 1.5kg, inkl. Wandarm und Netzteil 12VDC",790]
[null,"Domekamera"]
[null,null,"ZN8-MANTFN4L","H.264 4 Megapixel, 3.6mm, mechanische Tag/Nachtumschaltung, max. 30bps, IR-LEDs 6-7m, DWDR, AGC, DIS, POI, 12VDC / PoE, 53mm (H) x 100mm (D), 650g",258]
[null,null,"ZN8-DANTVF59L","H.264 4 Megapixel, 3.0mm - 12mm, mechanische Tag/Nachtumschaltung, max. 30bps, IRLEDs 10-20m, DWDR, AGC, DIS, POI, 12VDC / 24VAC / PoE, 111.5mm (H) x 130mm (D), 815g",406]
[null,null,"ZN8-M4NTFN4L","1/3“ CMOS 2 Megapixel Mini Vandal Dome, 3.6mm, TDN, DNR, DWDR, IR-LEDs  ~10m, IP65, 12vdc/POE",248]
[null,"NVR"]
[null,null,"NR8-4M71","H.264 4-Kanal NVR, max. 6MP Aufzeichnung, 4x RJ-45 (PoE), HDMI / VGA, 1x SATA-Anschluss, 2x USB, RJ-45, 255 x 47.5 x 235, 930g",240]
[null,null,"NR8-8M71","H.264 8-Kanal NVR, max. 6MP Aufzeichnung, 8x RJ-45 (PoE), HDMI / VGA, 1x SATA-Anschluss, 2x USB, RJ-45, 372 x 44.5 x 311, 2.8kg",318]
[null,null,"NR8-16M74","H.264 16-Kanal NVR, max. 6MP Aufzeichnung, 16x RJ-45 (PoE), HDMI / VGA, 4x SATA-Anschluss, 3x USB, RJ-45, 440 x 67 x 376, 3.6kg",1098]
[null,null,"NR8-32M78-0","H.264 32-Kanal NVR, max. 6MP Aufzeichnung, 2x RJ-45, HDMI / VGA, 8x SATA-Anschluss, 2x USB, RJ-45, 440 x 89.9 x 435, 7.2kg",738]
[null,"Zubehör"]
["Bitte beachten Sie das folgende PDF in Bezug auf die Kombinierbarkeit des Zubehörs:",null,"ZA8-CBK625","Deckel abgehängte Montage",30]
[null,null,"ZA8-CBK624 ","Wandhalterung",80]
[null,null,"ZA8-CBK626","Eckhalterung",50]
[null,null,"ZA8-CBK627","Masthalter",60]
[null,null,"ZA8-CBK623","Abgehängte Montage",60]
[null,null,"ZA8-CBK633B","Montagebox",70]
[null,null,"ZA8-CBK634","Montagebox",30]
[null,null,"ZA8-CBK636 ","Wall Mount",70]
[null,null,"ZA8-CBK637 ","Abgehängte Montage",60]
[null,null,"ZA8-BK604","Masthalter",210]
[null,null,"ZA8-BK605","Eckhalterung",160]
[null,null,"ZA8-BK607B","Deckenhalterung",40]
[null,null,"ZA8-CBK640","Pendant Mount",50]
[null,null,"ZA8-CBK642","Flush Mount",70]
[null,"Service Equipment"]
[null,null,"ZW-N22F","Wireles service equipment, zur Einrichtung  / Installationsunterstützung für IP Kameras",240]
[]
[null,"Bullet"]
[null,null,"ZN-B2MTP","H.264, mechanische Tag/Nacht-Bulletkamera mit 2,0 MP-HD Auflösung, 3 mm - 9 mm, P-Iris, Fokus und Zoom per Remote einstellbar, integrierte IR-LEDs",690]
[null,null,"ZN-B2MTP-2","H.264, mechanische Tag/Nacht-Bulletkamera mit 2,0 MP-HD Auflösung, 10 mm - 23 mm, P-Iris, Fokus und Zoom per Remote einstellbar, integrierte IR-LEDs",700]
[null,null,"ZN-B6DMP55HE","H.264, mechanische Tag/Nacht-Bulletkamera mit 5,0 MP-HD Auflösung, 1/1.8\" Sony ExmorR CMOS, WDR, 3.6 mm - 10 mm, P-Iris, Fokus und Zoom per Remote einstellbar, integrierte IR-LEDs",950]
[null,"Innendome"]
[null,null,"ZN-D2MTP-IR","H.264 mechanische Tag/Nacht-Domekamera mit 2,0 MP Full-HD Auflösung, 3 mm - 9 mm, P-Iris, Fokus und Zoom per Remote einstellbar, IR-LEDs",500]
[null,null,"ZN-D6DMP55LHE ","H.264, mechanische Tag/Nacht-Domekamera mit 5,0 MP-HD Auflösung, 1/1.8\" Sony ExmorR CMOS, WDR, 3.6 mm - 10 mm, P-Iris, Fokus und Zoom per Remote einstellbar, integrierte IR-LEDs",670]
[null,"Außendome"]
[null,null,"ZN-DT2MTP","H.264 mechanische Tag/Nacht-Domekamera mit 2,0 MP Full-HD Auflösung, vandalismusgeschützt, 3 mm - 9 mm, P-Iris, Fokus und Zoom per Remote einstellbar",650]
[null,null,"ZN-DT2MTP-IR","H.264 mechanische Tag/Nacht-Domekamera mit 2,0 MP Full-HD Auflösung, vandalismusgeschützt, 3 mm - 9 mm, P-Iris, Fokus und Zoom per Remote einstellbar, IR-LEDs",700]
[null,null,"ZN-D6DTMP55LHE ","H.264, mechanische Tag/Nacht-Domekamera mit 5,0 MP-HD Auflösung, 1/1.8\" Sony ExmorR CMOS, WDR, 3.6 mm - 10 mm, P-Iris, Fokus und Zoom per Remote einstellbar, integrierte IR-LEDs, IK10 / IP66",870]
[null,"Autofocus"]
[null,null,"ZN-M2AF","H.264 Autofokuskamera mit Full-HD Auflösung, 5.0 mm - 25 mm, Dual Stream (H.264, MJPEG), 1/2.8\" Sony IMX-036 CMOS, 0,24 lux (F3.5 / 30IRE (Farbe)), PoE, UVV",450]
[null,"Mini-Serie"]
[null,null,"ZN-MB243M","H.264 Bulletkamera mit 2,0 MP Full-HD Auflösung, 4.0mm, Dual Stream (H.264, MJPEG), 1/2,8\" Progressive Scan CMOS, IR-LEDs, IP66, inkl. Halterung",300]
[null,null,"ZN-MB260M","H.264 Bulletkamera mit 2,0 MP Full-HD Auflösung, 6.0mm, Dual Stream (H.264, MJPEG), 1/2,8\" Progressive Scan CMOS, IR-LEDs, IP66, inkl. Halterung",300]
[null,null,"ZN-MDI260M-IR","H.264 Domekamera mit 2,0 MP Full-HD Auflösung, 6.0mm, Dual Stream (H.264, MJPEG), 1/2,8\"Sony CMOS, IR-LEDs",300]
[null,null,"ZN-MD243M","H.264 Domekamera mit 2,0 MP Full-HD Auflösung, 4,0 mm, Dual Stream (H.264, MJPEG), 1/2,8\"Sony IMX-036 CMOS, UVV, PoE, IP66, Nachfolger sobald vergriffen: ZN-M4NTFN4L",360]
[null,null,"ZN-M4NTFN3L ","H.264 Eyeballkamera mit 2,0 MP Full-HD Auflösung, 2.8 mm, Dual Stream (H.264, MJPEG), 1/2.8\"Sony Exmor CMOS, 12VDC / PoE, IP66",360]
[null,null,"ZN-M4NFN3L","H.264 Dome Kamera mit 2,0 MP Full-HD Auflösung, 2.8 mm, Dual Stream (H.264, MJPEG), 1/2.9\"Sony Exmor CMOS",300]
[null,null,"ZN-N4NVD56","H.264 Bullet Kamera mit 2,0 MP Full-HD Auflösung, 2.8 mm - 12 mm, Dual Stream (H.264, MJPEG), 1/2.8\"Sony Exmor CMOS, PoE, IP66",420]
[null,null,"ZN-N4NFN5","H.264 Bullet Kamera mit 2,0 MP Full-HD Auflösung, 4 mm, Dual Stream (H.264, MJPEG), 1/2.9\"Sony Exmor CMOS, PoE, IP66",300]
[null,"PTZ"]
[null,null,"ZN-P4NT50","PTZ Dome IP66 / IK10, 25 bps @ 2MP Full-HD, 1/2.8\" CMOS, ICR, DWDR, 0.4 Lux F1.6 50 IRE, 0.03 Lux F1.6 50 IRE (n/b), 4.7 - 94mm, SD card slot, 24VAC / PoE+",2450]
[null,null,"ZN-P4NT50L","PTZ Dome IP66, 25 bps @ 2MP Full-HD, 1/2.8\" CMOS, ICR, DWDR, IR-LEDs, 0.4 Lux F1.6 50 IRE, 0 Lux F1.6 50 IRE (n/b IR on), 4.7 - 94mm, SD card slot, 24VAC ",3560]
[null,"Zubehör"]
[null,null,"ZNA-CA1","Adapter für PixelPro Außendomeserie (außer Miniserie) zur abgehängten Montage",60]
[null,null,"PMA2","Masthalter für ZNA-WM2A",60]
[null,null,"ZNA-WM2A","Adapter für PixelPro Außendomeserie (außer Miniserie) zur Wandmontage",130]
[null,null,"ZC-FM3","Adapter zur versenkten Wand-/Deckenmontage PixelPro Innendomeserie (außer Miniserie)",60]
[null,null,"ZC7-PM1","Adapter zur abgehängten Montage PixelPro Innendomeserie (außer Miniserie)",40]
[null,null,"ZC7-WM1","Wandmontageadapter PixelPro Innendomeserie (außer Miniserie)",70]
[null,null,"ZNA-POEExtender","Spannungsversorgung für PoE Kameras",40]
[null,null,"ZNA-CMB3A ","Deckenhalter für ZN-6DT",80]
[null,null,"ZNA-ICB3A","Deckeneinbauadapter für ZN-6DT",30]
[null,null,"ZNA-WMB3A","Wandhalter für ZN-6DT",80]
[null,null,"ZNA-JB3A ","Anschaltbox für ZN-6 und N4 Serie",70]
[null,null,"ZNA-WMB3 ","Wandhalter für ZN-P4NT50(L)",130]
[null,null,"ZNA-CMB3 ","Deckenhalter für ZN-P4NT50(L)",130]
[null,null,"ZNA-PM3","Masthalter ZN-P4NT50(L)",60]
[null,null,"ZNA-CM3 ","Eckhalter für ZN-P4NT50(L)",80]
[null,"NVR"]
[null,null,"NR8H","8-Kanal Triplex Netzwerkrekorder, H.264 Kompression, LINUX OS, LAN, HDMI/VGA Ausgang, 200 Bilder pro Sekunde bei 1080p, 8-Port PoE Switch integriert, bis zu 5 S-ATA Festplatten einbaubar, Smartphonezugriff, Nachfolger sobald vergriffen: NR-8M65",1400]
[null,null,"NR16H","16-Kanal Triplex Netzwerkrekorder, H.264 Kompression, LINUX OS, LAN, HDMI/VGA Ausgang, 400 Bilder pro Sekunde bei 1080p, 8-Port PoE Switch integriert, inkl. externem 8-Port PoE Switch, bis zu 5 S-ATA Festplatten einbaubar, Smartphonezugriff, , Nachfolger sobald vergriffen: NR-16M65",1700]
[null,null,"NR-4M62  ","4-Kanal Triplex Netzwerkrekorder, H.264 Kompression, LINUX OS, LAN, HDMI/VGA-Ausgang, 5MP@15bps / 3MP, 1080p Echtzeitaufzeichnung, 4-Port PoE Switch integriert, bis zu 2 S-ATA Festplatten einbaubar, Smartphonezugriff",720]
[null,null,"NR-8M62","8-Kanal Triplex Netzwerkrekorder, H.264 Kompression, LINUX OS, LAN, HDMI/VGA-Ausgang, 200 Bilder pro Sekunde bei 1080p, 8-Port PoE Switch integriert, bis zu 2 S-ATA Festplatten einbaubar, Smartphonezugriff",990]
[null,null,"NR-16M62 ","16-Kanal Triplex Netzwerkrekorder, H.264 Kompression, LINUX OS, LAN, HDMI/VGA-Ausgang, 5MP@15bps / 3MP, 1080p Echtzeitaufzeichnung, 8-Port PoE Switch integriert, bis zu 2 S-ATA Festplatten einbaubar, Smartphonezugriff",1100]
[null,null,"NR-8M65","8-Kanal Triplex Netzwerkrekorder, H.264 Kompression, LINUX OS, LAN, HDMI/VGA Ausgang, 5MP@15bps / 3MP, 1080p Echtzeitaufzeichnung, 8-Port PoE Switch integriert, bis zu 5 S-ATA Festplatten einbaubar, Smartphonezugriff",1600]
[null,null,"NR-16M65 ","16-Kanal Triplex Netzwerkrekorder, H.264 Kompression, LINUX OS, LAN, HDMI/VGA Ausgang, 5MP@15bps / 3MP, 1080p Echtzeitaufzeichnung, 8-Port PoE Switch integriert, inkl. externem 8-Port PoE Switch, bis zu 5 S-ATA Festplatten einbaubar, Smartphonezugriff",1900]
[null,"Zubehör"]
[null,null,"NR-RM1","Rackmount NR4HL-V / NR8HL-V / NRxM62",19]
[null,null,"NR-RM2","Rackmount NR8H / NR16H / NRxM65",19]
[null,null,"NR16PoE-2","8-Port PoE Switch, kaskadierbar",460]
[null,"HDD 24/7"]
[null,null,"ZRS-HDD1000","S-ATA HDD 1TB  WD Purple 24/7",69]
[null,null,"ZRS-HDD2000","S-ATA HDD 2TB  WD Purple 24/7",99]
[null,null,"ZRS-HDD3000","S-ATA HDD 3TB  WD Purple 24/7",129]
[null,null,"ZRS-HDD4000","S-ATA HDD 4TB  WD Purple 24/7",159]
["PixelPro GXi Serie",null,null,"     "]
[null,"CS-Mount",null,"     "]
[null,null,"ZN-NH22XE","H.264 2 Megapixel, mech. Tag/Nachtkamera, 1/3\", 1,0 Lux (Farbe) 0,001 Lux (s/w), CS mount, 25B/s, inkl. Video Analyse Software, OSD, Schnittstellen SD-card slot, PoE/12VDC ",700]
[null,"Dome"]
[null,null,"ZN-DN312XE-M","H.264 2 Megapixel Dome, mechanische Tag/Nachtkamera, 1/2.7\"- CMOS, Brennweite 3,0 mm - 9,0mm, Fokus und Zoom per Remote einstellbar, F1.2, 1,0 Lux (Farbe) / 0,001 Lux (s/w), effektive Auflösung 1920x1080 (einstellbar), 25B/s, Dual stream,  inkl. Video Analyse Software (weitere Funktionen optional), mit BNC Anschluss (zur Installation), Audio Ein-/ Ausgang (G.711), PoE, 12 VDC, 144mmØ x 121mm (H), 520g",780]
[null,null,"ZN-DNT352XE-M","H.264 2 Megapixel Dome, mechanische Tag/Nachtkamera, 1/2.7\"- CMOS, Brennweite 3,0 mm - 9,0mm, Fokus und Zoom per Remote einstellbar, F1.2, 1,0 Lux (Farbe / 0,001 Lux (s/w), effektive Auflösung 1920x1080 (einstellbar), 25B/s, Dual stream,  inkl. Video Analyse Software (weitere Funktionen optional), mit BNC Anschluss (zur Installation), Audio Ein-/ Ausgang (G.711), PoE, 12 VDC, 115mmØ x 129mm (H), IP66, 1,2kg",740]
[null,null,"ZN-DNT352XE-MIR","H.264 2 Megapixel IR Dome, mechanische Tag/Nachtkamera, 1/2.7\"- CMOS, Brennweite 3,0 mm - 9,0mm, Fokus und Zoom per Remote einstellbar, F1.2, 1,0 Lux (Farbe / 0 Lux (s/w IR on), effektive Auflösung 1920x1080 (einstellbar), 25B/s, Dual stream,  inkl. Video Analyse Software (weitere Funktionen optional), mit BNC Anschluss (zur Installation), Audio Ein-/ Ausgang (G.711), PoE, 12 VDC, 155mmØ x 129mm (H), IP66, 1,2kg",920]
[null,"Bullet"]
[null,null,"ZN1-B4NVD43","H.264 Bulletkamera, 2.0 MP Full-HD, 25bps, 3-9mm, MFZ, PoE/DC12V, MicroSD, IP66, VCA",580]
[null,null,"ZN1-B4NMZ56","H.264 Bulletkamera, 2.0MP Full-HD, 3-9mm, 1/2.9\", IR-LEDs, IP66, VCA",630]
[null,"Pinhole"]
[null,null,"ZN1-V4FN3","H.264 Pinhole-Kamera, 2.0MP Full-HD, 25bps, 2.8mm, 1/3\" CMOS, VCA",570]
[null,"PTZ"]
[null,null,"ZN-PTZ202XE","H.264 PTZ Innendome, 30 bps @ Full-HD, 1/3\" CMOS, mechaniische Tag/Nachtkamera, 1.5 Lux (50 IRE) (Farbe), 0.1 Lux (s/W), 20x optischer Zoom, 8x digitalzoom, DSS, inkl. auto-tracking und VCA",2690]
[]
[null,null,"ZN-PTZ202XE-XT","H.264 PTZ Außendome, 30 bps @ Full-HD, 1/3\" CMOS, mechaniische Tag/Nachtkamera, 1.5 Lux (50 IRE) (Farbe), 0.1 Lux (s/W), 20x optischer Zoom, 8x digitalzoom, DSS, inkl. auto-tracking und VCA, IP66",2980]
["IP-Server",null,null,"     "]
[null,"Server",null,"     "]
[null,null,"ZA-NVE12K","19\" Netzwerk Video Encoder Lösung bis zu 12 Kanälen/Rack, 1HE, 3 Karteneinschubstellen (HotSwap), inklusive Weitbereichsnetzteil (85~264VAC/43~63Hz/2A), (BxHxT) 482x44x286 mm, 1,8Kg ohne Einsteckkarten (370g/Karte), unterstützte Einschubkarten ZN-RS4012AE oder ZN-RS4012VE",660]
[null,null,"ZA-NVE40K","19\" Netzwerk Video Encoder Lösung bis zu 40 Kanälen, 4HE, 10 Karteneinschubstellen (HotSwap), inklusive Weitbereichsnetzteil (90~264VAC/43~63Hz/2A), (BxHxT) 482x177x325 mm, 6,9Kg ohne Einsteckkarten (380g/Karte), unterstützte Einschubkarten ZN-RS4040AE oder ZN-RS4040VE",2040]
[null,null,"ZS1-4DB1","H.264/MJPEG, 4ch Video Encoder Blade, fps100/120@D1, Audio In2/Out1, DC12V, Video Analytics (Intrusion detection. Advanced VCA optional)",800]
[null,null,"ZS1-4DB2","H.264/MJPEG, 4ch Video Encoder Blade, fps100/120@D1, Audio In2/Out1, DC12V, Video Analytics (Intrusion detection. Advanced VCA optional)",800]
["VCA / Video Contents Analytic für GXi "]
[null,"Inklusivlizenzen - bereits in der Hardware integriert"]
[null,null,"ZNS-PRES1","40 Detektionszonen, Manipulationserkennung (Tamper detection), On-Screen Zähler (On-screen counters), Zähllinie (Counting line)","inklusiv"]
[null,null,"ZNS-PRES","40 Detektionszonen, Manipulationserkennung (Tamper detection), Verfolgungsfilter (Tailgating filter), On-Screen Zähler (On-screen counters), Zähllinie (Counting line)","inklusiv"]
[null,"Optionale Lizenzen"]
[null,null,"ZNS-COUNT","40 Detektionszonen, Manipulationserkennung (Tamper detection), On-Screen Zähler (On-screen counters), Zähllinie (Counting line)",105]
[null,null,"ZNS-ACCESS","40 Detektionszonen, Manipulationserkennung (Tamper detection), Verfolgungsfilter (Tailgating filter), On-Screen Zähler (On-screen counters), Zähllinie (Counting line)\n",125]
[null,null,"ZNS-DETECT","40 Detektionszonen, Manipulationserkennung (Tamper detection), Beseitigung von Kamerawacklern (Camera shake elimination), Überwachungs-Tracker (Surveillance tracker), Anwesenheitserkennung (Presence filter), Klassifizierungs- und Geschwindigkeitsfilter und Kalibrierung (Class and speed filter and calibration), Richtungs- und Verweilfilter (Direction and dwell filters)",125]
[null,null,"ZNS-FOLLOW","Manipulationserkennung (Tamper detection), Beseitigung von Kamerawacklern (Camera shake elimination), Überwachungs-Tracker (Surveillance tracker), PTZ automatische Verfolgung (PTZ Auto-tracking)",190]
[null,null,"ZNS-SURV","40 Detektionszonen, Manipulationserkennung (Tamper detection), Beseitigung von Kamerawacklern (Camera shake elimination), Überwachungs-Tracker (Surveillance tracker), Filter und verlassene / entnommene Objekterkennung (Full filter set and abandoned / removed object), Klassifizierungs- und Geschwindigkeitsfilter und Kalibrierung (Class and speed filter and calibration), Verfolgungsfilter (Tailgating filter), On-Screen Zähler (On-screen counters), Meta-Daten (Meta data)",170]
[null,null,"ZNS-PRO","40 Detektionszonen, Manipulationserkennung (Tamper detection), Beseitigung von Kamerawacklern (Camera shake elimination), Überwachungs-Tracker (Surveillance tracker), Anwesenheitserkennung (Presence filter), Filter und verlassene / entnommene Objekterkennung (Full filter set and abandoned / removed object), Klassifizierungs- und Geschwindigkeitsfilter und Kalibrierung (Class and speed filter and calibration), Verfolgungsfilter (Tailgating filter), On-Screen Zähler (On-screen counters), Meta-Daten (Meta data), Personenverfolgung (People tracker), Zähllinie (Counting line)",250]
[null,null,"ZNS-ADVANCEDIP","40 Detektionszonen, Manipulationserkennung (Tamper detection), Beseitigung von Kamerawacklern (Camera shake elimination), Überwachungs-Tracker (Surveillance tracker), Filter und verlassene / entnommene Objekterkennung (Full filter set and abandoned / removed object), Klassifizierungs- und Geschwindigkeitsfilter und Kalibrierung (Class and speed filter and calibration), Verfolgungsfilter (Tailgating filter), On-Screen Zähler (On-screen counters), Meta-Daten (Meta data), Zähllinien",210]
[null,null,"ZNS-TRACK","40 Detektionszonen, Manipulationserkennung (Tamper detection), Beseitigung von Kamerawacklern (Camera shake elimination), Überwachungs-Tracker (Surveillance tracker), Anwesenheitserkennung (Presence filter), Filter und verlassene / entnommene Objekterkennung (Full filter set and abandoned / removed object), Klassifizierungs- und Geschwindigkeitsfilter und Kalibrierung (Class and speed filter and calibration), Verfolgungsfilter (Tailgating filter), On-Screen Zähler (On-screen counters), Meta-Daten (Meta data), PTZ automatische Verfolgung (PTZ Auto-tracking)",350]
["Zubehör GXi",null,null,"     "]
[null,null,"ZNA-POEExtender","Spannungsversorgung für PoE Kameras",40]
[null,null,"ZCA-220-3.0A","Netzteil zur Innenmontage, 24 VAC, 3.0 A     ",90]
[null,null,"ZCA-PSU220","Außennetzteil (IP66) mit Alarm- und Anschlußverteilung, 24 VAC, 3,1 A        ",253]
[null,null,"JBK-U100","Anschlussbox",110]
[null,"ZN-DN312XE-M/ZN-DNT352XE-M"]
[null,null,"WMB-3000","Wandmontageadapter",60]
[null,null,"CMB-3000","Deckenmontageadapter",80]
[null,null,"CMA-3000","Eckmontageadapter",80]
[null,null,"PMA-3000","Mastmontageadapter",80]
[null,null,"GBP-35XX","Montagebox Adapterplatte",20]
[null,null,"SD-35XX","Getönte Kuppel",10]
[null,"ZN-DN312XE"]
[null,null,"FMB-3102","Unterputz Montageadapter",120]
[null,"ZN-DNT352XE"]
[null,null,"FMB-3502","Unterputz Montageadapter",120]
[null,"ZN-PTZ202XE-XT"]
[null,null,"WMB-4600","Wandmontageadapter",170]
[null,null,"CMB-4600","Deckenmontageadapter",170]
[null,null,"CMA-4600","Eckmontageadapter",170]
[null,null,"PMA-4600","Mastmontageadapter",130]
[null,"ZN-DNT372XE"]
[null,null,"WMB-3000S","Wandmontageadapter",110]
[null,null,"CMB-3000S","Deckenmontageadapter",120]
[null,null,"FMB-3702","Unterputz Montageadapter",150]
[null,"ZN-DN332XE"]
[null,null,"FMB-3302","Unterputz Montageadapter",120]
[null,"Nautilus PTZ"]
[null,null,"LZN-NDNC30X","Nautilus HD-IP PTZ Camera, 30:1 Optical Zoom, TDN, WDR, Wiper, 4\" PCD Adaptor, IK10, IP67, ONVIF",5800]
[null,null,"LZN-NDNC30X-IR","Nautilus HD-IP PTZ Camera, 30:1 Optical Zoom, TDN, WDR, Wiper, Built in Adaptive LED Illuminator (IR 150m, White Light 100m), 4\" PCD Adaptor, IK10, IP67, ONVIF",6700]
[null,"Nautilus Accessories"]
[null,null,"LZ-NSJCB","Standard PSU",330]
[null,null,"LZ-NIJCB","Intelligent Junction Box PSU c/w Alarms and Outputs",850]
[null,null,"LZ-10MUC","10m Umbilical Cable (purchase with each Nautilus PTZ Camera)",160]
[]
[null,"Service Equipment"]
[null,null,"ZW-N22F","Wireles service equipment, zur Einrichtung  / Installationsunterstützung für IP Kameras",240]

{"sheet":"Analog Cameras & DVR","index":3,"n_rows":171,"n_cols":5,"rows_kept":171,"cut":false,"hidden":false,"merged":[[20,1,20,2],[38,1,38,3],[85,0,85,1],[0,0,0,3]]}
["Analoge Kameras & DVR / Gehäuse"]
[]
[]
[null,null,"Modell","Beschreibung","EURO"]
[null,"Kameraserie 1/3\""]
[null,"GX5"]
[null,null,"ZC-YX270P","1/3\" CCD, Farbkamera, 700 TVL, 0.0003 lux (Farbe) / 0.00003 lux (s/w) F1.2 / 30IRE / Sens-up, DNR, DWDR, BLC, HLC, 16x Digitalzoom, DC-Iris, 12/24VDC, 108.4mm x 46mm x 60mm",150]
[null,"Standard ",null,"     "]
[null,null,"ZC-YX280P","1/3\" CCD, Farbkamera, 700TVL, BLC, HLC, OSD, 12VDC/24VAC",150]
[null,null,"ZC-YX280PE","1/3\" CCD, Farbkamera, 700TVL,  BLC, HLC, OSD, 230VAC",150]
[null,null,"ZC-NX280P","1/3\" CCD, Tag/Nacht-Kamera, 700TVL, BLC, HLC, OSD,  12VDC/24VAC",180]
[null,"IR-Bulletkameras "]
[null,null,"ZC-BNT8039PXA","Mechanische Tag/Nacht Außenkamera IP67 mit Varioobjektiv 3,0 - 9,0 mm, DC-gesteuerte Blende (F1,4), 1/3\" IT-CCD, 700 Linien, 0 Lux (IR an), 24 integrierte IR-LEDs, 12 VDC/24 VAC, Kabelführung durch den Wandarm",240]
[null,null,"ZC-BNX8039PBA","Mechanische Tag/Nacht Außenkamera IP67 mit Varioobjektiv 3,0 - 9,0 mm, DC-gesteuerte Blende (F1,4), 1/3\" IT-CCD, 600 Linien, 0 Lux (IR an), 24 integrierte IR-LEDs, 12 VDC/24 VAC, Brennweite und Fokuseinstellung extern einstellbar, Kabelführung durch den Wandarm",240]
[null,"Domekameras",null,"     "]
[null,null,"ZC-D8039PBA","Farbkamera mit Vario-Objektiv 3,0 - 9,0 mm, DC-gesteuerte Blende, 1/3\" IT-CCD, 600 Linien, 0,5 Lux (F1,2) elektronische Farb/SW Umschaltung, 3-achsiges Modul, 12 VDC/24 VAC",160]
[null,null,"ZC-D8039PXA","Farbkamera mit Vario-Objektiv 3,0 - 9,0 mm, DC-gesteuerte Blende, 1/3\" IT-CCD, 700 Linien, 0,5 Lux (F1,2) elektronische Farb/SW Umschaltung, 3-achsiges Modul, 12 VDC/24 VAC",180]
[null,"Domekameras vandalismusgeschützt",null,"     "]
[null,null,"ZC-DNT8039PBA","Außengehäuse mit IP67, Tag/Nacht-Kamera mit Vario-Objektiv 3,0 - 9,0 mm, DC-gesteuerte Blende, 1/3\" IT-CCD, 600 Linien, 0,04 Lux (F1,4) mechanische Farb/SW Umschaltung, 3-achsiges Modul, 12 VDC/24 VAC",210]
[null,null,"ZC-DNT8039PXA","Außengehäuse mit IP67, Tag/Nacht-Kamera mit Vario-Objektiv 3,0 - 9,0 mm, DC-gesteuerte Blende, 1/3\" IT-CCD, 700 Linien, 0,04 Lux (F1,4) mechanische Farb/SW Umschaltung, 3-achsiges Modul, 12 VDC/24 VAC",230]
[null,"Zubehör 8000er Serie"]
[null,null,"ZCA-SM800","Servicekabel für die 8000er Serie, zum Abgreifen des Videosignals",10]
[null,null,"ZCA-FM8T","Unterputz Montageadapter für ZC-DT8000 Außendome",30]
[null,null,"ZC-FM3","Unterputz Montageadapter für ZC-D8000 Innendome",60]
[null,null,"ZCA-PM8T","Adapter zur abgehängten Montage für ZC-DT8000 Außendome",40]
[null,null,"ZC7-WM1","Wandhalter Innendome",70]
[null,null,"ZC8-WM2","Wandhalter Außendome",120]
[null,null,"PMA2","Masthalter für ZC8-WM2A",60]
[null,"Montagearme",null,"     "]
[null,null,"BK140","Montagearm 14 cm, aus Metall, schwarz, wahlweise weiß, Justierung mit Werkzeug     ",10]
[null,null,"BCV140","Montagearm 14 cm, aus Metall, schwarz, wahlweise weiß, Justierung werkzeugfrei mittels Überwurfmuffe     ",13]
[null,null,"BKX","Verlängerung für BK/BCV, 50 mm, schwarz, wahlweise weiß     ",5]
[null,"Power supply units",null,"     "]
[null,null,"CV12P","Steckernetzteil, 12 VDC, 1000 mA     ",35]
[null,null,"CV12UP","Unterputznetzteil, z.B. zum verdeckten Einbau, 12 VDC, 1000 mA",55]
[null,null,"CV12-II","Netzteil zur Festmontage, 12 VDC, 800 mA     ",26]
[null,null,"CV24-II","Netzteil zur Festmontage, 24 VAC, 400 mA     ",26]
[null,null,"CV2416-8A","19“-Rackmontage, Primär Eingang umschaltbar 110/230 8A",700]
[null,"Motordomekamera-System ZC-PT"]
[null,null,"ZC-PT212P","Motordome im Innengehäuse, 12-facher optischer Zoom, 3.8mm - 45.6mm, 1/4'’-CCD, 0.002 lux (Farbe), 0.0002 lux (s/w), 650 TVL, Privatzonen, Tag/Nachtfunktion, WDR, DNR, inkl Netzteil",1000]
[null,null,"ZC-PT212P-XT","Motordome im Außengehäuse, 12-facher optischer Zoom, 3.8mm - 45.6mm, 1/4'’-CCD, 0.002 lux (Farbe), 0.0002 lux (s/w), 650 TVL, Privatzonen, Tag/Nachtfunktion, WDR, DNR, IP66",1200]
[null,null,"ZC-PT236P","Motordome im Innengehäuse, 36-facher optischer Zoom, 3,4 - 120 mm, 1/4\"-CCD ExView, 0,01 Lux, 650 TVL, Privatzonenmaskierung, WDR, DNR",1300]
[null,null,"ZC-PT236P-XT","Motordome im Außengehäuse, 36-facher optischer Zoom, 3,4 - 120 mm, 1/4\"-CCD ExView, 0,01 Lux, 650 TVL, Privatzonenmaskierung, WDR, DNR, IP66",1400]
[null,"Zubehör ZC-PT",null,"     "]
[null,null,"ZCA-SC201","Bedienteil (3-achsig) für ZC-PT Domeserie, max. 223 Domekameras, Steuerung von MPX und DVR     ",930]
[null,null,"ZCA-DS4","RS485 Datenverteiler, 1 Eingang, 4 Ausgänge, 1HE,19\" Gehäuse, benötigt ein 12VDC/8W Netzteil (nicht im Lieferumfang)",450]
[null,null,"ZCA-DS8","RS485 Datenverteiler, 1 Eingang, 8 Ausgänge, 1HE,19\" Gehäuse, benötigt ein 12VDC/8W Netzteil (nicht im Lieferumfang)",500]
[null,null,"ZCA-DS16","RS485 Datenverteiler, 1 Eingang, 16 Ausgänge, 1HE,19\" Gehäuse, benötigt ein 12VDC/8W Netzteil (nicht im Lieferumfang)",550]
[null,null,"ZCA-TB200","Adapter zum Einbau in abgehängte Decken     ",80]
[null,null,"ZCA-TB200A","Adapter zum Einbau in abgehängte Decken für ZC-PT212P     ",45]
[null,null,"ZCA-HC200","Adapter zur Verwendung unter „harten Decken“     ",57]
[null,null,"ZCA-GT100","Einfacher Montagearm zur Adaption an Wand-, Ecken- oder Mastmontageadapter, zur Aufnahme der Innen- und Außengehäuse     ",80]
[null,null,"ZCA-ST25","Rohrverlängerungen für abgehängte Montage, 25 cm, zur Aufnahme der Innen- und Außengehäuse     ",80]
[null,null,"ZCA-ST50","Rohrverlängerungen für abgehängte Montage, 50 cm, zur Aufnahme der Innen- und Außengehäuse     ",92]
[null,null,"ZCA-SP200","Wandhalter",138]
[null,null,"ZCA-PTDM","Mastmontageplatte schmal (232 x 136 mm), ohne Verteilerfunktion, zur Aufnahme des GT200/100     ",92]
[null,null,"ZCA-PWDM","Mastmontageplatte breit (270 x 170 mm), ohne Verteilerfunktion, zur Aufnahme des GT200/100     ",92]
[null,null,"ZCA-PTB","Mastmontagebox schmal (291 x 170 x 250 mm) zur Aufnahme des GT200/100 und direkten Verkabelung am Mast     ",253]
[null,null,"ZCA-PWB","Mastmontagebox breit (270 x 168 x 150 mm) zur Aufnahme des GT200/100 und direkten Verkabelung am Mast     ",253]
[null,null,"ZCA-CST","Eckmontageplatte zur Aufnahme des GT200/100, ohne Verteilerfunktion     ",92]
[null,null,"ZCA-CTB","Eckmontagebox schmal (300 x 164 x 222 mm) zur Aufnahme des GT200/100 und direkten Verkabelung      ",230]
[null,null,"ZCA-CWB","Eckmontagebox breit (232 x 234 x 210 mm) zur Aufnahme des GT200/100 und direkten Verkabelung     ",230]
[null,null,"ZCA-220-1.5A","Netzteil zur Innenmontage für ZC-PT Serie, 24 VAC, 1,5 A     ",69]
[null,null,"ZCA-220-3.0A","Netzteil zur Innenmontage für ZC-PT Serie, 24 VAC, 3,0 A     ",90]
[null,null,"ZCA-PSU220","Außennetzteil (IP66) mit Alarm- und Anschlußverteilung, 24 VAC, 3,1 A     ",253]
[null,null,"ZCA-IPA","Adapter zur Aufnahme der Innengehäuse an das Außenzubehör GT 200 und ST 25/50     ",80]
[null,null,"ZCA-IPA3","Adapter zur Aufnahme des ZC-PT212P für das Außenzubehör GT 100/200 und ST 25/50     ",80]
[null,"Motordomecamera-system ZC-PT336P-IR 360°"]
[null,null,"ZC-PT336P-IR","360° PTZ Außendomekamera, 1/4\" Sony Super HAD CCD, mechanische Tag/Nacht-Kamera, 0.1 Lux (50 IRE): (Tagmodus), 0.01 Lux (ICR On): (Nachtmodus), 36x optischer Zoom, 12x digitaler Zoom, WDR, DNR, integrierte IR-LEDs",3040]
[null,"Zubehör für ZC-PT336P-IR"]
[null,null,"ZCA-CM3","Deckenmontageadapter",110]
[null,null,"ZCA-WM3","Wandmontagearm",130]
[null,null,"ZCA-CMA3","Eckmontageadapter",140]
[null,null,"ZCA-PMA3","Mastmontageadapter",160]
[null,null,"ZCA-PM3","Aufmastmontageadapter",120]
[null,null,"ZCA-SC301","3-Achsen-Controller",650]
[null,null,"ZCA-J307","Anschlussbox inkl. PCB und Kabel",150]
[null,null,"ZCA-J308","Anschlussbox ohne PCB und Kabel",110]
[null,"Nautilus PTZ"]
[null,null,"LZN-NDNC30X","Nautilus 960H Analogue PTZ Camera, 18:1 Optical Zoom, TDN, WDR, Wiper, 4\" PCD Adaptor, IK10, IP67",4000]
[null,null,"LZN-NDNC30X-IR","Nautilus 960H Analogue PTZ Camera, 18:1 Optical Zoom, TDN, WDR, Wiper, Built in Adaptive LED Illuminator (IR 150m, White Light 100m), 4\" PCD Adaptor, IK10, IP67",5000]
[null,"Nautilus Accessories"]
[null,null,"LZ-NSJCB","Standard PSU",330]
[null,null,"LZ-NIJCB","Intelligent Junction Box PSU c/w Alarms and Outputs",850]
[null,null,"LZ-10MUC","10m Umbilical Cable (purchase with each Nautilus PTZ Camera)",160]
["DVR",null,null,"     "]
[null,null,null,"     ","ENG EURO"]
["DigiMaster Serie",null,null,"     "]
[null,null,"DR-4FX1","4-Kanal H.264, Pentaplex, 100bps@960H, 1 x HDD einbaubar, R/T, HDMI, 1 spot out, 4alarm in, 1 alarm out, RS-485, 2xUSB",280]
[null,null,"DR-8FX2","8-Kanal H.264, Pentaplex, 200bps@960H, 2 x HDD einbaubar, R/T, HDMI, 1 spot out, 4alarm in, 1 alarm out, RS-485, 2xUSB",460]
[null,null,"DR-16FX2","16-Kanal H.264, Pentaplex, 400bps@960H, 2 x HDD einbaubar, R/T, HDMI, 1 spot out, 4alarm in, 1 alarm out, RS-485, 2xUSB",580]
[null,null,"DR4H-DVD","4-Kanal Pentaplex Digitalrekorder, H.264 Kompression, LINUX OS,  Bildwiederholrate bei Aufzeichnung 100 B/s (CIF), 50 B/s (2CIF), 25 B/s(4CIF), Smartphone & PDA support, 2 x S-ATA Festplatten einbaubar, bis zu 2 TB, CD/DVD-Brenner, LAN, VGA-Ausgang, Alarm 4xEin-/1xAusgang, RS485, 2 x USB",420]
[null,null,"DR8H-DVD","8-Kanal Pentaplex Digitalrekorder, H.264 Kompression, LINUX OS,  Bildwiederholrate bei Aufzeichnung 200 B/s (CIF), 100 B/s (2CIF), 50 B/s(4CIF), Smartphone & PDA support, 4 x S-ATA Festplatten einbaubar, bis zu 2 TB, CD/DVD-Brenner, LAN, VGA-Ausgang, Alarm 8xEin-/4xAusgang, RS485, 3 x USB",980]
[null,null,"DR-8FX5","8-Kanal H.264, Pentaplex, 200bps@960H, 2HE, 5 x HDD einbaubar, R/T, HDMI, loop-out, 4 spot out, 10 alarm in, 4 alarm out, 2x RS-485, 1x RS-232, 2x LAN, eSATA, 3x USB",1120]
[null,null,"DR16FX5","16-Kanal H.264, Pentaplex, 400bps@960H, 2HE, 5 x HDD einbaubar, R/T, HDMI, loop-out, 4 spot out, 10 alarm in, 4 alarm out, 2x RS-485, 1x RS-232, 2x LAN, eSATA, 3x USB",1250]
[null,"Accessories"]
[null,null,"DR-RM1","Rackmount DR4H",19]
[null,null,"DR-RM2 ","Rackmount DR-xFX5",19]
["AHD"]
[null,null,"DR-4M41A","4CH AHD 1080p, 12bps/1080p, BNC, 4CH audio in, 1CH audio out, 1 VGA & 1 HDMI, 1 RJ45, 2 USB, 1 HDD (optional)",295]
[null,null,"DR-8M41A","8CH AHD 1080p, 12bps/1080p, BNC, 8CH audio in, 1CH audio out, 1 VGA & 1 HDMI, 1 RJ45, 2 USB, 1 HDD (optional)",375]
[null,null,"DR-16M42A","16CH AHD 1080p, 12bps/1080p, BNC, 4CH audio in, 1CH audio out, 1 VGA & 1 HDMI, 1 RJ45, 2 USB, 2 HDD (optional)",950]
[null,null,"DR-16F45AT","16CH AHD /TVI/IP 8 Kanäle, 25bps/1080p, BNC, 16CH audio in, 1CH audio out, 1 VGA & 1 HDMI, 1 RJ45, 3 USB, 5 HDD (optional)",1400]
[null,"HDD 24/7",null,"     "]
[null,null,"ZRS-HDD1000","S-ATA HDD 1TB  WD Purple 24/7",69]
[null,null,"ZRS-HDD2000","S-ATA HDD 2TB  WD Purple 24/7",99]
[null,null,"ZRS-HDD3000","S-ATA HDD 3TB  WD Purple 24/7",129]
[null,null,"ZRS-HDD4000","S-ATA HDD 4TB  WD Purple 24/7",159]
["Ganz Genstar AHD"]
[null,"Domecamera"]
[null,null,"Z8-M4NTFN4LAP","Sensor Sony IMX322, 1920(H)×1080(V),  0.01Lux, F1.2, 3.6mm,  12VDC, mechanische Tag/Nachtumschaltung",132]
[null,null,"Z8-D4NTVF56LAP","Sensor sony IMX322, 1920(H)×1080(V),  0.01Luxm, F1.2, 2.8-12mm,  12VDC, mechanische Tag/Nachtumschaltung \n",189]
[null,"Bulletcamera"]
[null,null,"Z8-N4NFN4AP","Sensor sony IMX322, 1920(H)×1080(V), 0.01Lux, F1.2, 3.6mm, 12VDC, mechanische Tag/Nachtumschaltung",126]
[null,null,"Z8-N4NVF56AP","Sensor sony IMX322, 1920(H)×1080(V), 0.01Lux, F1.2, 2.8-12mm, 12VDC, mechanische Tag/Nachtumschaltung ",183]
[null,null,"Z8-B4NVF56AP","Sensor sony IMX322, 1920(H)×1080(V), 0.01Lux, F1.2, 2.8-12mm, 12VDC,  mechanische Tag/Nachtumschaltung ",189]
["GANZ Lite"]
[null,"Bulletcameras"]
[null,null,"LYB-IR212PS","Bulletcamera IP66, 1/3\" Sony Super HAD CCD, 2.8mm - 12mm, 650 lines, 0 Lux (IR on), IR-LEDs, 12VDC, DSC",110]
[null,null,"LYX-IR622PS","Bulletcamera IP66, 1/3\" Sony Super HAD CCD, 6mm - 22mm, 700 lines, 0 Lux (IR on), IR-LEDs, 12VDC",120]
[null,null,"LYB-IR-212PS-CB","Bulletcamera IP66, 1/3\" Sony Super HAD CCD, 2.8mm - 12mm, 650 lines, 0 Lux (IR on), IR-LEDs, 12VDC, for ceiling mount, DSC",110]
[null,null,"LYB-SIR212PS","Bulletcamera IP66, 1/3\" Sony Super HAD CCDII, 2.8mm - 12mm, 650 lines, 0 Lux (IR on), Smart-IR-LEDs, 12VDC/24 VAC",120]
[null,null,"LYB-SIR622PS","Bulletcamera IP66, 1/3\" Sony Super HAD CCDII, 6mm - 22mm, 650 lines, 0 Lux (IR on), Smart-IR-LEDs, 12VDC/24 VAC, DSC",130]
[null,"Domecameras"]
[null,null,"LDWB212PS-2","Indoor domecamera with 4mm - 9mm lens, 1/3\" Pixim CMOS, 0,1 Lux (F1,2 / 50IRE), 690TVL, WDR, 3DNR, 12 VDC",110]
[null,null,"LFTB-IR3.6PS","Flat domecamera with 3.6mm lens, 1/3\" Sony Effio-E ExView CCD II, 0 Lux (IR on), 650 TVL, 12 VDC, integrated IR-LED, IP66",80]
[null,null,"LTB-IR3.6PS","Outdoorcamera IP66 with fix lens, 1/3\" IT-CCD, 3.6mm, 650 lines, 0 Lux (IR on), integrated IR-LEDs, 12 VDC, DSC",70]
[null,null,"LTB-IR49PS","Outdoor domecamera IP66 with variolens, 1/3\" IT-CCD, 4mm - 9mm, 650 lines, 0 Lux (IR on), integrated IR-LEDs, 12 VDC, DSC",100]
[null,null,"LTX-IR212PS","Outdoor domecamera IP66 with Variolens, 1/3\" IT-CCD, 2.8mm - 12mm, 700 lines, 0 Lux (IR on), integrated IR-LEDs, 12 VDC, DSC",110]
[null,null,"LTNX-IR212PA","Outdoor domecamera IP66 with Variolens 2.8 - 12mm, 1/3\" IT-CCD, 650 lines, 0 Lux (IR on), IR-LEDs with ca. 20m range, 12VDC/24 VAC",160]
[null,"Boxcameras"]
[null,null,"LCNX-PS","CS-mountcamera, 1/3\" 960H High Sensivity CCD, 700 lines, 0.01 Lux, DWDR, BLC, DNR, 12VDC",90]
[null,null,"LCNX-PES","CS-mountcamera, 1/3\" 960H High Sensivity CCD, 700 lines, 0.01 Lux, DWDR, BLC, DNR, 230VAC",100]
[null,null,"LCWB-P-2","CS-Mount WDR Day-/Nightcamera, 690 lines, 1/3\" Pixim CMOS, 0,1 lux, mechanichal day-/night switching, 12VDC/24VAC",160]
[null,null,"LCWB-PE-2","CS-Mount WDR Day-/Nightcamera, 690 lines, 1/3\" Pixim CMOS, 0,1 lux, mechanichal day-/night switching, 230VAC",160]
[null,"DVR"]
[null,null,"LR04","4-channel Triplex Digitalrecorder, H.264 compression, LINUX OS, LAN, VGA-Out, 1x S-ATA HDD possible, up to 2 TB.,  Smartphone & PDA support. Alarm In-/Output, RS485",240]
[null,null,"LR08","8-channel Triplex Digitalrecorder, H.264 compression, LINUX OS, LAN, VGA-Out, 1x S-ATA HDD possible, up to 2 TB.,  Smartphone & PDA support. Alarm In-/Output, RS485",350]
[null,null,"LR16","16-channel Triplex Digitalrecorder, H.264 compression, LINUX OS, LAN, VGA-Out, 1x S-ATA HDD possible, up to 2 TB.,  Smartphone & PDA support. Alarm In-/Output, RS485",520]
["Gehäuse"]
[null,null,"GH-FI","Staubschutzgehäuse (IP66) aus Kunststoff, der GH-FAST Serie, ohne Sonnendach, und Heizung, inkl. Wandarm (GH-FWM)     ",72]
[null,null,"GH-12","IP67, inkl. Sonnenschutzdach und Heizung 12 VDC, ohne Wandarm     ",102]
[null,null,"GH-24","IP67, inkl. Sonnenschutzdach und Heizung 24 VAC, ohne Wandarm     ",102]
[null,null,"GH-230","IP67, inkl. Sonnenschutzdach und Heizung 230 VAC, ohne Wandarm     ",102]
[null,null,null,"     "]
[null,null,"GH-FWC12","Kunststoffgehäuse IP66, inkl. Sonnenschutzdach und Heizung 12 VDC, mit intern vorverkabeltem (90 cm, Koax- u. Netzkabel) Wardarm, beidseitig zu öffnen      ",130]
[null,null,"GH-FWC24","Kunststoffgehäuse IP66, inkl. Sonnenschutzdach und Heizung 24 VAC, mit intern vorverkabeltem (90 cm, Koax- u. Netzkabel) Wardarm, beidseitig zu öffnen     ",130]
[null,null,"GH-FWC230","Kunststoffgehäuse IP66, inkl. Sonnenschutzdach und Heizung 230 VAC, mit intern vorverkabeltem (90 cm, Koax- u. Netzkabel) Wardarm, beidseitig zu öffnen     ",130]
[null,null,"GH-FWU230-G","Kunststoffgehäuse IP66, inkl. Sonnenschutzdach und Heizung 230 VAC, mit intern vorverkabeltem (90 cm, CAT5- u. Netzkabel) Wandarm, beidseitig zu öffnen, Glasscheibe     ",150]
[null,null,"GH-FW230-G","Kunststoffgehäuse IP66, inkl. Sonnenschutzdach und Heizung 230 VAC, mit verdeckter Kabelführung im Wandarm, beidseitig zu öffnen, Glasscheibe     ",130]
[null,null,"GH-FW12","Kunststoffgehäuse IP66, inkl. Sonnenschutzdach und Heizung 12 VDC, mit Wandarm, beidseitig zu öffnen     ",110]
[null,null,"GH-FW24","Kunststoffgehäuse IP66, inkl. Sonnenschutzdach und Heizung 24 VAC, mit Wandarm, beidseitig zu öffnen     ",110]
[null,null,"GH-FW230","Kunststoffgehäuse IP66, inkl. Sonnenschutzdach und Heizung 230 VAC, mit Wandarm, beidseitig zu öffnen     ",110]
[null,null,"GH-F12","Kunststoffgehäuse IP66, inkl. Sonnenschutzdach und Heizung 12 VDC, ohne Wandarm, beidseitig zu öffnen     ",80]
[null,null,"GH-F24","Kunststoffgehäuse IP66, inkl. Sonnenschutzdach und Heizung 24 VAC, ohne Wandarm, beidseitig zu öffnen     ",80]
[null,null,"GH-F-iPaK-P","Kunststoffgehäuse IP66, beidseitig zu öffnen, inkl. Sonnenschutzdach, Wandarm, Heizung und PoE Splitter (GH-SP), 12 VDC für die Heizung und Kameraversorgung",350]
[null,"Zubehör"]
[null,null,"GH-FWM","Wandarm, inkl. Gelenkkopf für GH-F Serie, 20 cm     ",20]
[null,null,"GH-CM","Deckenhalterung für innen liegende Kabelführung für GH-Serie     ",140]
[null,null,"GH-CM2","Deckenhalterung für innen liegende Kabelführung für GH-F Serie     ",159]
[null,null,"GH-SM","Distanzplatte für Wandarm, zur seitlichen Kabelaufputzführung     ",16]
[null,null,"GH-PAR","Mastmontageadapter für Masten von 60 bis 140 mm Ø     ",43]
[null,null,"GH-PS24/12 ","Kameranetzteil 24 VAC/12 VDC, 360 mA     ",45]
[null,null,"GH-PS230/12 ","Kameranetzteil 230 VAC/12 VDC, 360 mA     ",45]
[null,null,"GH-PS230/24 ","Kameranetzteil 230 VAC/24 VAC, 500 mA     ",45]
[null,null,"GH-PS230/12H","Kamera Netzteil für die GH-F Serie, 230 VAC/12VDC 1,5 A     ",55]
[null,null,"GH-B24","Optionaler Lüfter 24VAC für die GH und GH-F Serie     ",59]
[null,null,"GH-B12","Optionaler Lüfter 12 VDC für die GH und GH-F Serie     ",59]
[null,null,"GH-FHT12","Optionale Heizung 12 VDC für die GH-F Serie, Temperaturbereich -40°C - + 50°C     ",59]
[null,null,"GH-FHT24","Optionale Heizung 24 VAC für die GH-F Serie. Temperaturbereich -40°C - + 50°C     ",65]
[null,null,"GH-FHT230","Optionale Heizung 230 VAC für die GH-F Serie. Temperaturbereich -40°C - + 50°C     ",115]

{"sheet":"Monitors","index":4,"n_rows":16,"n_cols":5,"rows_kept":16,"cut":false,"hidden":false,"merged":[]}
["Monitore"]
[null,null,"Modell ","Beschreibung","EURO"]
["LED"]
[null,null,"LME17","LED TFT 17\", max. 1280x1024 @ 60Hz, 5ms, Bildformat 4:3, PAL/NTSC, eingebaute Lautsprecher, 12VDC, VESA 75x75mm (BS M4 x 12 mm Schraube), mit Tischfuß",400]
[null,null,"LME19","LED TFT 19\", max. 1280x1024 @ 60Hz, 5ms, Bildformat 4:3, PAL/NTSC, eingebaute Lautsprecher, 12VDC, VESA 75x75mm (BS M4 x 12 mm Schraube), mit Tischfuß",430]
[null,null,"LME23.6SP","LED TFT, max. 1920x1080 @ 60Hz, 5ms, Bildformat 16:9, PAL/NTSC, eingebaute Lautsprecher, 12VDC, VESA 100x100mm, mit Tischfuß, HDMI-Kabel, Fernbedienung, Bildschirmschutz ",570]
[null,null,"LME32","LED TFT, max. 1920x1080 @ 60Hz, 8.5ms, Bildformat 16:9, PAL/NTSC, eingebaute Lautsprecher, VESA 200mm x 100mm / 200mmx200mm, HDMI-Kabel, Fernbedienung, Stromkabel",1000]
[null,null,"LED2225W","LED TFT 21.5\", max. 1920x1080, built-in loudspeakers, VESA 75x75, with desktop base, VGA/HDMI",94]
[null,null,"LED2455W","LED TFT 23.6\", max. 1920x1080, built-in loudspeakers, VESA 100x100, with desktop base, VGA/HDMI",530]
[null,null,"LED2765W","LED TFT 27\", max. 2560x1440, built-in loudspeakers, VESA 100x100, with desktop base, VGA/HDMI",900]
[null,"Accessoires"]
[null,null,"ZMA-HL3-2-S","LCD- Wandhalter, schwarz, für VESA Standard Lochabstände (75/100/100x200/200), 2-teilig, Wandabstand 18mm, bis zu 35Kg belastbar, für LCD von 23\" bis 37\"",14]
[null,null,"ZMA-H9-2-S","LCD- Wandhalter Neigbar ±6°, schwarz, für VESA Standard Lochabstände (50/75/100), 2-teilig, Wandabstand 40mm, bis zu 20Kg belastbar, für LCD von 10\" bis 30\"",10]
[null,null,"ZMA-H5-1-S","LCD- Wandhalter, Neig-/Schwenkbar ±20°/±10° , schwarz, für VESA Standard Lochabstände (75/100), mit Wasserwaage, mit Kabelaufhängung, mit Einrastfunktion, Wandabstand 75mm, bis zu 20 Kg belastbar, für LCD von 10\" bis 30\"",22]
[null,null,"ZMA-HL4-1-S","LCD-Deckenhalter, Neig-/Schwenkbar ±20°/±135°, mit Kabelführung durch das Halterohr, schwarz, für VESA Standard Lochabstände (50/75/100), bis zu 30Kg belastbar, für LCD von 10\" bis 30\", einstellbare Länge 600 - 850mm",30]
[null,null,"LMA-UWM100","LCD- Wandhalter, für VESA Standard Lochabstände (200x200/300x200/400x100/400x200), bis zu 100 kg belastbar",49]

{"sheet":"Thermal & Low Light","index":5,"n_rows":88,"n_cols":5,"rows_kept":88,"cut":false,"hidden":false,"merged":[]}
["Thermalkameras & Low Light"]
[]
[]
[null,null,"Modell ","Beschreibung","EURO"]
["Genstar IP"]
[null,null,"ZNT8-BA1F33","Ungekühlter Infrarot focal plane array (FPA) Detektor, Spektralbereich 8-14um, Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide, Bildverbesserungsfunktionen, SD-Kartenslot, Onvif Profile S, IP66, DC12V/POE, -10℃ ~ +50℃, 1900g",5178]
[null,null,"ZNT8-BA1F30","Ungekühlter Infrarot focal plane array (FPA) Detektor, Spektralbereich 8-14um, Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide, Bildverbesserungsfunktionen, SD-Kartenslot, Onvif Profile S, IP66, DC12V/POE, -10℃ ~ +50℃, 1900g",5269]
[null,null,"ZNT8-BA1F24","Ungekühlter Infrarot focal plane array (FPA) Detektor, Spektralbereich 8-14um, Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide, Bildverbesserungsfunktionen, SD-Kartenslot, Onvif Profile S, IP66, DC12V/POE, -10℃ ~ +50℃, 1900g",5355]
[null,null,"ZNT8-BA1F25","Ungekühlter Infrarot focal plane array (FPA) Detektor, Spektralbereich 8-14um, Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide, Bildverbesserungsfunktionen, SD-Kartenslot, Onvif Profile S, IP66, DC12V/POE, -10℃ ~ +50℃, 1900g",6348]
[null,null,"ZNT8-BA1F26","Ungekühlter Infrarot focal plane array (FPA) Detektor, Spektralbereich 8-14um, Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide, Bildverbesserungsfunktionen, SD-Kartenslot, Onvif Profile S, IP66, DC12V/POE, -10℃ ~ +50℃, 1900g",7029]
[null,null,"ZNT8-BA1F33-T","Ungekühlter Infrarot focal plane array (FPA) Detektor, Spektralbereich 8-14um,  Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide, Bildverbesserungsfunktionen, Temperaturmesspunkt oder Temperaturkönnen festgelegt werden im Thermalbild, Display und Monitor Temperaturwerte:Höchste/Niedrigste Temperatur, Temperaturmessung, Vollbildanzeige, Alarm: Konfiguration der Alarmbedingungen: Temperaturwarnung, Temperaturalarm, Temperaturänderung, SD-Kartenslot, Onvif Profile S, IP66, DC12V/POE,-10℃ ~ +50℃, 1900g",5472]
[null,null,"ZNT8-BA1F30-T","Ungekühlter Infrarot focal plane array (FPA) Detektor, Spektralbereich 8-14um,  Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide, Bildverbesserungsfunktionen, Temperaturmesspunkt oder Temperaturkönnen festgelegt werden im Thermalbild, Display und Monitor Temperaturwerte:Höchste/Niedrigste Temperatur, Temperaturmessung, Vollbildanzeige, Alarm: Konfiguration der Alarmbedingungen: Temperaturwarnung, Temperaturalarm, Temperaturänderung, SD-Kartenslot, Onvif Profile S, IP66, DC12V/POE,-10℃ ~ +50℃, 1900g",5563]
[null,null,"ZNT8-BA1F24-T","Ungekühlter Infrarot focal plane array (FPA) Detektor, Spektralbereich 8-14um,  Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide, Bildverbesserungsfunktionen, Temperaturmesspunkt oder Temperaturkönnen festgelegt werden im Thermalbild, Display und Monitor Temperaturwerte:Höchste/Niedrigste Temperatur, Temperaturmessung, Vollbildanzeige, Alarm: Konfiguration der Alarmbedingungen: Temperaturwarnung, Temperaturalarm, Temperaturänderung, SD-Kartenslot, Onvif Profile S, IP66, DC12V/POE,-10℃ ~ +50℃, 1900g",5654]
[null,null,"ZNT8-BA1F25-T","Ungekühlter Infrarot focal plane array (FPA) Detektor, Spektralbereich 8-14um,  Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide, Bildverbesserungsfunktionen, Temperaturmesspunkt oder Temperaturkönnen festgelegt werden im Thermalbild, Display und Monitor Temperaturwerte:Höchste/Niedrigste Temperatur, Temperaturmessung, Vollbildanzeige, Alarm: Konfiguration der Alarmbedingungen: Temperaturwarnung, Temperaturalarm, Temperaturänderung, SD-Kartenslot, Onvif Profile S, IP66, DC12V/POE,-10℃ ~ +50℃, 1900g",6348]
[null,null,"ZNT8-BA1F26-T","Ungekühlter Infrarot focal plane array (FPA) Detektor, Spektralbereich 8-14um,  Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide, Bildverbesserungsfunktionen, Temperaturmesspunkt oder Temperaturkönnen festgelegt werden im Thermalbild, Display und Monitor Temperaturwerte:Höchste/Niedrigste Temperatur, Temperaturmessung, Vollbildanzeige, Alarm: Konfiguration der Alarmbedingungen: Temperaturwarnung, Temperaturalarm, Temperaturänderung, SD-Kartenslot, Onvif Profile S, IP66, DC12V/POE,-10℃ ~ +50℃, 1900g",7029]
[null,null,"ZNT8-CA1F33","Ungekühlter Infrarot focal plane array (FPA) Detektor, Spektralbereich 8-14um, Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide, Bildverbesserungsfunktionen, SD-Kartenslot, Onvif Profile S, DC12V/POE,-20℃ ~ +55℃, 700g",5608]
[null,null,"ZNT8-CA1F30","Ungekühlter Infrarot focal plane array (FPA) Detektor, Spektralbereich 8-14um, Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide, Bildverbesserungsfunktionen, SD-Kartenslot, Onvif Profile S, DC12V/POE,-20℃ ~ +55℃, 700g",5197]
[null,null,"ZNT8-CA1F24","Ungekühlter Infrarot focal plane array (FPA) Detektor, Spektralbereich 8-14um, Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide, Bildverbesserungsfunktionen, SD-Kartenslot, Onvif Profile S, DC12V/POE,-20℃ ~ +55℃, 700g",5550]
[null,null,"ZNT8-CA1F25","Ungekühlter Infrarot focal plane array (FPA) Detektor, Spektralbereich 8-14um, Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide, Bildverbesserungsfunktionen, SD-Kartenslot, Onvif Profile S, DC12V/POE,-20℃ ~ +55℃, 700g",6938]
[null,null,"ZNT8-CA1F26","Ungekühlter Infrarot focal plane array (FPA) Detektor, Spektralbereich 8-14um, Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide, Bildverbesserungsfunktionen, SD-Kartenslot, Onvif Profile S, DC12V/POE,-20℃ ~ +55℃, 700g",6938]
[null,null,"ZNT8-CA1F33-T","Ungekühlter Infrarot focal plane array (FPA) Detektor, Spektralbereich 8-14um, Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide, Bildverbesserungsfunktionen, Temperaturmesspunkt oder Temperaturkönnen festgelegt werden im Thermalbild, Display und Monitor Temperaturwerte:Höchste/Niedrigste Temperatur, Temperaturmessung, Vollbildanzeige, Alarm: Konfiguration der Alarmbedingungen: Temperaturwarnung, Temperaturalarm, Temperaturänderung, SD-Kartenslot,Onvif Profile S, DC12V/POE, -20℃ ~ +55℃, 700g",5608]
[null,null,"ZNT8-CA1F30-T","Ungekühlter Infrarot focal plane array (FPA) Detektor, Spektralbereich 8-14um, Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide, Bildverbesserungsfunktionen, Temperaturmesspunkt oder Temperaturkönnen festgelegt werden im Thermalbild, Display und Monitor Temperaturwerte:Höchste/Niedrigste Temperatur, Temperaturmessung, Vollbildanzeige, Alarm: Konfiguration der Alarmbedingungen: Temperaturwarnung, Temperaturalarm, Temperaturänderung, SD-Kartenslot,Onvif Profile S, DC12V/POE, -20℃ ~ +55℃, 700g",5472]
[null,null,"ZNT8-CA1F24-T","Ungekühlter Infrarot focal plane array (FPA) Detektor, Spektralbereich 8-14um, Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide, Bildverbesserungsfunktionen, Temperaturmesspunkt oder Temperaturkönnen festgelegt werden im Thermalbild, Display und Monitor Temperaturwerte:Höchste/Niedrigste Temperatur, Temperaturmessung, Vollbildanzeige, Alarm: Konfiguration der Alarmbedingungen: Temperaturwarnung, Temperaturalarm, Temperaturänderung, SD-Kartenslot,Onvif Profile S, DC12V/POE, -20℃ ~ +55℃, 700g",5550]
[null,null,"ZNT8-CA1F25-T","Ungekühlter Infrarot focal plane array (FPA) Detektor, Spektralbereich 8-14um, Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide, Bildverbesserungsfunktionen, Temperaturmesspunkt oder Temperaturkönnen festgelegt werden im Thermalbild, Display und Monitor Temperaturwerte:Höchste/Niedrigste Temperatur, Temperaturmessung, Vollbildanzeige, Alarm: Konfiguration der Alarmbedingungen: Temperaturwarnung, Temperaturalarm, Temperaturänderung, SD-Kartenslot,Onvif Profile S, DC12V/POE, -20℃ ~ +55℃, 700g",6511]
[null,null,"ZNT8-CA1F26-T","Ungekühlter Infrarot focal plane array (FPA) Detektor, Spektralbereich 8-14um, Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide, Bildverbesserungsfunktionen, Temperaturmesspunkt oder Temperaturkönnen festgelegt werden im Thermalbild, Display und Monitor Temperaturwerte:Höchste/Niedrigste Temperatur, Temperaturmessung, Vollbildanzeige, Alarm: Konfiguration der Alarmbedingungen: Temperaturwarnung, Temperaturalarm, Temperaturänderung, SD-Kartenslot,Onvif Profile S, DC12V/POE, -20℃ ~ +55℃, 700g",7235]
[null,null,"ZNT8-PC124-T","\"Dual Vision Thermal, Spektralbereich 8-14um, Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide, Bildverbesserungsfunktionen, Temperaturmesspunkt oder Temperaturkönnen festgelegt werden im Thermalbild, Display und Monitor Temperaturwerte:Höchste/Niedrigste Temperatur, Temperaturmessung, Vollbildanzeige, Alarm: Konfiguration der Alarmbedingungen: Temperaturwarnung, Temperaturalarm, Temperaturänderung, Vision:1/2.8\"\" Sony COMS Sensor, 1920x1080/25fps(PAL); 1920x1080/30fps(NTSC), 22X ZOOM, ICR, DeFog, AWB, Pan: 0°to 360°;Tilt -90°to 90°, Protokoll Pelco-D, Bitrate 2400/4800/9600/19200 bps, DC9-DC36V , AC24V(Optional),-20℃ ~ +55℃, IP66 ,Onvif Profile S, 10Kg",9657]
[null,null,"ZNT8-PC125-T","\"Dual Vision Thermal, Spektralbereich 8-14um, Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide, Bildverbesserungsfunktionen, Temperaturmesspunkt oder Temperaturkönnen festgelegt werden im Thermalbild, Display und Monitor Temperaturwerte:Höchste/Niedrigste Temperatur, Temperaturmessung, Vollbildanzeige, Alarm: Konfiguration der Alarmbedingungen: Temperaturwarnung, Temperaturalarm, Temperaturänderung, Vision:1/2.8\"\" Sony COMS Sensor, 1920x1080/25fps(PAL); 1920x1080/30fps(NTSC), 22X ZOOM, ICR, DeFog, AWB, Pan: 0°to 360°;Tilt -90°to 90°, Protokoll Pelco-D, Bitrate 2400/4800/9600/19200 bps, DC9-DC36V , AC24V(Optional),-20℃ ~ +55℃, IP66 ,Onvif Profile S, 10Kg",9544]
[null,null,"ZNT8-PC126-T","\"Dual Vision Thermal, Spektralbereich 8-14um, Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide, Bildverbesserungsfunktionen, Temperaturmesspunkt oder Temperaturkönnen festgelegt werden im Thermalbild, Display und Monitor Temperaturwerte:Höchste/Niedrigste Temperatur, Temperaturmessung, Vollbildanzeige, Alarm: Konfiguration der Alarmbedingungen: Temperaturwarnung, Temperaturalarm, Temperaturänderung, Vision:1/2.8\"\" Sony COMS Sensor, 1920x1080/25fps(PAL); 1920x1080/30fps(NTSC), 22X ZOOM, ICR, DeFog, AWB, Pan: 0°to 360°;Tilt -90°to 90°, Protokoll Pelco-D, Bitrate 2400/4800/9600/19200 bps, DC9-DC36V , AC24V(Optional),-20℃ ~ +55℃, IP66 ,Onvif Profile S, 10Kg",10311]
[null,null,"ZNT8-PC135-T","Dual Vision Thermal, Spektralbereich 8-14um,  Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide• Bildverbesserungsfunktionen, Temperaturmesspunkt oder Temperaturkönnen festgelegt werden im Thermalbild, Display und Monitor Temperaturwerte:Höchste/Niedrigste Temperatur, Temperaturmessung, Vollbildanzeige,\nAlarm: Konfiguration der Alarmbedingungen: Temperaturwarnung, Temperaturalarm, Temperaturänderung, Vision: 1/2.8\"\" Sony COMS Sensor, 1920x1080/25fps(PAL); 1920x1080/30fps(NTSC); Super WDR >120dB, ICR,V-F Lens 10 ~320mm, Auto Iris(Optional), Pan: 0°to 360°;Tilt -45°to 45°, Protokoll Pelco-D,Bitrate 2400/4800/9600/19200 bps,DC9-DC36V ,AC24V(Optional),-20℃～+55℃, IP66, Onvif Profile S, 50Kg",38761]
[null,null,"ZNT8-PC134-T","Dual Vision Thermal, Spektralbereich 8-14um,  Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide• Bildverbesserungsfunktionen, Temperaturmesspunkt oder Temperaturkönnen festgelegt werden im Thermalbild, Display und Monitor Temperaturwerte:Höchste/Niedrigste Temperatur, Temperaturmessung, Vollbildanzeige,\nAlarm: Konfiguration der Alarmbedingungen: Temperaturwarnung, Temperaturalarm, Temperaturänderung, Vision: 1/2.8\"\" Sony COMS Sensor, 1920x1080/25fps(PAL); 1920x1080/30fps(NTSC); Super WDR >120dB, ICR,V-F Lens 10 ~320mm, Auto Iris(Optional), Pan: 0°to 360°;Tilt -45°to 45°, Protokoll Pelco-D,Bitrate 2400/4800/9600/19200 bps,DC9-DC36V ,AC24V(Optional),-20℃～+55℃, IP66, Onvif Profile S, 50Kg",31166]
[null,null,"ZNT8-PC136-T","Dual Vision Thermal, Spektralbereich 8-14um,  Bis zu 420x315 pixels, Ausgangs-Auflösung D1/CIF, thermische Empfindlichkeit 50mK, Bildmodi black heat/incandescent/Rainbow/red iron oxide• Bildverbesserungsfunktionen, Temperaturmesspunkt oder Temperaturkönnen festgelegt werden im Thermalbild, Display und Monitor Temperaturwerte:Höchste/Niedrigste Temperatur, Temperaturmessung, Vollbildanzeige,\nAlarm: Konfiguration der Alarmbedingungen: Temperaturwarnung, Temperaturalarm, Temperaturänderung, Vision: 1/2.8\"\" Sony COMS Sensor, 1920x1080/25fps(PAL); 1920x1080/30fps(NTSC); Super WDR >120dB, ICR,V-F Lens 10 ~320mm, Auto Iris(Optional), Pan: 0°to 360°;Tilt -45°to 45°, Protokoll Pelco-D,Bitrate 2400/4800/9600/19200 bps,DC9-DC36V ,AC24V(Optional),-20℃～+55℃, IP66, Onvif Profile S, 50Kg",63139]
[]
["PixelPro Gxi"]
[null,null,"ZN-TH1109VE-07-H","H.264/MPEG4/MJPEG, Netzwerk-Thermalkamera, QVGA(320×240), f=7.5mm (FoV 42.1°), Bildwiederholrate 9Hz, Analog Output Audio I/O, PoE/DC12V, MicroSD, USB, Video Analytics (Advanced VCA optional)",6650]
[null,null,"ZN-TH1109VE-16-H","H.264/MPEG4/MJPEG, Netzwerk-Thermalkamera, QVGA(320×240), f=16.7mm (FoV 18.7°), Bildwiederholrate 9Hz, Analog Output Audio I/O, PoE/DC12V, MicroSD, USB, Video Analytics (Advanced VCA optional)",7480]
[null,null,"ZN-TH1109VE-25-H","H.264/MPEG4/MJPEG, Netzwerk-Thermalkamera, QVGA(320×240), f=25mm (FoV 12.4°), Bildwiederholrate 9Hz, Analog Output Audio I/O, PoE/DC12V, MicroSD, USB, Video Analytics (Advanced VCA optional)",7480]
[null,null,"ZN-TH1109VE-35-H","H.264/MPEG4/MJPEG, Netzwerk-Thermalkamera, QVGA(320×240), f=35mm (FoV 8.9°), Bildwiederholrate 9Hz, Analog Output Audio I/O, PoE/DC12V, MicroSD, USB, Video Analytics (Advanced VCA optional)",8620]
[null,null,"ZN-TH1109VE-50-H","H.264/MPEG4/MJPEG, Netzwerk-Thermalkamera, QVGA(320×240), f=50mm (FoV 6.2°), Bildwiederholrate 9Hz, Analog Output Audio I/O, PoE/DC12V, MicroSD, USB, Video Analytics (Advanced VCA optional)",9180]
[null,null,"ZN-TH110FVE-07-H","H.264/MPEG4/MJPEG, Netzwerk-Thermalkamera, QVGA(320×240), f=7.5mm (FoV 42.1°), Bildwiederholrate 30Hz, Analog Output Audio I/O, PoE/DC12V, MicroSD, USB, Video Analytics (Advanced VCA optional)",6650]
[null,null,"ZN-TH110FVE-16-H","H.264/MPEG4/MJPEG, Netzwerk-Thermalkamera, QVGA(320×240), f=16.7mm (FoV 18.7°), Bildwiederholrate 30Hz, Analog Output Audio I/O, PoE/DC12V, MicroSD, USB, Video Analytics (Advanced VCA optional)",7480]
[null,null,"ZN-TH110FVE-25-H","H.264/MPEG4/MJPEG, Netzwerk-Thermalkamera, QVGA(320×240), f=25mm (FoV 12.4°), Bildwiederholrate 30Hz, Analog Output Audio I/O, PoE/DC12V, MicroSD, USB, Video Analytics (Advanced VCA optional)",7480]
[null,null,"ZN-TH110FVE-35-H","H.264/MPEG4/MJPEG, Netzwerk-Thermalkamera, QVGA(320×240), f=35mm (FoV 8.9°), Bildwiederholrate 30Hz, Analog Output Audio I/O, PoE/DC12V, MicroSD, USB, Video Analytics (Advanced VCA optional)",8620]
[null,null,"ZN-TH110FVE-50-H","H.264/MPEG4/MJPEG, Netzwerk-Thermalkamera, QVGA(320×240), f=50mm (FoV 6.2°), Bildwiederholrate 30Hz, Analog Output Audio I/O, PoE/DC12V, MicroSD, USB, Video Analytics (Advanced VCA optional)",9180]
["GANZ Thermal"]
[null,null,"ZNT6-HAT1FN20-P","Fixed Thermal, 17um, 50 NETD, 320X240 Auflösung, 30 fps, 40 Grad FOV, PAL",3594]
[null,null,"ZNT6-HAT1FN29-P","Fixed Thermal, 17um, 50 NETD, 320X240 Auflösung, 30 fps, 24 Grad FOV, PAL",3792]
[null,null,"ZNT6-HAT1FN23-P","Fixed Thermal, 17um, 50 NETD, 320X240 Auflösung, 30 fps, 16 Grad FOV, PAL",3864]
[null,null,"ZNT6-HAT1FN25-P","Fixed Thermal, 17um, 50 NETD, 320X240 Auflösung, 30 fps, 9 Grad FOV, PAL",4696]
[null,null,"ZNT6-HAT1FN26-P","Fixed Thermal, 17um, 50 NETD, 320X240 Auflösung, 30 fps, 6 Grad FOV, PAL",5870]
[null,null,"ZNT6-HBT1FN20-P","Fixed Thermal, 17um, 50 NETD, 320X240 Auflösung, 9 fps, 40 Grad FOV, PAL",3594]
[null,null,"ZNT6-HBT1FN29-P","Fixed Thermal, 17um, 50 NETD, 320X240 Auflösung, 9 fps, 24 Grad FOV, PAL",3792]
[null,null,"ZNT6-HBT1FN23-P","Fixed Thermal, 17um, 50 NETD, 320X240 Auflösung, 9 fps, 16 Grad FOV, PAL",3864]
[null,null,"ZNT6-HBT1FN25-P","Fixed Thermal, 17um, 50 NETD, 320X240 Auflösung, 9 fps, 9 Grad FOV, PAL",4696]
[null,null,"ZNT6-HBT1FN26-P","Fixed Thermal, 17um, 50 NETD, 320X240 Auflösung, 9 fps, 6 Grad FOV, PAL",5870]
[null,null,"ZNT6-PAT1FN20-P","Pan & Tilt Thermal, 17um, 50 NETD, 320X240 Auflösung, 30 fps, 40 Grad FOV, PAL",5510]
[null,null,"ZNT6-PAT1FN29-P","Pan & Tilt Thermal, 17um, 50 NETD, 320X240 Auflösung, 30 fps, 24 Grad FOV, PAL",5690]
[null,null,"ZNT6-PAT1FN23-P","Pan & Tilt Thermal, 17um, 50 NETD, 320X240 Auflösung, 30 fps, 16 Grad FOV, PAL",5830]
[null,null,"ZNT6-PAT1FN25-P","Pan & Tilt Thermal, 17um, 50 NETD, 320X240 Auflösung, 30 fps, 9 Grad FOV, PAL",6644]
[null,null,"ZNT6-PBT1FN20-P","Pan & Tilt Thermal, 17um, 50 NETD, 320X240 Auflösung, 9 fps, 40 Grad FOV, PAL",5510]
[null,null,"ZNT6-PBT1FN29-P","Pan & Tilt Thermal, 17um, 50 NETD, 320X240 Auflösung, 9 fps, 24 Grad FOV, PAL",5690]
[null,null,"ZNT6-PBT1FN23-P","Pan & Tilt Thermal, 17um, 50 NETD, 320X240 Auflösung, 9 fps, 16 Grad FOV, PAL",5830]
[null,null,"ZNT6-PBT1FN25-P","Pan & Tilt Thermal, 17um, 50 NETD, 320X240 Auflösung, 9 fps, 9 Grad FOV, PAL",6644]
[null,null,"ZNT6-HAT2FN32-P","Fixed Thermal, 17um, 50 NETD, 640X480 Auflösung, 30 fps, 90 Grad FOV, PAL",8130]
[null,null,"ZNT6-HAT2FN21-P","Fixed Thermal, 17um, 50 NETD, 640X480 resolutio, 30 fps, 44 Grad FOV, PAL",7728]
[null,null,"ZNT6-HAT2FN22-P","Fixed Thermal, 17um, 50 NETD, 640X480 Auflösung, 30 fps, 37 Grad FOV, PAL",7678]
[null,null,"ZNT6-HAT2FN24-P","Fixed Thermal, 17um, 50 NETD, 640X480 Auflösung, 30 fps, 25 Grad FOV, PAL",7706]
[null,null,"ZNT6-HAT2FN25-P","Fixed Thermal, 17um, 50 NETD, 640X480 Auflösung, 30 fps, 18 Grad FOV, PAL",7858]
[null,null,"ZNT6-HAT2FN26-P","Fixed Thermal, 17um, 50 NETD, 640X480 Auflösung, 30 fps, 12 Grad FOV, PAL",9038]
[null,null,"ZNT6-HBT2FN32-P","Fixed Thermal, 17um, 50 NETD, 640X480 Auflösung, 9 fps, 90 Grad FOV, PAL",8130]
[null,null,"ZNT6-HBT2FN21-P","Fixed Thermal, 17um, 50 NETD, 640X480 Auflösung, 9 fps, 44 Grad FOV, PAL",7728]
[null,null,"ZNT6-HBT2FN22-P","Fixed Thermal, 17um, 50 NETD, 640X480 Auflösung, 9 fps, 37 Grad FOV, PAL",7678]
[null,null,"ZNT6-HBT2FN24-P","Fixed Thermal, 17um, 50 NETD, 640X480 Auflösung, 9 fps, 25 Grad FOV, PAL",7706]
[null,null,"ZNT6-HBT2FN25-P","Fixed Thermal, 17um, 50 NETD, 640X480 Auflösung, 9 fps, 18 Grad FOV, PAL",7858]
[null,null,"ZNT6-HBT2FN26-P","Fixed Thermal, 17um, 50 NETD, 640X480 Auflösung, 9 fps, 12 Grad FOV, PAL",9038]
[null,null,"ZNT6-PAT2FN21-P","Pan & Tilt Thermal, 17um, 50 NETD, 640X480 Auflösung, 30 fps, 44 Grad FOV, PAL",9938]
[null,null,"ZNT6-PAT2FN22-P","Pan & Tilt Thermal, 17um, 50 NETD, 640X480 Auflösung, 30 fps, 37 Grad FOV, PAL",9964]
[null,null,"ZNT6-PAT2FN24-P","Pan & Tilt Thermal, 17um, 50 NETD, 640X480 Auflösung, 30 fps, 25 Grad FOV, PAL",10118]
[null,null,"ZNT6-PAT2FN25-P","Pan & Tilt Thermal, 17um, 50 NETD, 640X480 Auflösung, 30 fps, 18 Grad FOV, PAL",10236]
[null,null,"ZNT6-PBT2FN21-P","Pan & Tilt Thermal, 17um, 50 NETD, 640X480 Auflösung, 9 fps, 44 Grad FOV, PAL",9938]
[null,null,"ZNT6-PBT2FN22-P","Pan & Tilt Thermal, 17um, 50 NETD, 640X480 Auflösung, 9 fps, 37 Grad FOV, PAL",9964]
[null,null,"ZNT6-PBT2FN24-P","Pan & Tilt Thermal, 17um, 50 NETD, 640X480 Auflösung, 9 fps, 25 Grad FOV, PAL",10118]
[null,null,"ZNT6-PBT2FN25-P","Pan & Tilt Thermal, 17um, 50 NETD, 640X480 Auflösung, 9 fps, 18 Grad FOV, PAL",10236]
[null,null,"WB-1W","Wall mount bracket for fixed Thermal",116]
[null,null,"JB-1W","Ceiling Bracket for fixed Thermal",137]
[null,null,"WMK3-1W","Wall Mount bracket for Pan & Tilt Thermal",250]
["Low Light"]
[null,null,"SSC-9600","2 Megapixel CS-Mount Color Night Vision-Camera, mechanische Tag/Nachtumschaltung, 2/3\" Progressive Scan CMOS, Color 0.005 lux, WDR, DNR, DFOG, Privatzone masking, SDI / BNC Out, 650g",15750]
[null,null,"KC-2000","HD-Color-Night-Vision-Camera, 2/3\" CMOS, CS-Mount, color 0.005 lux , SD-card slot, HDMI-out, integrated microphone, DFOG, DNR, Mic-In, Audio-Out, 1.1kg","auf Anfrage"]

{"sheet":"Raytec","index":6,"n_rows":478,"n_cols":3,"rows_kept":478,"cut":false,"hidden":false,"merged":[]}
["Raytec"]
[]
[]
["Modell ","Beschreibung","EURO"]
["VAR-i8-3","VARIO i8 Adaptive Illumination, triple panel, 850nm with 3 angle options included, 12-24V ",2290]
["VAR-i4-3","VARIO i4 Adaptive Illumination, triple panel, 850nm with 3 angle options included, 12-24V ",1280]
[]
["VAR-i8-2","VARIO i8 Adaptive Illumination, double panel, 850nm with 3 angle options included, 12-24V ",1590]
["VAR-i4-2","VARIO i4 Adaptive Illumination,double panel, 850nm with 3 angle options included, 12-24V ",860]
["VAR-i2-2","VARIO i2 Adaptive Illumination, double panel, 850nm with 3 angle options included, 12-24V ",600]
[]
["**NEW**"]
["VAR-i16-1","VARIO i16 standard pack 10°x10°, 35°x10° and 60°x25° angles included, clear and black, 24V, 850nm",1350]
["VAR-i8-1","VARIO i8 standard pack 10°x10°, 35°x10° and 60°x25° angles included, clear and black, 12-24V, 850nm",810]
["VAR-i4-1","VARIO i4 standard pack 10°x10°, 35°x10° and 60°x25° angles included, clear and black, 12-24V, 850nm",440]
["VAR-i2-1","VARIO i2 standard pack 10°x10°, 35°x10° and 60°x25° angles included, clear and black, 12-24V, 850nm",310]
[]
[null,"940nm options available. Add -C to codes above. Add 10% to price."]
[]
["VARIO White-Light Series"]
["VAR-w8-3","VARIO w8 Adaptive Illumination, triple panel, White-Light with 3 angle options included, 12-24V ",2290]
["VAR-w4-3","VARIO w4 Adaptive Illumination, triple panel, White-Light with 3 angle options included, 12-24V ",1280]
[]
["VAR-w8-2","VARIO w8 Adaptive Illumination, double panel, White-Light with 3 angle options included, 12-24V ",1590]
["VAR-w4-2","VARIO w4 Adaptive Illumination, double panel, White-Light with 3 angle options included, 12-24V ",860]
["VAR-w2-2","VARIO w2 Adaptive Illumination, double panel, White-Light with 3 angle options included, 12-24V",600]
[]
["**NEW**"]
["VAR-w16-1","VARIO w16, standard pack 10°x10°, 35°x10° and 60°x25° angles included, silver and white, 24V, white-light",1350]
["VAR-w8-1","VARIO w8, standard pack 10°x10°, 35°x10° and 60°x25° angles included, silver and white, 12-24V, white-light",810]
["VAR-w4-1","VARIO w4, standard pack 10x10, 35x10 and 60x25 angles included, silver and white, 12-24V, white-light",440]
["VAR-w2-1","VARIO w2, standard pack 10°x10°, 35°x10° and 60°x25° angles included, silver and white, 12-24V, white-light",310]
[]
["Please note: All VARIO illuminators utilise standard Raytec interchangeable lenses."]
[]
[]
["VARIO IP PoE Network Illuminators - Low Voltage"]
[]
["VARIO IP PoE Infra-Red Series – 24V DC Input"]
["VAR-IPPoE-i8-1","VARIO IP PoE Network Illuminator - i8, 850nm with 3 angle options included, 24V DC or PoE++ power input & Cat 5 data input",930]
["VAR-IPPoE-i4-1","VARIO IP PoE Network Illuminator - i4, 850nm with 3 angle options included, 24V DC or PoE+ power input & Cat 5 data input",600]
[null,"940nm options available. Add -C to codes above. Add 10% to price."]
["VARIO IP PoE White-Light Series – 24V DC Input"]
["VAR-IPPoE-w8-1","VARIO IP PoE Network Illuminator - w8, White-Light with 3 angle options included, 24V DC or PoE++ power input & Cat 5 data input",930]
["VAR-IPPoE-w4-1","VARIO IP PoE Network Illuminator - w4, White-Light with 3 angle options included, 24V DC or PoE+ power input & Cat 5 data input",600]
[]
[]
["VARIO Specialist Lighting"]
[]
[]
["VARIO Hybrid - Combined Infra-Red and White-Light in a single unit"]
["VAR-hy8-1 ","VARIO Hybrid 8 Infra-Red 850nm and White-Light, with 3 angle options included, 12-24V ",1010]
["VAR-hy8-1-C ","VARIO Hybrid 8 Infra-Red 940nm and White-Light, with 3 angle options included, 12-24V  ",1120]
[]
[]
["VARIO Lighthouse Kit - Fully integrated lighting and housing solution"]
["VAR-VLK-i4-2","VARIO Lighthouse Kit , 2 x 850nm, 3 angle options, Cat5e and power/aux cable",1170]
["VAR-VLK-i4-2-C","VARIO Lighthouse Kit , 2 x 940nm, 3 angle options, Cat5e and power/aux cable",1250]
["VAR-VLK-w4-2","VARIO Lighthouse Kit , 2 x White-Light, 3 angle options, Cat5e and power/aux cable",1170]
[]
[]
["VARIO D-zoom - High power LED with remotely adjustable beam angle"]
["VAR-DZ -i8-1","VARIO D-Zoom i8, Infra-Red, 850nm – angles 10° to 80°",930]
["VAR-DZ -i8-1-C","VARIO D-Zoom i8, Infra-Red, 940nm – angles 10° to 80°",1020]
["VAR-DZ -w8-1","VARIO D-Zoom w8, White-Light – angles 10° to 80°",930]
[]
["VARIO ESP"]
["Purpose Designed VARIO LED Lighting for the Pelco Esprit “Specific SMR model” "]
["powered directly from the camera"]
[]
["Order x2 VAR-i2-1","For Pelco Esprit SMR # 1-208BV1 "]
["Order x2 VAR-i4-1","For Pelco Esprit  SMR # 1-2BUUEI"]
["Order x2 VAR-i8-1","For Pelco Esprit SMR # 1-26OSZH"]
[]
["Mixed angle combinations available via adjusting the VARIO interchangeable lensing."]
["940nm and White-Light versions available - contact Raytec."]
[]
["VARIO Accessories"]
["Please note: All VARIO illuminators utilise standard Raytec interchangeable lenses (not applicable for VARIO D-Zoom)"]
[]
["VARIO Infra-Red Interchangeable Lenses"]
[]
["**NEW**"]
["VAR-i16-LENS-8030","VARIO i16 lens insert - 80°H x 30°V ",40]
["VAR-i16-LENS-12050","VARIO i16 lens insert - 120°H x 50°V ",40]
["VAR-i8-LENS-8030","VARIO i8 lens insert - 80°H x 30°V ",40]
["VAR-i8-LENS-12050","VARIO i8 lens insert - 120°H x 50°V ",40]
["VAR-i4-LENS-8030","VARIO i4 lens insert - 80°H x 30°V ",40]
["VAR-i4-LENS-12050","VARIO i4 lens insert - 120°H x 50°V ",40]
["VAR-i2-LENS-8030","VARIO i2 lens insert - 80°H x 30°V ",40]
["VAR-i2-LENS-12050","VARIO i2 lens insert - 120°H x 50°V ",40]
[]
["VARIO White-Light Interchangeable Lenses"]
[]
["**NEW**"]
["VAR-w16-LENS-8030","VARIO w16 lens insert -  80°H x 30°V ",40]
["VAR-w16-LENS-12050","VARIO w16 lens insert - 120°H x 50°V ",40]
["VAR-w8-LENS-8030","VARIO w8 lens insert -  80°H x 30°V ",40]
["VAR-w8-LENS-12050","VARIO w8 lens insert - 120°H x 50°V ",40]
["VAR-w4-LENS-8030","VARIO w4 lens insert - 80°H x 30°V",40]
["VAR-w4-LENS-12050","VARIO w4 lens insert - 120°H x 50°V ",40]
["VAR-w2-LENS-8030","VARIO w2 lens insert - 80°H x 30°V ",40]
["VAR-w2-LENS-12050","VARIO w2 lens insert - 120°H x 50°V ",40]
[]
["VARIO Remote Control"]
["(Not applicable for VARIO IP)"]
["VAR-rc-V1","Remote control to enable advanced features in VARIO",50]
[]
[]
["VARIO Power Supply Units"]
["Purpose designed to power all VARIO illuminators including VARIO IP"]
["VAR-PSU-1x2","VARIO PSU - 24V, 20W, 1xO/P for 1x2 series VARIO illuminator",150]
["VAR-PSU-2x4","VARIO PSU - 24V, 50W, 2xO/P for 2x4 series VARIO illuminators",180]
["VAR-PSU-2x8","VARIO PSU - 24V, 100W, 2xO/P for 2x8 series VARIO illuminators",260]
["VAR-PSU-3x8","VARIO PSU - 24V, 150W, 3xO/P for 3x8 series VARIO illuminators",350]
[]
["VARIO Daytime Set-up Tool"]
["VAR-DST","Daytime set-up/positioning tool for all VARIO lighting units ",40]
[]
[]
["PLATINUM IR Series - Ultra High Performance – High Voltage"]
[]
["Includes standard PSU"]
["RM300-PLT-AI-05","RAYMAX 300, 5-15° Platinum Adaptive Illumination, 850nm, inc PSU",2570]
["RM300-PLT-AI-10","RAYMAX 300, 10-30° Platinum Adaptive Illumination, 850nm, inc PSU",2340]
["RM300-PLT-AI-30","RAYMAX 300, 30-90° Platinum Adaptive Illumination, 850nm, inc PSU",2340]
["RM300-PLT-AI-50","RAYMAX 300, 50-180° Platinum Adaptive Illumination, 850nm, inc PSU",2340]
[]
["RM200-PLT-AI-10","RAYMAX 200, 10-20° Platinum Adaptive Illumination, 850nm, inc PSU",1750]
["RM200-PLT-AI-30","RAYMAX 200, 30-60° Platinum Adaptive Illumination, 850nm, inc PSU",1750]
["RM200-PLT-AI-50","RAYMAX 200, 50-100° Platinum Adaptive Illumination, 850nm, inc PSU",1750]
["RM200-PLT-AI-120","RAYMAX 200, 120-180° Platinum Adaptive Illumination, 850nm, inc PSU",1750]
[]
["RM100-PLT-AI-10","RAYMAX 100, 10-20° Platinum Adaptive Illumination, 850nm, inc PSU",1240]
["RM100-PLT-AI-30","RAYMAX 100, 30-60° Platinum Adaptive Illumination, 850nm, inc PSU",1240]
["RM100-PLT-AI-50","RAYMAX 100, 50-100° Platinum Adaptive Illumination, 850nm, inc PSU",1240]
["RM100-PLT-AI-120","RAYMAX 100, 120-180° Platinum Adaptive Illumination, 850nm, inc PSU",1240]
[]
[null,"940nm Options Available. Add -C to codes above. Same price as 10 degree model. 5° versions available for ultimate distance."]
[]
[]
["RAYMAX Series - High Voltage Infra-Red"]
[]
["**NEW**"]
["Panoramic Ultra Series"]
["RM300-AI-PANUT","RAYMAX 300, Panoramic Ultra Illumination, 60-180°x 5°, 850nm, inc PSU",2100]
["RM150-AI-PANUT","RAYMAX 150, Panoramic Ultra Illumination, 60-180°x 5°,  850nm, inc PSU",1470]
[]
["Ultimate Adaptive Illumination Products - Triple Panel"]
["RAYMAX 300 - includes standard PSU"]
["RM300-AI-10","RAYMAX 300, 10-30° Adaptive Illumination, 850nm, inc PSU ",2340]
["RM300-AI-30","RAYMAX 300, 30-90° Adaptive Illumination, 850nm, inc PSU ",2170]
["RM300-AI-50","RAYMAX 300, 50-180° Adaptive Illumination, 850nm, inc PSU",2170]
[null,"940nm Options Available. Add -C to codes above. Same price as 10° model."]
[]
["RAYMAX 150 - includes standard PSU"]
["RM150-AI-30","RAYMAX 150, 30-100° Adaptive Illumination, 850nm, inc PSU",1390]
["RM150-AI-50","RAYMAX 150, 50-180° Adaptive Illumination, 850nm, inc PSU",1390]
[null,"940nm Options Available. Add -C to codes above. Same price as 10° model."]
[]
["Adaptive Illumination Products"]
["RAYMAX 200 - includes standard PSU"]
["RM200-AI-10","RAYMAX 200, 10-20° Adaptive Illumination, 850nm, inc PSU",1750]
["RM200-AI-30","RAYMAX 200, 30-60° Adaptive Illumination, 850nm, inc PSU",1590]
["RM200-AI-50","RAYMAX 200, 50-100° Adaptive Illumination, 850nm, inc PSU",1590]
["RM200-AI-120","RAYMAX 200, 120-180° Adaptive Illumination, 850nm, inc PSU",1590]
[null,"940nm Options Available. Add -C to codes above. Same price as 10° model."]
[]
["RAYMAX 100 - includes standard PSU"]
["RM100-AI-10","RAYMAX 100, 10-20° Adaptive Illumination, 850nm, inc PSU",1240]
["RM100-AI-30","RAYMAX 100, 30-60° Adaptive Illumination, 850nm, inc PSU",920]
["RM100-AI-50","RAYMAX 100, 50-100° Adaptive Illumination, 850nm, inc PSU",920]
["RM100-AI-120","RAYMAX 100, 120-180° Adaptive Illumination, 850nm, inc PSU",920]
[null,"940nm Options Available. Add -C to codes above. Same price as 10° model."]
[]
["RAYMAX 50 - includes standard PSU"]
["RM50-AI-10","RAYMAX 50, 10-20° Adaptive Illumination, 850nm, inc PSU",640]
["RM50-AI-30","RAYMAX 50, 30-60° Adaptive Illumination, 850nm, inc PSU",500]
["RM50-AI-50","RAYMAX 50, 50-100° Adaptive Illumination, 850nm, inc PSU",500]
["RM50-AI-120","RAYMAX 50, 120-180° Adaptive Illumination, 850nm, inc PSU",500]
[null,"940nm Options Available. Add -C to codes above. Same price as 10° model."]
[]
["RAYMAX 25 - includes standard PSU - non AI"]
["RM25-10","RAYMAX 25, 10°, 850nm, inc PSU",420]
["RM25-30","RAYMAX 25, 30°, 850nm, inc PSU",350]
["RM25-50","RAYMAX 25, 50°, 850nm, inc PSU",350]
["RM25-120","RAYMAX 25, 120°, 850nm, inc PSU",350]
[null,"940nm Options Available. Add -C to codes above. Same price as 10° model."]
[]
["Raymax Illuminators with PoE Input - For internal applications only"]
["RAYMAX 25 PoE Series - includes integrated PSU, can be powered via PoE or 12-24V"]
["RM25-10-PoE","RAYMAX 25, 10°, 850nm, PoE compatible",360]
["RM25-30-PoE","RAYMAX 25, 30°, 850nm, PoE compatible",330]
["RM25-50-PoE","RAYMAX 25, 50°, 850nm, PoE compatible",330]
["RM25-120-PoE","RAYMAX 25, 120°, 850nm, PoE compatible",330]
[null,"940nm Options Available. Add -C to codes above. Same price as 10 degree model."]
[]
["Raymax High Power PoE Illuminators with PoE Input - For internal and external applications "]
["RAYMAX 50 PoE Series - includes integrated PSU, powered via PoE"]
["RM50-10-PoE","RAYMAX 50, 10°, 850nm, PoE compatible",530]
["RM50-30-PoE","RAYMAX 50, 30°, 850nm, PoE compatible",490]
["RM50-50-PoE","RAYMAX 50, 50°, 850nm, PoE compatible",490]
["RM50-120-PoE","RAYMAX 50, 120°, 850nm, PoE compatible",490]
[null,"940nm Options Available. Add -C to codes above. Same price as 10 degree model."]
[]
[]
["RAYLUX Series - Hi Voltage White-Light  All RAYLUX products are now powered by PLATINUM technology."]
[]
["Panoramic Series"]
["RL300-AI-PAN","RAYLUX 300, Panoramic Illumination, 60-180°x25°, White-Light inc PSU",2060]
["RL150-AI-PAN","RAYLUX 150, Panoramic Illumination, 60-180°x25°, White-Light inc PSU",1470]
[]
["Raylux Directional Series"]
["Ultimate Adaptive Illumination Products - Triple Panel"]
["RAYLUX 300 - includes standard PSU"]
["RL300-AI-05","RAYLUX 300, 5-15° Adaptive Illumination, White-Light, inc PSU",2570]
["RL300-AI-10","RAYLUX 300, 10-30° Adaptive Illumination, White-Light, inc PSU",2220]
["RL300-AI-30","RAYLUX 300, 30-90° Adaptive Illumination, White-Light, inc PSU",2060]
["RL300-AI-50","RAYLUX 300, 50-180° Adaptive Illumination, White-Light, inc PSU",2060]
[]
["RAYLUX 150 - includes standard PSU"]
["RL150-AI-30","RAYLUX 150, 30-90° Adaptive Illumination, White-Light, inc PSU",1470]
["RL150-AI-50","RAYLUX 150, 50-180° Adaptive Illumination, White-Light, inc PSU",1470]
[]
["Adaptive Illumination Products"]
["RAYLUX 200 - includes standard PSU"]
["RL200-AI-10","RAYLUX 200, 10-20° Adaptive Illumination, White-Light, inc PSU",1630]
["RL200-AI-30","RAYLUX 200, 30-60° Adaptive Illumination, White-Light, inc PSU",1470]
["RL200-AI-50","RAYLUX 200, 50-100° Adaptive Illumination, White-Light, inc PSU",1470]
["RL200-AI-120","RAYLUX 200, 120-180° Adaptive Illumination, White-Light, inc PSU",1470]
[]
["RAYLUX 100 - includes standard PSU"]
["RL100-AI-10","RAYLUX 100, 10-20° Adaptive Illumination, White-Light, inc PSU",1010]
["RL100-AI-30","RAYLUX 100, 30-60° Adaptive Illumination, White-Light, inc PSU",920]
["RL100-AI-50","RAYLUX 100, 50-100° Adaptive Illumination, White-Light, inc PSU",920]
["RL100-AI-120","RAYLUX 100, 120-180° Adaptive Illumination, White-Light, inc PSU",920]
[]
["RAYLUX 50 - includes standard PSU"]
["RL50-AI-10","RAYLUX 50,10-20 degree Adaptive Illumination, White-Light, inc PSU",640]
["RL50-AI-30","RAYLUX 50, 30-60° Adaptive Illumination, White-Light, inc PSU",580]
["RL50-AI-50","RAYLUX 50, 50-100° Adaptive Illumination, White-Light, inc PSU",580]
["RL50-AI-120","RAYLUX 50, 120-180° Adaptive Illumination, White-Light, inc PSU",580]
[]
["RAYLUX 25 - includes standard PSU - non AI"]
["RL25-10","RAYLUX 25, 10°, White-Light, inc PSU",420]
["RL25-30","RAYLUX 25, 30°, White-Light, inc PSU",370]
["RL25-50","RAYLUX 25, 50°, White-Light, inc PSU",370]
["RL25-120","RAYLUX 25, 120°, White Light, inc PSU",370]
[]
["Raylux High Power Poe Illuminators with PoE Input – For internal and external applications "]
["RAYLUX 50 PoE Series - includes integrated PSU, powered via PoE"]
["RL50-10-PoE","RAYLUX 50, 10°, White-Light, PoE compatible",530]
["RL50-30-PoE","RAYLUX 50, 30°, White-Light, PoE compatible",490]
["RL50-50-PoE","RAYLUX 50, 50°, White-Light, PoE compatible",490]
["RL50-120-PoE","RAYLUX 50, 120°, White-Light, PoE compatible",490]
[]
[]
[]
["RAYLUX URBAN Series"]
[]
["Urban - Adaptive Illumination Products (UBA)"]
["Includes standard PSU and environmental protection shield"]
["UBA-48-50","RAYLUX URBAN, 80W Max, 50°+ AI, White-Light, inc PSU",1510]
["UBA-48-120","RAYLUX URBAN, 80W Max, 120°+ AI, White-Light, inc PSU",1510]
["UBA-48-120H-80V","RAYLUX URBAN, 80W Max, 120°+ Horizontal x 80° Vertical, Oval AI, White-Light, inc PSU",1510]
[null,"Warm White Options Available"]
[]
["UBA-32-50","RAYLUX URBAN, 50W Max, 50°+ AI, White-Light, inc PSU",1080]
["UBA-32-120","RAYLUX URBAN, 50W Max, 120°+ AI, White-Light, inc PSU",1080]
["UBA-32-120H-80V","RAYLUX URBAN, 50W Max, 120°+ Horizontal x 80° Vertical, Oval AI, White-Light, inc PSU",1080]
[null,"Warm White Options Available"]
[]
["URBAN - Fixed Illumination Products (UBF)"]
["Includes standard PSU and environmental protection shield"]
["UBF-24-50","RAYLUX URBAN, 40W Max, 50° Illumination, White-Light, inc PSU",860]
["UBF-24-120","RAYLUX URBAN, 40W Max,120° Illumination, White-Light, inc PSU",860]
["UBF-24-120H-80V","RAYLUX URBAN, 40W Max, 120° Horizontal x 80° Vertical, Oval Illumination, White-Light, inc PSU",860]
[null,"Warm White Options Available"]
[]
["UBF-16-50","RAYLUX URBAN, 25W Max, 50° Illumination, White-Light, inc PSU",730]
["UBF-16-120","RAYLUX URBAN, 25W Max,120° Illumination, White-Light, inc PSU",730]
["UBF-16-120H-80V","RAYLUX URBAN, 25W Max, 120° Horizontal x 80° Vertical, Oval Illumination, White-Light, inc PSU",730]
[null,"Warm White Options Available"]
[]
["URBAN PLUS "]
["UBPL-70-001","RAYLUX URBAN PLUS, 79W Max, narrow angle, White-Light, integrated PSU and bracket, 90-305V ac",1870]
["UBPL-70-002","RAYLUX URBAN PLUS, 79W Max, standard angle,White-Light, integrated PSU and bracket,90-305V ac",1870]
["UBPL-70-003","RAYLUX URBAN PLUS, 79W Max, wide angle, White-Light, integrated PSU and bracket, 90-305V ac",1870]
[]
["UBPL-56-001","RAYLUX URBAN PLUS, 61W Max, narrow angle, White-Light, integrated PSU and bracket, 90-305V ac",1630]
["UBPL-56-002","RAYLUX URBAN PLUS, 61W Max, standard angle, White-Light, integrated PSU and bracket, 90-305V ac",1630]
["UBPL-56-003","RAYLUX URBAN PLUS, 61W Max, wide angle, White-Light, integrated PSU and bracket, 90-305V ac",1630]
[]
["UBPL-42-001","RAYLUX URBAN PLUS, 48W Max, narrow angle, White-Light, integrated PSU and bracket, 90-305V ac",1400]
["UBPL-42-002","RAYLUX URBAN PLUS, 48W Max, standard angle, White-Light, integrated PSU and bracket, 90-305V ac",1400]
["UBPL-42-003","RAYLUX URBAN PLUS, 48W Max, wide angle, White-Light, integrated PSU and bracket, 90-305V ac",1400]
[]
[]
["UBBAY-70-N-001","RAYLUX URBAN BAY. 145W max, Neutral White-Light, integrated PSU, rack optimized spread, 90-305V ac",1290]
["UBBAY-70-N-002","RAYLUX URBAN BAY. 145W max, Neutral White-Light, integrated PSU, high optimized spread, 90-305V ac",1290]
["UBBAY-70-N-003","RAYLUX URBAN BAY. 145W max, Neutral White-Light, integrated PSU, area optimized spread, 90-305V ac",1290]
[]
["UBBAY-70-C-001","RAYLUX URBAN BAY. 145W max, Cool White-Light, integrated PSU, rack optimized spread, 90-305V ac",1290]
["UBBAY-70-C-002","RAYLUX URBAN BAY. 145W max, Cool White-Light, integrated PSU, high optimized spread, 90-305V ac",1290]
["UBBAY-70-C-003","RAYLUX URBAN BAY. 145W max, Cool White-Light, integrated PSU, area optimized spread, 90-305V ac",1290]
[]
[]
["SPARTAN Hazardous Area Lighting"]
["ATEX and IEC Ex LED Floodlights for Zone 1 and Zone 2"]
[]
["SPARTAN Flood Infra-Red"]
[]
["SPARTAN Flood IR 12 (Small)"]
["Circular Beam Pattern "]
["SPX-FL12-I-1010","SPARTAN Flood 12 LED, 850nm 10°x10° beam",1650]
["SPX-FL12-I-3030","SPARTAN Flood 12 LED, 850nm 30°x30° beam",1650]
["SPX-FL12-I-5050 ","SPARTAN Flood 12 LED, 850nm 50°x50° beam",1650]
["SPX-FL12-I-120120","SPARTAN Flood 12 LED, 850nm 120°x120° beam",1650]
["Elliptical Beam Pattern "]
["SPX-FL12-I-3510","SPARTAN Flood 12 LED, 850nm 35°x10° beam",1650]
["SPX-FL12-I-6025","SPARTAN Flood 12 LED, 850nm 60°x25° beam",1650]
["SPX-FL12-I-8030","SPARTAN Flood 12 LED, 850nm 80°x30° beam",1650]
["SPX-FL12-I-12050","SPARTAN Flood 12 LED, 850nm 120°x50° beam",1650]
[]
["SPARTAN Flood IR 24 (Medium) "]
["Circular Beam Pattern "]
["SPX-FL24-I-1010","SPARTAN Flood 24 LED, 850nm 10°x10° beam",2110]
["SPX-FL24-I-3030","SPARTAN Flood 24 LED, 850nm 30°x30° beam",2110]
["SPX-FL24-I-5050","SPARTAN Flood 24 LED, 850nm 50°x50° beam",2110]
["SPX-FL24-I-120120","SPARTAN Flood 24 LED, 850nm 120°x120° beam",2110]
["Elliptical Beam Pattern"]
["SPX-FL24-I-3510","SPARTAN Flood 24 LED, 850nm 35°x10° beam",2110]
["SPX-FL24-I-6025","SPARTAN Flood 24 LED, 850nm 60°x25° beam",2110]
["SPX-FL24-I-8030","SPARTAN Flood 24 LED, 850nm 80°x30° beam ",2110]
["SPX-FL24-I-12050","SPARTAN Flood 24 LED, 850nm 120°x50° beam",2110]
[]
["SPARTAN Flood IR 48 (Large)"]
["Circular Beam Pattern "]
["SPX-FL48-I-1010","SPARTAN Flood 48 LED, 850nm 10°x10° beam",4220]
["SPX-FL48-I-3030","SPARTAN Flood 48 LED, 850nm 30°x30° beam",4220]
["SPX-FL48-I-5050","SPARTAN Flood 48 LED, 850nm 50°x50° beam ",4220]
["SPX-FL48-I-120120","SPARTAN Flood 48 LED, 850nm 120°x120° beam",4220]
["Elliptical Beam Pattern "]
["SPX-FL48-I-3510","SPARTAN Flood 48 LED, 850nm 35°x10° beam ",4220]
["SPX-FL48-I-6025","SPARTAN Flood 48 LED, 850nm 60°x25° beam ",4220]
["SPX-FL48-I-8030","SPARTAN Flood 48 LED, 850nm 80°x30° beam ",4220]
["SPX-FL48-I-12050","SPARTAN Flood 48 LED, 850nm 120°x50° beam",4220]
[]
["SPARTAN Flood White-Light"]
[]
["SPARTAN Flood WL 12 (Small) "]
["Circular Beam Pattern"]
["SPX-FL12-W-1010","SPARTAN Flood 12 LED, White-Light 10°x10° beam",1650]
["SPX-FL12-W-3030","SPARTAN Flood 12 LED, White-Light 30°x30° beam",1650]
["SPX-FL12-W-5050","SPARTAN Flood 12 LED, White-Light 50°x50° beam",1650]
["SPX-FL12-W-120120","SPARTAN Flood 12 LED, White-Light 120°x120° beam",1650]
["Elliptical Beam Pattern "]
["SPX-FL12-W-3510","SPARTAN Flood 12 LED, White-Light 35°x10° beam ",1650]
["SPX-FL12-W-6025  ","SPARTAN Flood 12 LED, White-Light 60°x25° beam",1650]
["SPX-FL12-W-8030  ","SPARTAN Flood 12 LED, White-Light 80°x30° beam",1650]
["SPX-FL12-W-12050","SPARTAN Flood 12 LED, White-Light 120°x50° beam",1650]
[]
["SPARTAN Flood WL 24 (Medium)"]
["Circular Beam Pattern"]
["SPX-FL24-W-1010","SPARTAN Flood 24 LED, White-Light 10°x10° beam",2110]
["SPX-FL24-W-3030","SPARTAN Flood 24 LED, White-Light 30°x30° beam",2110]
["SPX-FL24-W-5050","SPARTAN Flood 24 LED, White-Light 50°x50° beam",2110]
["SPX-FL24-W-120120","SPARTAN Flood 24 LED, White-Light 120°x120° beam",2110]
["Elliptical Beam Pattern"]
["SPX-FL24-W-3510  ","SPARTAN Flood 24 LED, White-Light 35°x10° beam",2110]
["SPX-FL24-W-6025","SPARTAN Flood 24 LED, White-Light 60°x25° beam",2110]
["SPX-FL24-W-8030","SPARTAN Flood 24 LED, White-Light 80°x30° beam",2110]
["SPX-FL24-W-12050","SPARTAN Flood 24 LED, White-Light 120°x50° beam",2110]
[]
["SPARTAN Flood WL 48 (Large) "]
["Circular Beam Pattern"]
["SPX-FL48-W-1010  ","SPARTAN Flood 48 LED, White-Light 10°x10° beam",4220]
["SPX-FL48-W-3030  ","SPARTAN Flood 48 LED, White-Light 30°x30° beam",4220]
["SPX-FL48-W-5050  ","SPARTAN Flood 48 LED, White-Light 50°x50° beam",4220]
["SPX-FL48-W-120120  ","SPARTAN Flood 48 LED, White-Light 120°x120° beam",4220]
["Elliptical Beam Pattern "]
["SPX-FL48-W-3510","SPARTAN Flood 48 LED, White-Light 35°x10° beam",4220]
["SPX-FL48-W-6025  ","SPARTAN Flood 48 LED, White-Light 60°x25° beam",4220]
["SPX-FL48-W-8030  ","SPARTAN Flood 48 LED, White-Light 80°x30° beam",4220]
["SPX-FL48-W-12050  ","SPARTAN Flood 48 LED, White-Light 120°x50° beam",4220]
[]
["T4 as standard – Contact Raytec for T5 and T6 Variants"]
[]
["SPARTAN Options"]
["With Photocell","Add ‘-PC’ to the end of the part code."]
["Emergency Versions","Available for all 24 and 48 size models. Add ‘-EM’ to the end of the part code."]
[]
[]
["Specialist Lighting"]
[]
["Hybrid Series – IR + White-Light"]
[]
["HYBRID 300 - includes standard PSU"]
["HY300-10","HYBRID 300, 2 x 10° IR, 850nm, 10° White-Light, AI, inc PSU",2340]
["HY300-30","HYBRID 300, 2 x 30° IR, 850nm, 30° White-Light, AI, inc PSU",2170]
["HY300-50","HYBRID 300, 2 x 50° IR, 850nm, 50° White-Light, AI, inc PSU",2170]
["HY300-120","HYBRID 300, 2 x 120° IR, 850nm, 120° White-Light, AI, inc PSU",2170]
[null,"Mixed angles available."]
[]
["HYBRID 200 - includes standard PSU"]
["HY200-10","HYBRID 200, 10° IR, 850nm, 10° White-Light, AI, inc PSU",1750]
["HY200-30","HYBRID 200, 30° IR, 850nm, 30° White-Light, AI, inc PSU",1590]
["HY200-50","HYBRID 200, 50° IR, 850nm, 50° White-Light, AI, inc PSU",1590]
["HY200-120","HYBRID 200, 120° IR, 850nm, 120° White-Light, AI, inc PSU",1590]
[null,"Mixed angles available."]
[]
["HYBRID 150 - includes standard PSU"]
["HY150-10","HYBRID 150, 2 x 10° IR, 850nm, 10° White-Light, AI, inc PSU",1530]
["HY150-30","HYBRID 150, 2 x 30° IR, 850nm, 30° White-Light, AI, inc PSU",1390]
["HY150-50","HYBRID 150, 2 x 50° IR, 850nm, 50° White-Light, AI, inc PSU",1390]
["HY150-120","HYBRID 150, 2 x 120° IR, 850nm, 120° White-Light, AI, inc PSU",1390]
[null,"Mixed angles available."]
[]
["**NEW**"]
["VARIO Universal Bracketry"]
[]
["VUB-WALL","VARIO Universal Bracket - Wall Mount, incl fixings",30]
["VUB-POLE","VARIO Universal Bracket - Pole Mount, incl fixings",40]
["VUB-PLATE-3x2","VUB Mounting Plate for 3x VARIO 2 series illuminators",40]
["VUB-PLATE-3x4","VUB Mounting Plate for 3x VARIO 4 series illuminators",50]
["VUB-PLATE-3x8","VUB Mounting Plate for 3x VARIO 8 series illuminators",50]
["VUB-PLATE-1x16","VUB Mounting Plate for 1x VARIO 16 series illuminators",20]
["VUB-PLATE-PSU","VUB Mounting Plate for 1x VARIO PSU",40]
[]
["VARIO/ RAYMAX / RAYLUX Bracketry options"]
[]
["SB1","Single Bracket for Top Pan/Tilt mount ",50]
["DB2","Twin Bracket for Top Pan/Tilt mount ",60]
["WB1","Wall Bracket - L Bracket",30]
["PBC-1","Pole Bracket Clamp for 1x RAYMAX or RAYLUX Illuminator",50]
["PBC-2","Pole Bracket Clamp for 2x RAYMAX or RAYLUX Illuminators",90]
["PBC-PSU-ADAP","Adaptor plate to allow the aditional mounting of PSU to pole - see ordering table below",50]
[]
[null,"Pole Mounting Product Combinations"]
[null,"To Mount 1x illuminator (PSU mounted elsewhere)"]
[null,"To Mount 2x illuminators (PSU mounted elsewhere)"]
[null,"To Mount 1x illuminator + 1x PSU (to suit RM/RL25, 50, 100, 200)"]
[null,"To Mount 2x illuminators + 2x PSUs  (to suit RM/RL25, 50, 100, 200)"]
[null,"To Mount 1x RM/RL 300 series illuminator + 1x PSU "]
[]
[]
["RAYLUX Urban Bracketry Options"]
[]
["UB-WB","RAYLUX URBAN, Wall Bracket, 90 Degree, Cable Managed",40]
["UB-TS-S","RAYLUX URBAN, Top Stub Bracket, Single, 90 Degree, Cable Managed",250]
["UB-TS-T","RAYLUX URBAN, Top Stub Bracket, Twin, 90 Degree, Cable Managed",370]
["UB-TS-S-5","RAYLUX URBAN, Top Stub Bracket, Single, 5 Degree Uplift, Cable Managed",250]
["UB-TS-T-5","RAYLUX URBAN, Top Stub Bracket, Twin, 5 Degree Uplift, Cable Managed",370]
["UB-HB-S","RAYLUX URBAN, Hockey Bracket, Single, Cable Managed",420]
["UB-HB-T","RAYLUX URBAN, Hockey Bracket, Twin, Cable Managed",700]
[]
[]
["RAYMAX / RAYLUX Additional Power Supply Options"]
["Special Feature Power Supplies"]
[]
["Twin & Multiple PSUs","Available auf Anfrage"]
[]
["~ PRO PRO Series PSU","Includes photocell following contact for switching of dual mode cameras and 12V dc output for powering cameras PLUS: ",40]
[null,"Platform for upgrade via additional plug in module boards with advanced lighting features"]
[null,"Platform for upgrade via additional plug in module boards with advanced lighting features"]
[null,"TO ORDER: Add ~ PRO to product code, available only with 100 and 200 series."]
[]
[null,"PRO Series PSU’s are not ordered as a separate line item. To order a PRO series PSU, add the PSU part code as "]
[null,"a suffix to the original illuminator part code and add the price of the PSU to the price of the illuminator. "]
[null,"Eg: To order an RM200-AI-30 with a PRO series PSU the part code is RM200-AI-30-PRO."]
[]
["IQ- Module (For PRO PSU)","Additional plug in board for the PRO series PSU offering increased  functionality for all RAYMAX and RAYLUX ",50]
[null,"illuminators. Settings include: Ecologic, Perma Light, Dim, Boost, Detterent, Timer Function."]
[]
["Pulse-Module (for PRO PSU)","Additional plug in board for the PRO series PSU allowing Raytec illuminators to deliver pulsed lighting. ",50]
[null,"Compatible with IR and WL options, both PAL and NTSC cameras and both analogue and digital systems."]
[null,"Note: Plug in PSU modules are ordered as a separate line item and are supplied separatley to the core products."]
[null,"Installation is a simple one click fit into the PRO PSU."]

{"sheet":"Videotec","index":7,"n_rows":596,"n_cols":4,"rows_kept":596,"cut":false,"hidden":false,"merged":[[0,0,0,2]]}
["Videotec"]
[null,"Modell","Beschreibung","EURO"]
[null,"DBH06","Wandhalterung mit interner Kabelführung DBH18",52]
[null,"DBH07","Decken/Brüstungshalterung für DBH18",197]
[null,"DBH18K0F022","MEDUSA Domeumhausung mit Sonnendach und getönter Kuppel (benötigt internen Kameraadapter)",226]
[null,"DBH18K0F028","MEDUSA Domeumhausung mit Sonnendach und klarer Kuppel (benötigt internen Kameraadapter)",226]
[null,"DBHWGC","Mastadapter Ø from 210mm to 225mm (8.2in -8.85in)",86]
[null,"DCJ.3","Matrix und Telemetrie-Keyboard mit three axis joystick",705]
[null,"DCRE485","RS485 data multiplexer, 1 input / 8 outputs",335]
[null,"DCT.2","Matrix, DVR und Telemetrie-Keyboard, Touch-Screen, Drei-Achsen-Joystick",867]
[null,"DCTEL","Matrix und Telemetrie-Keyboard",255]
[null,"DCZ","USB keyboard zur Steuerung von CCTV-Anwendungen vom PC",636]
[null,"DTMRX2","Telemetrieempfänger 12 Funktionen, 230Vac",289]
[null,"DTMRX224","Telemetrieempfänger 12 Funktionen, 24Vac",289]
[null,"DTRX3","Telemetrieempfänger 17 Funktionen, 230Vac",565]
[null,"DTRX324","Telemetrieempfänger 17 Funktionen, 24Vac",565]
[null,"DTRXDC","Telemetrieempfänger 13 Funktionen for PTH355P",451]
[null,"DTWRX","Optionales Board für die Fernsteuerung des Wischers und der Wasserpumpe in stand-alone Gehäuse via RS485. Für die Tanks der WASPT-Serie.",49]
[null,"HEB32K0A000B","HEB Gehäuse 320mm mit Sonnendach",113]
[null,"HEB32K1A000B","HEB Gehäuse 320mm mit Sonnendach und Heizung IN 120/230Vac",137]
[null,"HEB32K2A000B","HEB Gehäuse 320mm mit Sonnendach und Heizung IN 12Vdc/24Vac",137]
[null,"HEG37K0A000","HEG Gehäuse 365mm mit Sonnendach",170]
[null,"HEG37K1A000","HEG Gehäuse 365mm mit Sonnendach und Heizung IN 120/230Vac",192]
[null,"HEG37K1A074","HEG Gehäuse 365mm mit Sonnendach und Doppelheizung IN 120/230Vac",231]
[null,"HEG37K1A143","HEG Gehäuse 365mm mit Sonnendach und lüftergestützte dreifach Heizung IN 120/230Vac, 120W",285]
[null,"HEG37K2A000","HEG Gehäuse 365mm mit Sonnendach und Heizung IN 12Vdc/24Vac",192]
[null,"HEG47K1A000","HEG Gehäuse 450mm mit Sonnendach und Heizung IN 120/230Vac",205]
[null,"HEG47K1A018","HEG Gehäuse 450mm mit Sonnendach, Heizung und Lüfter 230Vac mit Doppelfilter zum Luftaustausch",318]
[null,"HEG47K2A000","HEG Gehäuse 450mm mit Sonnendach und Heizung IN 12Vdc/24Vac",205]
[null,"HEG47K2A016","HEG Gehäuse 450mm mit Sonnendach, Heizung und Lüfter 24Vac mit Doppelfilter zum Luftaustausch",281]
[null,"HEK30K1Y000B","HEK Gehäuse 300mm mit Sonnendach und Heizung IN 120/230Vac",104]
[null,"HEK30K2Y000B","HEK Gehäuse 300mm mit Sonnendach und Heizung IN 12Vdc/24Vac",104]
[null,"HEK30K2Y015B","HEK Gehäuse 300mm mit Sonnendach und lüftergestützte Heizung 24Vac",138]
[null,"HGV52K1A100","HGV Gehäuse 520mm mit Sonnendach, dreifach lüftergestützte Heizung, Wischer 230Vac und Netzteil IN 100-240VAC - OUT 12Vdc",1310]
[null,"HGV52K2A200","HGV Gehäuse 520mm mit Sonnendach, dreifach lüftergestützte Heizung, Wischer 24Vac",1310]
[null,"HOT39D0A000","PUNTO Gehäuse",48]
[null,"HOT39D1A000","PUNTO Gehäuse mit Heizung IN 120/230Vac",59]
[null,"HOT39D1A085","PUNTO Gehäuse mit Heizung IN 120/230Vac und Wandhalterung WBOV2A",84]
[null,"HOT39D2A000","PUNTO Gehäuse mit Heizung IN 12Vdc/24Vac",59]
[null,"HOT39D2A085","PUNTO Gehäuse mit Heizung IN 12Vdc/24Vac und Wandhalterung WBOV2A",84]
[null,"HOT39K1A000","PUNTO Gehäuse mit Sonnendach und Heizung IN 120/230Vac",71]
[null,"HOT39K2A000","PUNTO Gehäuse mit Sonnendach und Heizung IN 12Vdc/24Vac",71]
[null,"HOT39K2A700","PUNTO Hi-PoE Gehäuse for Power Over Ethernet Kameras",168]
[null,"HOV32K1A000","HOV Gehäuse 300mm mit Sonnendach und Heizung IN 120/230Vac",144]
[null,"HOV32K1A018","HOV Gehäuse 300mm mit Sonnendach, Heizung und Lüfter 230Vac mit Doppelfilter zum Luftaustausch",259]
[null,"HOV32K1A100","HOV Gehäuse 300mm mit Sonnendach, Heizung IN 120/230Vac, Wischer 230Vac",435]
[null,"HOV32K2A000","HOV Gehäuse 300mm mit Sonnendach und Heizung IN 12Vdc/24Vac",144]
[null,"HOV32K2A016","HOV Gehäuse 300mm mit Sonnendach, Heizung und Lüfter 24Vac und mit Doppelfilter zum Luftaustausch",223]
[null,"HOV32K2A017","HOV Gehäuse 300mm mit Sonnendach, Heizung und Lüfter 12Vdc mit Doppelfilter zum Luftaustausch",223]
[null,"HOV32K2A147","HOV Gehäuse 300mm mit Sonnendach, Heizung und Lüfter 24Vac mit Doppelfilter zum Luftaustausch, Wischer 24Vac",508]
[null,"HOV32K2A200","HOV Gehäuse 300mm mit Sonnendach, Heizung IN 12Vdc/24Vac, Wischer 24Vac",435]
[null,"HOV32K2A700","HOV Gehäuse for Power Over Ethernet Kameras mit IPM technology",302]
[null,"HOV32K2A716","HOV Gehäuse for Power Over Ethernet Kameras mit IPM technology, Lüfter mit Doppelfilter zum Luftaustausch",339]
[null,"HOV32K2A720","HOV Gehäuse for Power Over Ethernet Kameras mit IPM technology, Heizung für glass de-icing",423]
[null,"HPV36D0A000B","VERSO COMPACT Gehäuse 360mm",69]
[null,"HPV36K0A000B","VERSO COMPACT Gehäuse 360mm mit Sonnendach",80]
[null,"HPV36K1A000B","VERSO COMPACT Gehäuse 360mm mit Sonnendach und Heizung IN 120/230Vac",98]
[null,"HPV36K2A000B","VERSO COMPACT Gehäuse 360mm mit Sonnendach und Heizung IN 12Vdc/24Vac",98]
[null,"HPV36K2A015B","VERSO COMPACT Gehäuse 360mm mit Sonnendach und lüftergestützte Heizung 24Vac",125]
[null,"HPV42K0A000","VERSO Gehäuse 420mm mit Sonnendach",100]
[null,"HPV42K1A000","VERSO Gehäuse 420mm mit Sonnendach und Heizung IN 120/230Vac",118]
[null,"HPV42K1A160","VERSO POLAR Gehäuse 420mm mit Sonnendach und reinforced Heizung für low temperatures (-55°C) IN 120/230Vac, 120W",176]
[null,"HPV42K2A000","VERSO Gehäuse 420mm mit Sonnendach und Heizung IN 12Vdc/24Vac",118]
[null,"HPV42K2A016","VERSO Gehäuse 420mm mit Sonnendach, Heizung und Lüfter 24Vac mit Doppelfilter zum Luftaustausch",209]
[null,"HPV42K2A017","VERSO Gehäuse 420mm mit Sonnendach, Heizung und Lüfter 12Vdc mit Doppelfilter zum Luftaustausch",209]
[null,"HPV42K2A160","VERSO POLAR Gehäuse 420mm mit Sonnendach und reinforced Heizung für low temperatures (-55°C), IN 12Vdc/24Vac, 60W",176]
[null,"HPV42K2A700","VERSO Gehäuse for Power Over Ethernet Kameras mit IPM technology",266]
[null,"HPV42K2A716","VERSO Gehäuse for Power Over Ethernet Kameras mit IPM technology, Lüfter mit Doppelfilter zum Luftaustausch",301]
[null,"HTG37K1A000","HTG Gehäuse 365mm mit Sonnendach und Heizung IN 120/230Vac und Ø55mm Germanium Frontscheibe",1571]
[null,"HTG37K2A000","HTG Gehäuse 365mm mit Sonnendach und Heizung IN 12Vdc/24Vac und Ø55mm Germanium Frontscheibe",1571]
[null,"HTV32K1A000","HTV Gehäuse 300mm mit Sonnendach und Heizung IN 120/230Vac und Ø55mm Germanium Frontscheibe",1479]
[null,"HTV32K2A000","HTV Gehäuse 300mm mit Sonnendach und Heizung IN 12Vdc/24Vac und Ø55mm Germanium Frontscheibe",1479]
[null,"IRH10H8A","Infrarot LED Strahler 10°, Hi-Power, 850nm, 12/24Vdc-24Vac, Reichweite bis zu 140m (460ft)",335]
[null,"IRH10H9A","Infrarot LED Strahler 10°, Hi-Power, 940nm, 12/24Vdc-24Vac, Reichweite bis zu 100m (328ft)",451]
[null,"IRH10L8A","Infrarot LED Strahler 10°, Low-Power, 850nm, 12/24Vdc-24Vac, Reichweite bis zu 100m (328ft)",231]
[null,"IRH30H8A","Infrarot LED Strahler 30°, Hi-Power, 850nm, 12/24Vdc-24Vac, Reichweite bis zu 84m (276ft)",335]
[null,"IRH30H9A","Infrarot LED Strahler 30°, Hi-Power, 940nm, 12/24Vdc-24Vac, Reichweite bis zu 60m (197ft)",451]
[null,"IRH30HWA","LED Strahler Weißlicht 30°, 24Vac - 12/24Vdc, Reichweite bis zu 60m",335]
[null,"IRH30L8A","Infrarot LED Strahler 30°, Low-Power, 850nm, 12/24Vdc-24Vac, Reichweite bis zu 60m (197ft)",231]
[null,"IRH60H8A","Infrarot LED Strahler 60°, Hi-Power, 850nm, 12/24Vdc-24Vac, Reichweite bis zu 56m (184ft)",335]
[null,"IRH60H9A","Infrarot LED Strahler 60°, Hi-Power, 940nm, 12/24Vdc-24Vac, Reichweite bis zu 40m (131ft)",451]
[null,"IRH60HWA","LED Strahler Weißlicht 60°, 24Vac - 12/24Vdc, Reichweite bis zu 40m",335]
[null,"IRH60L8A","Infrarot LED Strahler 60°, Low-Power, 850nm, 12/24Vdc-24Vac, Reichweite bis zu 40m (131ft)",231]
[null,"IRHPS120","Netzteil IN 120Vac 50/60Hz OUT 24Vac 30W",104]
[null,"IRHPS230","Netzteil IN 230Vac 50/60Hz OUT 24Vac 30W",104]
[null,"IRN10A8AS00","Infrarot LED Strahler 10°, 850nm, 100/240Vac, Reichweite bis zu 240m",613]
[null,"IRN10A9AS00","Infrarot LED Strahler 10°, 940nm, 100/240Vac, Reichweite bis zu 140m",948]
[null,"IRN10B8AS00","Infrarot LED Strahler 10°, 850nm, 24Vac-12/24Vdc, Reichweite bis zu 240m",509]
[null,"IRN10B9AS00","Infrarot LED Strahler 10°, 940nm, 24Vac-12/24Vdc, Reichweite bis zu 140m",821]
[null,"IRN30A8AS00","Infrarot LED Strahler 30°, 850nm, 100/240Vac, Reichweite bis zu 130m",613]
[null,"IRN30A9AS00","Infrarot LED Strahler 30°, 940nm, 100/240Vac, Reichweite bis zu 80m",948]
[null,"IRN30AWAS00","LED Strahler Weißlicht 30°, 100/240Vac, Reichweite bis zu 120m",613]
[null,"IRN30B8AS00","Infrarot LED Strahler 30°, 850nm, 24Vac - 12/24Vdc, Reichweite bis zu 130m",509]
[null,"IRN30B9AS00","Infrarot LED Strahler 30°, 940nm, 24Vac - 12/24Vdc, Reichweite bis zu 80m",821]
[null,"IRN30BWAS00","LED Strahler Weißlicht 30°, 24Vac - 12/24Vdc, Reichweite bis zu 120m",509]
[null,"IRN60A8AS00","Infrarot LED Strahler 60°, 850nm, 100/240Vac, Reichweite bis zu 80m",613]
[null,"IRN60A9AS00","Infrarot LED Strahler 60°, 940nm, 100/240Vac, Reichweite bis zu 60m",948]
[null,"IRN60AWAS00","LED Strahler Weißlicht 60°, 100/240Vac, Reichweite bis zu 90m",613]
[null,"IRN60B8AS00","Infrarot LED Strahler 60°, 850nm, 24Vac - 12/24Vdc, Reichweite bis zu 80m",509]
[null,"IRN60B9AS00","Infrarot LED Strahler 60°, 940nm, 24Vac - 12/24Vdc, Reichweite bis zu 60m",821]
[null,"IRN60BWAS00","LED Strahler Weißlicht 60°, 24Vac - 12/24Vdc, Reichweite bis zu 90m",509]
[null,"NTC2K1309","Thermalkamera mit ungekühltem VOx Microbolometer Thermalsensor, 9mm lens, 7.5-8.3Hz, 320x256, Edelstahl-Gehäuse, 24Vac",7742]
[null,"NTC2K1313","Thermalkamera mit ungekühltem VOx Microbolometer Thermalsensor, 13mm lens, 7.5-8.3Hz, 320x256, Edelstahl-Gehäuse, 24Vac",7742]
[null,"NTC2K1319","Thermalkamera mit ungekühltem VOx Microbolometer Thermalsensor, 19mm lens, 7.5-8.3Hz, 320x256, Edelstahl-Gehäuse, 24Vac",7742]
[null,"NTC2K1325","Thermalkamera mit ungekühltem VOx Microbolometer Thermalsensor, 25mm lens, 7.5-8.3Hz, 320x256, Edelstahl-Gehäuse, 24Vac",8752]
[null,"NTC2K1335","Thermalkamera mit ungekühltem VOx Microbolometer Thermalsensor, 35mm lens, 7.5-8.3Hz, 320x256, Edelstahl-Gehäuse, 24Vac",8752]
[null,"NTC2K1350","Thermalkamera mit ungekühltem VOx Microbolometer Thermalsensor, 50mm lens, 7.5-8.3Hz, 320x256, Edelstahl-Gehäuse, 24Vac",10098]
[null,"NTC2K1360","Thermalkamera mit ungekühltem VOx Microbolometer Thermalsensor, 60mm lens, 7.5-8.3Hz, 320x256, Edelstahl-Gehäuse, 24Vac",12455]
[null,"NTC2K1609","Thermalkamera mit ungekühltem VOx Microbolometer Thermalsensor, 9mm lens, 7.5-8.3Hz, 640x512, Edelstahl-Gehäuse, 24Vac",13801]
[null,"NTC2K1613","Thermalkamera mit ungekühltem VOx Microbolometer Thermalsensor, 13mm lens, 7.5-8.3Hz, 640x512, Edelstahl-Gehäuse, 24Vac",13801]
[null,"NTC2K1619","Thermalkamera mit ungekühltem VOx Microbolometer Thermalsensor, 19mm lens, 7.5-8.3Hz, 640x512, Edelstahl-Gehäuse, 24Vac",13801]
[null,"NTC2K1625","Thermalkamera mit ungekühltem VOx Microbolometer Thermalsensor, 25mm lens, 7.5-8.3Hz, 640x512, Edelstahl-Gehäuse, 24Vac",14699]
[null,"NTC2K1635","Thermalkamera mit ungekühltem VOx Microbolometer Thermalsensor, 35mm lens, 7.5-8.3Hz, 640x512, Edelstahl-Gehäuse, 24Vac",14699]
[null,"NTC2K1650","Thermalkamera mit ungekühltem VOx Microbolometer Thermalsensor, 50mm lens, 7.5-8.3Hz, 640x512, Edelstahl-Gehäuse, 24Vac",16157]
[null,"NTC2K1660","Thermalkamera mit ungekühltem VOx Microbolometer Thermalsensor, 60mm lens, 7.5-8.3Hz, 640x512, Edelstahl-Gehäuse, 24Vac",18401]
[null,"NTL1K1000","Large Edelstahl-Gehäuse mit Sonnendach, Heizung IN 120/230Vac und Ø55mm (2.1in) Germanium Frontscheibe",3366]
[null,"NTL1K1300","Large Edelstahl-Gehäuse mit Sonnendach, Heizung IN 120/230Vac und Ø70mm (2.8in) Germanium Frontscheibe",5049]
[null,"NTL1K1500","Large Edelstahl-Gehäuse mit Sonnendach, Heizung IN 120/230Vac und Ø110mm (4.3in) Germanium Frontscheibe",7630]
[null,"NTM1K1000","Edelstahl-Gehäuse mit Sonnendach, Heizung IN 120/230Vac und Ø55mm (2.1in) Germanium Frontscheibe",2693]
[null,"NTW0K2000","Flüssigkeitgekühltes Edelstahl-Gehäuse equipped mit Zinc Selenide glass for Thermalkameras, wavelength 7.5 - 14μm (up to 200°C/500°F)",5835]
[null,"NTW0K3000","Flüssigkeitgekühltes Edelstahl-Gehäuse equipped mit Sapphire glass for shortwave Thermalkameras, wavelength 0.75 – 4.5 μm (up to 400°C/752°F)",2693]
[null,"NXCOL","Pole mount adaptor for NXWBS1, NXWBPT und NXWBL",277]
[null,"NXCW","Corner mount adaptor for NXWBS1, NXWBPT und NXWBL",139]
[null,"NXFIGRU","Filtering group for compressed air cleaning",668]
[null,"NXFWBT","Edelstahl- parapet mount for NXPTH P&T",216]
[null,"NXL1K1000","Edelstahl-Gehäuse mit Sonnendach und Heizung IN 120/230Vac",1987]
[null,"NXL2K1000","Edelstahl-Gehäuse mit Sonnendach und Heizung IN 12Vdc/24Vac",1987]
[null,"NXM0D1000B","Edelstahl-Gehäuse",1000]
[null,"NXM1K1000B","Gehäuse mit Sonnendach und Heizung IN 120/230Vac, 40W",1098]
[null,"NXM1K1050","Edelstahl-Gehäuse mit Sonnendach und double Heizung IN 120/230Vac, 80W",1144]
[null,"NXM2K1000B","Edelstahl-Gehäuse mit Sonnendach und Heizung IN 12Vdc/24Vac, 20W",1098]
[null,"NXM36D0000","Edelstahl-Gehäuse 360mm",665]
[null,"NXM36K1000","Edelstahl-Gehäuse 360mm mit Sonnendach und Heizung IN 120/230Vac, 40W",728]
[null,"NXM36K1050","Edelstahl-Gehäuse 360mm mit Sonnendach und double Heizung IN 120/230Vac, 80W",763]
[null,"NXM36K2000","Edelstahl-Gehäuse 360mm mit Sonnendach und Heizung IN 12Vdc/24Vac, 20W",728]
[null,"NXPTH210","Edelstahl- Pan & Tilt 230Vac, 50/60Hz, mit preset, max load 40kg (88lb)",4264]
[null,"NXPTH211","Edelstahl- Pan & Tilt 24Vac, 50/60Hz, mit preset, max load 40kg (88lb)",4264]
[null,"NXPTZ1PVW0000A","NXPTZ in AISI316L, 230Vac, mit Tag/Nacht Kamera 36x PAL, Wischer",8303]
[null,"NXPTZ1PVW0Z00A","NXPTZ in AISI316L, IP version (H.264/AVC),  230Vac, mit Tag/Nacht Kamera 36x, Wischer",8842]
[null,"NXPTZ2NVW0000A","NXPTZ in AISI316L, 24Vac, mit Tag/Nacht Kamera 36x NTSC, Wischer",8303]
[null,"NXPTZ2PVW0000A","NXPTZ in AISI316L, 24Vac, mit Tag/Nacht Kamera 36x PAL, Wischer",8303]
[null,"NXPTZ2PVW0Z00A","NXPTZ in AISI316L, IP version (H.264/AVC), 24Vac, mit Tag/Nacht Kamera 36x PAL, Wischer",8842]
[null,"NXPTZ3NVW0000A","NXPTZ in AISI316L, 120Vac, mit Tag/Nacht Kamera 36x NTSC, Wischer",8303]
[null,"NXPTZ3PVW0Z00A","NXPTZ in AISI316L, IP version (H.264/AVC), 120Vac, mit Tag/Nacht Kamera 36x, Wischer",8842]
[null,"NXPTZCOL","Pole mount adaptor",342]
[null,"NXPTZCW","Corner mount adaptor",250]
[null,"NXPTZT1PAW0000A","NXPTZT Edelstahl- positioning unit 230Vac, mit Tag/Nacht Kamera 36x PAL, Thermalkamera 35mm, 320x256, 7.5-8.3Hz, Wischer",17391]
[null,"NXPTZT1PAW0000AH","NXPTZT Edelstahl- positioning unit 230Vac, mit Tag/Nacht Kamera 36x PAL, Thermalkamera 35mm, 320x256, 25Hz, Wischer",17728]
[null,"NXPTZT1PAW0Z00A","NXPTZT in AISI 316L, IP H.264 version, 230Vac, mit Tag/Nacht Kamera 36x,Thermalkamera 35mm, 320x256, 7.5-8.3Hz, Wischer",17930]
[null,"NXPTZT1PAW0Z00AH","NXPTZT in AISI 316L, IP H.264 version, 230Vac, Tag/Nacht Kamera 36x,Thermalkamera 35mm, 320x256, 25Hz, Wischer",18267]
[null,"NXPTZT1PBW0000A","NXPTZT Edelstahl- positioning unit 230Vac, mit Tag/Nacht Kamera 36x PAL, Thermalkamera 25mm, 320x256, 7.5-8.3Hz, Wischer",17391]
[null,"NXPTZT1PBW0000AH","NXPTZT Edelstahl- positioning unit 230Vac, mit Tag/Nacht Kamera 36x PAL, Thermalkamera 25mm, 320x256, 25Hz, Wischer",17728]
[null,"NXPTZT1PBW0Z00A","NXPTZT in AISI 316L, IP H.264 version, 230Vac, mit Tag/Nacht Kamera 36x,Thermalkamera 25mm, 320x256, 7.5-8.3Hz, Wischer",17930]
[null,"NXPTZT1PBW0Z00AH","NXPTZT in AISI 316L, IP H.264 version, 230Vac, Tag/Nacht Kamera 36x,Thermalkamera 25mm, 320x256, 25Hz, Wischer",18267]
[null,"NXPTZT1PDW0000A","NXPTZT in AISI 316L, 230Vac, Tag/Nacht Kamera 36x, PAL, Thermalkamera 35mm, 640x512, 7.5-8.3Hz, Wischer",24769]
[null,"NXPTZT1PDW0000AH","NXPTZT in AISI 316L, 230Vac, Tag/Nacht Kamera 36x, PAL, Thermalkamera 35mm, 640x512, 25-30Hz, Wischer",25105]
[null,"NXPTZT1PDW0Z00A","NXPTZT in AISI 316L, IP H.264 version, 230Vac, Tag/Nacht Kamera 36x, Thermalkamera 35mm, 640x512, 7.5-8.3Hz, Wischer",25307]
[null,"NXPTZT1PDW0Z00AH","NXPTZT in AISI 316L, IP H.264 version, 230Vac, Tag/Nacht Kamera 36x, Thermalkamera 35mm, 640x512, 25-30Hz, Wischer",25644]
[null,"NXPTZT1PEW0000A","NXPTZT in AISI 316L, 230Vac, Tag/Nacht Kamera 36x, PAL, Thermalkamera 25mm, 640x512, 7.5-8.3Hz, Wischer",24769]
[null,"NXPTZT1PEW0000AH","NXPTZT in AISI 316L, 230Vac, Tag/Nacht Kamera 36x, PAL, Thermalkamera 25mm, 640x512, 25-30Hz, Wischer",25105]
[null,"NXPTZT1PEW0Z00A","NXPTZT in AISI 316L, IP H.264 version, 230Vac, Tag/Nacht Kamera 36x, Thermalkamera 25mm, 640x512, 7.5-8.3Hz, Wischer",25307]
[null,"NXPTZT1PEW0Z00AH","NXPTZT in AISI 316L, IP H.264 version, 230Vac, Tag/Nacht Kamera 36x, Thermalkamera 25mm, 640x512, 25-30Hz, Wischer",25644]
[null,"NXPTZT2NAW0000A","NXPTZT Edelstahl- positioning unit 24Vac, mit Tag/Nacht Kamera 36x NTSC, Thermalkamera 35mm, 320x256, 7.5-8.3Hz, Wischer",17391]
[null,"NXPTZT2NAW0000AH","NXPTZT Edelstahl- positioning unit 24Vac, mit Tag/Nacht Kamera 36x NTSC, Thermalkamera 35mm, 320x256, 25Hz, Wischer",17728]
[null,"NXPTZT2NBW0000A","NXPTZT Edelstahl- positioning unit 24Vac, mit Tag/Nacht Kamera 36x NTSC, Thermalkamera 25mm, 320x256, 7.5-8.3Hz, Wischer",17391]
[null,"NXPTZT2NBW0000AH","NXPTZT Edelstahl- positioning unit 24Vac, mit Tag/Nacht Kamera 36x NTSC, Thermalkamera 25mm, 320x256, 25Hz, Wischer",17728]
[null,"NXPTZT2NDW0000A","NXPTZT in AISI 316L, 24Vac, Tag/Nacht Kamera 36x, NTSC, Thermalkamera 35mm, 640x512, 7.5-8.3Hz, Wischer",24769]
[null,"NXPTZT2NDW0000AH","NXPTZT in AISI 316L, 24Vac, Tag/Nacht Kamera 36x, NTSC, Thermalkamera 35mm, 640x512, 25-30Hz, Wischer",25105]
[null,"NXPTZT2NEW0000A","NXPTZT in AISI 316L, 24Vac, Tag/Nacht Kamera 36x, NTSC, Thermalkamera 25mm, 640x512, 7.5-8.3Hz, Wischer",24769]
[null,"NXPTZT2NEW0000AH","NXPTZT in AISI 316L, 24Vac, Tag/Nacht Kamera 36x, NTSC, Thermalkamera 25mm, 640x512, 25-30Hz, Wischer",25105]
[null,"NXPTZT2PAW0000A","NXPTZT Edelstahl- positioning unit 24Vac, mit Tag/Nacht Kamera 36x PAL, Thermalkamera 35mm, 320x256, 7.5-8.3Hz, Wischer",17391]
[null,"NXPTZT2PAW0000AH","NXPTZT Edelstahl- positioning unit 24Vac, mit Tag/Nacht Kamera 36x PAL, Thermalkamera 35mm, 320x256, 25Hz, Wischer",17728]
[null,"NXPTZT2PAW0Z00A","NXPTZT in AISI 316L, IP H.264 version, 24Vac, Tag/Nacht Kamera 36x,Thermalkamera 35mm, 320x256, 7.5-8.3Hz, Wischer",17930]
[null,"NXPTZT2PAW0Z00AH","NXPTZT in AISI 316L, IP H.264 version, 24Vac, mit Tag/Nacht Kamera 36x,Thermalkamera 35mm, 320x256, 25Hz, Wischer",18267]
[null,"NXPTZT2PBW0000A","NXPTZT Edelstahl- positioning unit 24Vac, mit Tag/Nacht Kamera 36x PAL, Thermalkamera 25mm, 320x256, 7.5-8.3Hz, Wischer",17391]
[null,"NXPTZT2PBW0000AH","NXPTZT Edelstahl- positioning unit 24Vac, mit Tag/Nacht Kamera 36x PAL, Thermalkamera 25mm, 320x256, 25Hz, Wischer",17728]
[null,"NXPTZT2PBW0Z00A","NXPTZT  in AISI 316L, IP H.264 version, 24Vac, Tag/Nacht Kamera 36x,Thermalkamera 25mm, 320x256, 7.5-8.3Hz, Wischer",17930]
[null,"NXPTZT2PBW0Z00AH","NXPTZT in AISI 316L, IP H.264 version, 24Vac, Tag/Nacht Kamera 36x,Thermalkamera 25mm, 320x256, 25Hz, Wischer",18267]
[null,"NXPTZT2PDW0000A","NXPTZT in AISI 316L, 24Vac, Tag/Nacht Kamera 36x, PAL, Thermalkamera 35mm, 640x512, 7.5-8.3Hz, Wischer",24769]
[null,"NXPTZT2PDW0000AH","NXPTZT in AISI 316L, 24Vac, Tag/Nacht Kamera 36x, PAL, Thermalkamera 35mm, 640x512, 25-30Hz, Wischer",25105]
[null,"NXPTZT2PDW0Z00A","NXPTZT in AISI 316L, IP H.264 version, 24Vac, Tag/Nacht Kamera 36x, Thermalkamera 35mm, 640x512, 7.5-8.3Hz, Wischer",25307]
[null,"NXPTZT2PDW0Z00AH","NXPTZT in AISI 316L, IP H.264 version, 24Vac, Tag/Nacht Kamera 36x, Thermalkamera 35mm, 640x512, 25-30Hz, Wischer",25644]
[null,"NXPTZT2PEW0000A","NXPTZT in AISI 316L, 24Vac, Tag/Nacht Kamera 36x, PAL, Thermalkamera 25mm, 640x512, 7.5-8.3Hz, Wischer",24769]
[null,"NXPTZT2PEW0000AH","NXPTZT in AISI 316L, 24Vac, Tag/Nacht Kamera 36x, PAL, Thermalkamera 25mm, 640x512, 25-30Hz, Wischer",25105]
[null,"NXPTZT2PEW0Z00A","NXPTZT in AISI 316L, IP H.264 version, 24Vac, Tag/Nacht Kamera 36x, Thermalkamera 25mm, 640x512, 7.5-8.3Hz, Wischer",25307]
[null,"NXPTZT2PEW0Z00AH","NXPTZT in AISI 316L, IP H.264 version, 24Vac, Tag/Nacht Kamera 36x, Thermalkamera 25mm, 640x512, 25-30Hz, Wischer",25644]
[null,"NXPTZT3NAW0000A","NXPTZT Edelstahl- positioning unit 120Vac, mit Tag/Nacht Kamera 36x, NTSC,  Thermalkamera 35mm, 320x256, 7.5-8.3Hz, Wischer",17391]
[null,"NXPTZT3NAW0000AH","NXPTZT Edelstahl- positioning unit 120Vac,  Tag/Nacht Kamera 36x, Thermalkamera 35mm, 320x256, 25Hz, Wischer",17728]
[null,"NXPTZT3NBW0000A","NXPTZT Edelstahl- positioning unit 120Vac, Tag/Nacht Kamera 36x, NTSC, Thermalkamera 25mm, 320x256, 7.5-8.3Hz, Wischer",17391]
[null,"NXPTZT3NBW0000AH","NXPTZT Edelstahl- positioning unit 120Vac, Tag/Nacht Kamera 36x, Thermalkamera 25mm, 320x256, 25Hz, Wischer",17728]
[null,"NXPTZT3NDW0000A","NXPTZT in AISI 316L, 120Vac, Tag/Nacht Kamera 36x, NTSC, Thermalkamera 35mm, 640x512, 7.5-8.3Hz, Wischer",24769]
[null,"NXPTZT3NDW0000AH","NXPTZT in AISI 316L, 120Vac, Tag/Nacht Kamera 36x,, Thermalkamera 35mm, 640x512, 25-30Hz, Wischer",25105]
[null,"NXPTZT3NEW0000A","NXPTZT in AISI 316L, 120Vac, Tag/Nacht Kamera 36x,, Thermalkamera 25mm, 640x512, 7.5-8.3Hz, Wischer",24769]
[null,"NXPTZT3NEW0000AH","NXPTZT in AISI 316L, 120Vac, Tag/Nacht Kamera 36x,, Thermalkamera 25mm, 640x512, 25-30Hz, Wischer",25105]
[null,"NXPTZT3PAW0Z00A","NXPTZT in AISI 316L, IP H.264 version, 120Vac, mit Tag/Nacht Kamera 36x,NTSC, Thermalkamera 35mm, 320x256, 7.5-8.3Hz, Wischer",17930]
[null,"NXPTZT3PAW0Z00AH","NXPTZT in AISI 316L, IP H.264 version, 120Vac,  Tag/Nacht Kamera 36x,NTSC, Thermalkamera 35mm, 320x256, 25Hz, Wischer",18267]
[null,"NXPTZT3PBW0Z00A","NXPTZT in AISI 316L, IP H.264 version, 120Vac, Tag/Nacht Kamera 36x,NTSC, Thermalkamera 25mm, 320x256, 7.5-8.3Hz, Wischer",17930]
[null,"NXPTZT3PBW0Z00AH","NXPTZT in AISI 316L, IP H.264 version, 120Vac, Tag/Nacht Kamera 36x,NTSC, Thermalkamera 25mm, 320x256, 25Hz, Wischer",18267]
[null,"NXPTZT3PDW0Z00A","NXPTZT in AISI 316L, IP H.264 version, 120Vac, Tag/Nacht Kamera 36x, Thermalkamera 35mm, 640x512, 7.5-8.3Hz, Wischer",25307]
[null,"NXPTZT3PDW0Z00AH","NXPTZT in AISI 316L, IP H.264 version, 120Vac, Tag/Nacht Kamera 36x, Thermalkamera 35mm, 640x512, 25-30Hz, Wischer",25644]
[null,"NXPTZT3PEW0Z00A","NXPTZT in AISI 316L, IP H.264 version, 120Vac, Tag/Nacht Kamera 36x, Thermalkamera 25mm, 640x512, 7.5-8.3Hz, Wischer",25307]
[null,"NXPTZT3PEW0Z00AH","NXPTZT in AISI 316L, IP H.264 version, 120Vac, Tag/Nacht Kamera 36x, Thermalkamera 25mm, 640x512, 25-30Hz, Wischer",25644]
[null,"NXPTZTW","Halter für ceiling or parapet mounting",199]
[null,"NXPTZWB","Wandhalterung",462]
[null,"NXW0K1000","Flüssigkeitgekühltes Edelstahl-Gehäuse mit ONXAB2 air barrier, glass not included",1479]
[null,"NXW0K1025","Flüssigkeitgekühltes Edelstahl-Gehäuse mit ONXAB2 air barrier mit IR-proof glass",2079]
[null,"NXWBL","Edelstahl- Wandhalterung for NXL Gehäuse",520]
[null,"NXWBPTH1","Wall mount for heavy duty Edelstahl- P&T",462]
[null,"NXWBS1","Wandhalterung for Edelstahl-Gehäuses",266]
[null,"OBJA","Ball joint for Gehäuse",15]
[null,"ODBH18H110","Kamera adapter mit fan-assisted Heizung IN 100-240Vac und Kameranetzteil OUT 100-240Vac or 12Vdc, 3A",197]
[null,"ODBH18H114","Kamera adapter for SONY SNC-RX-530, SNC-RX-550, SNC-RX-570, SNC-RH124P, SNC-RS44P, SNC-RS46P mit fan-assisted Heizung IN 100-240Vac, Kameranetzteil OUT 12Vdc, 3A",197]
[null,"ODBH18H211","Kamera adapter mit fan-assisted Heizung IN 24Vac",197]
[null,"OHEBVF1","Lüfter kit mit thermostat air filter IN 12Vdc, not compatible mit WBOVA2 und WBOV3A2",33]
[null,"OHEBVF2","Lüfter kit mit thermostat air filter IN 24Vac, not compatible mit WBOVA2 und WBOV3A2",33]
[null,"OHEBVF3","Lüfter kit mit thermostat air filter IN 230Vac, not compatible mit WBOVA2 und WBOV3A2",61]
[null,"OHEGBB","Weatherproof junction box, IP55",52]
[null,"OHEGBPS1B","Weitbereichs-Kameranetzteil für Kamera IN 100-240Vac - OUT 12Vdc in weatherproof box",86]
[null,"OHEGBPS2B","Kameranetzteil IN 230Vac - OUT 24Vac in weatherproof box",86]
[null,"OHEH01B","Heizung IN 12Vdc/24Vac",20]
[null,"OHEH02B","Heizung IN 120/230Vac",20]
[null,"OHEH05B","Heizung IN 12Vdc/24Vac",22]
[null,"OHEH06B","Heizung IN 120/230Vac",22]
[null,"OHEH24B","Heizung IN 120/230Vac",21]
[null,"OHEH25B","Heizung IN 12Vdc/24Vac",21]
[null,"OHEH26","Heizung IN 120/230Vac",17]
[null,"OHEH27","Heizung IN 12Vdc/24Vac",17]
[null,"OHEPOWINJ","Hi-PoE Power Injector, 1 channel",104]
[null,"OHEPS01B","Weitbereichs-Kameranetzteil für Kamera IN 100-240Vac - OUT 12Vdc",49]
[null,"OHEPS02B","Kameranetzteil IN 230Vac - OUT 24Vac",43]
[null,"OHEPS05","Kameranetzteil IN 230Vac - OUT 12Vdc",50]
[null,"OHEPS06","Kameranetzteil IN 230Vac - OUT 24Vac",50]
[null,"OHEPS10B","Weitbereichs-Kameranetzteil für Kamera IN 100-240Vac - OUT 12Vdc",36]
[null,"OHEPS11B","Kameranetzteil IN 230Vac - OUT 24Vac",36]
[null,"OHEPS19B","Weitbereichs-Kameranetzteil für Kamera IN 100-240Vac - OUT 12Vdc",34]
[null,"OHEPS20","Kameranetzteil IN 230Vac - OUT 24Vac",27]
[null,"OHEPS22","Weitbereichs-Kameranetzteil für Kamera IN 100-240Vac - OUT 12Vdc, 1A",45]
[null,"OHEPS23","Kameranetzteil IN 230Vac - OUT 24Vac, 400mA",45]
[null,"OHEPS24","Kameranetzteil IN 230Vac - OUT 12Vdc, 400mA",44]
[null,"OHEPS25","Kameranetzteil IN 230Vac - OUT 24Vac, 400mA",38]
[null,"OHOTPS1","Weitbereichs-Kameranetzteil für Kamera IN 100-240Vac - OUT 12Vdc, 1A",34]
[null,"OHOTPS2","Kameranetzteil IN 230Vac - OUT 24Vac, 400mA",27]
[null,"OHOTS","Sonnendach",9]
[null,"OHOVPOEIPM","Kit retrofit for IPM technology on HOV Gehäuses",173]
[null,"OHOVPS1B","Weitbereichs-Kameranetzteil für Kamera IN 100-240Vac - OUT 12Vdc",34]
[null,"OHOVPS2B","Kameranetzteil IN 230Vac - OUT 24Vac",27]
[null,"OHOVTA1","Tamper switch on board mit tamper proof screws und key",42]
[null,"OHOVV1","Heizung fan assistant, continuous duty IN 12Vdc",26]
[null,"OHOVV2","Heizung fan assistant, continuous duty, IN 24Vac",26]
[null,"OHOVV3","Heizung fan assistant, continuous duty, IN 100/240Vac",51]
[null,"OHPVCF3","Lüfter kit mit thermostat und air filter IN 110/240Vac",57]
[null,"OHPVPOEIPM","Kit retrofit for IPM technology on VERSO Gehäuses",173]
[null,"OHPVTA1","Tamper switch mit tamper proof screws und key",29]
[null,"OHPVV1","Heizung fan assistant, continuous duty IN 12Vdc",26]
[null,"OHPVV2","Heizung fan assistant, continuous duty IN 24Vac",26]
[null,"OHPVV3","Heizung fan assistant, continuous duty IN 100-240Vac",51]
[null,"ONXAB1025B","Air barrier mit IR-proof glass",813]
[null,"ONXAB2","Air barrier mit tempered glass included",367]
[null,"ONXLH1","Heizung IN 120/230Vac",22]
[null,"ONXLH2","Heizung IN 12Vdc/24Vac",22]
[null,"ONXPS1B","Weitbereichs-Kameranetzteil für Kamera IN 100-240Vac - OUT 12Vdc",41]
[null,"ONXPS2B","Kameranetzteil IN 230Vac - OUT 24Vac",35]
[null,"ONXWQG","Quartz Glass",335]
[null,"ONXWTG","Tempered glass",25]
[null,"OSUPPIR","Halter für mounting 1 GEKO IRH Strahler under an Gehäuse",22]
[null,"OUCHWR","Front kit mit heated glass for ULISSE COMPACT",341]
[null,"OVARK","Kit for ALBERT units rack-mounting",91]
[null,"OWBIP2","Kit special gaskets for IP66 protection for WBOVA2 und WCM4A2 brackets",6]
[null,"OWBIP3","Kit special gaskets for IP66 protection for WBOVA2 und WCM4A2 brackets",6]
[null,"PTAC","Wandhalterung for PTH300 P&T",29]
[null,"PTCC1","Pole mount adaptor Ø 80 - 150mm (3.14 - 5.9in)",107]
[null,"PTH310","Pan & Tilt 230Vac, 50/60Hz, max load 12kg (26lb)",751]
[null,"PTH310P","Pan & Tilt mit preset 230Vac, 50/60Hz, max load 12kg (26lb)",919]
[null,"PTH311","Pan & Tilt 24Vac, 50/60Hz, max load 12kg (26lb)",734]
[null,"PTH311P","Pan & Tilt mit preset 24Vac, 50/60Hz, max load 12kg (26lb)",907]
[null,"PTH355P","Variable speed Pan & Tilt 24Vdc, mit preset, max load 12kg (26lb)",1086]
[null,"SM164B","Video matrix, 16 inputs und 4 outputs",728]
[null,"SM328B","Video matrix, 32 inputs, 8 outputs",2310]
[null,"SM82A","Video matrix, 8 inputs und 2 outputs",451]
[null,"TWM2","Mini twisted pair video transmitter, IN 12Vdc/24Vac",113]
[null,"TWRB2","Twisted pair video receiver in IP56 box, IN 12Vdc/24Vac",185]
[null,"TWRB2A","Twisted pair video receiver in IP56 box, 230Vac",185]
[null,"TWRC1","Rack box 19” for max 14 TWRR2 Europe cards und receivers Netzteil",453]
[null,"TWRR2","Twisted pair video receiver on Europe card for rack version, IN 12Vdc/24Vac",185]
[null,"TWT2","Twisted pair video transmitter in IP56 box, IN 12Vdc/24Vac",113]
[null,"TWT2A","Twisted pair video transmitter in IP56 box, 230Vac",126]
[null,"UC1BVRA000A","ULISSE COMPACT 230Vac, Kamera 10x PAL, IR LED Strahler 10°, I/O alarms",3282]
[null,"UC1PVQA000A","ULISSE COMPACT 230Vac, Kamera 36x PAL, IR LED Strahler 30°, I/O alarms",3675]
[null,"UC1PVQAZ00A","ULISSE COMPACT IP-based (H.264), 230Vac, Kamera 36x, IR LED Strahler 30°",4214]
[null,"UC1PVRA000A","ULISSE COMPACT 230Vac, Kamera 36x PAL, IR LED Strahler 10°, I/O alarms",3675]
[null,"UC1PVRAZ00A","ULISSE COMPACT IP-based (H.264), 230Vac, Kamera 36x, IR LED Strahler 10°",4214]
[null,"UC1PVSA000A","ULISSE COMPACT 230Vac, Kamera 36x PAL, I/O alarms",3136]
[null,"UC1PVSAZ00A","ULISSE COMPACT IP-based (H.264), 230Vac, Kamera 36x",3675]
[null,"UC1PVTA000A","ULISSE COMPACT 230Vac, Kamera 36x PAL, Wischer, IR LED Strahler 10°, I/O alarms",3849]
[null,"UC1PVTAZ00A","ULISSE COMPACT IP-based (H.264), 230Vac, Kamera 36x, Wischer, IR LED Strahler 10°",4388]
[null,"UC1PVUA000A","ULISSE COMPACT 230Vac, Kamera 36x PAL, Wischer, IR LED Strahler 30°, I/O alarms",3849]
[null,"UC1PVUAZ00A","ULISSE COMPACT IP-based (H.264), 230Vac, Kamera 36x, Wischer, IR LED Strahler 30°",4388]
[null,"UC1PVWA000A","ULISSE COMPACT 230Vac, Kamera 36x PAL, Wischer, I/O alarms",3310]
[null,"UC1PVWAZ00A","ULISSE COMPACT IP-based (H.264), 230Vac, Kamera 36x, Wischer",3849]
[null,"UC1PVZA000A","ULISSE COMPACT 230Vac, Tag/Nacht Kamera 36x PAL, Wischer, Weißlicht LED Strahler 30°, I/O alarm card",3883]
[null,"UC1PVZAZ00A","ULISSE COMPACT IP-based (H.264), 230Vac, Kamera 36x, Wischer, Weißlicht LED Strahler 30°",4421]
[null,"UC1QVQA000A","ULISSE COMPACT 230Vac, Kamera 28x PAL, IR LED Strahler 30°, I/O alarms",3535]
[null,"UC1QVQAZ00A","ULISSE COMPACT IP-based (H.264), 230Vac, Kamera 28x, IR LED Strahler 30°",4073]
[null,"UC1QVRA000A","ULISSE COMPACT 230Vac, Kamera 28x PAL, IR LED Strahler 10°, I/O alarms",3535]
[null,"UC1QVRAZ00A","ULISSE COMPACT IP-based (H.264), 230Vac, Kamera 28x, IR LED Strahler 10°",4073]
[null,"UC1QVTA000A","ULISSE COMPACT 230Vac, Kamera 28x PAL, Wischer, IR LED Strahler 10°, I/O alarms",3709]
[null,"UC1QVTAZ00A","ULISSE COMPACT IP-based (H.264), 230Vac, Kamera 28x, Wischer, IR LED Strahler 10°",4247]
[null,"UC1QVUA000A","ULISSE COMPACT 230Vac, Kamera 28x PAL, Wischer, IR LED Strahler 30°, I/O alarms",3709]
[null,"UC1QVUAZ00A","ULISSE COMPACT IP-based (H.264), 230Vac, Kamera 28x, Wischer, IR LED Strahler 30°",4247]
[null,"UC2MVQA000A","ULISSE COMPACT 24Vac, Kamera 28x NTSC, IR LED Strahler 30°, I/O alarms",3535]
[null,"UC2MVRA000A","ULISSE COMPACT 24Vac, Kamera 28x NTSC, IR LED Strahler 10°, I/O alarms",3535]
[null,"UC2MVSA000A","ULISSE COMPACT 24Vac, Kamera 28x NTSC, I/O alarms",2996]
[null,"UC2MVTA000A","ULISSE COMPACT 24Vac, Kamera 28x NTSC, Wischer, IR LED Strahler 10°, I/O alarms",3709]
[null,"UC2MVUA000A","ULISSE COMPACT 24Vac, Kamera 28x NTSC, Wischer, IR LED Strahler 30°, I/O alarms",3709]
[null,"UC2MVWA000A","ULISSE COMPACT 24Vac, Kamera 28x NTSC, Wischer, I/O alarms",3170]
[null,"UC2NVQA000A","ULISSE COMPACT 24Vac, Kamera 36x NTSC, IR LED Strahler 30°, I/O alarms",3675]
[null,"UC2NVRA000A","ULISSE COMPACT 24Vac, Kamera 36x NTSC, IR LED Strahler 10°, I/O alarms",3675]
[null,"UC2NVSA000A","ULISSE COMPACT 24Vac, Kamera 36x NTSC, I/O alarms",3136]
[null,"UC2NVTA000A","ULISSE COMPACT 24Vac, Kamera 36x NTSC, Wischer, IR LED Strahler 10°, I/O alarms",3849]
[null,"UC2NVUA000A","ULISSE COMPACT 24Vac, Kamera 36x NTSC, Wischer, IR LED Strahler 30°, I/O alarms",3849]
[null,"UC2NVWA000A","ULISSE COMPACT 24Vac, Kamera 36x NTSC, Wischer, I/O alarms",3310]
[null,"UC2NVZA000A","ULISSE COMPACT 24Vac mit Wischer, Tag/Nacht Kamera 36x NTSC, Weißlicht LED Strahler 30°, I/O alarm card",3883]
[null,"UC2PVQA000A","ULISSE COMPACT 24Vac, Kamera 36x PAL, IR LED Strahler 30°, I/O alarms",3675]
[null,"UC2PVQAZ00A","ULISSE COMPACT IP-based (H.264), 24Vac, Kamera 36x, IR LED Strahler 30°",4214]
[null,"UC2PVRA000A","ULISSE COMPACT 24Vac, Kamera 36x PAL, IR LED Strahler 10°, I/O alarms",3675]
[null,"UC2PVRAZ00A","ULISSE COMPACT IP-based (H.264), 24Vac, Kamera 36x, IR LED Strahler 10°",4214]
[null,"UC2PVSA000A","ULISSE COMPACT 24Vac, Kamera 36x PAL, I/O alarms",3136]
[null,"UC2PVSAZ00A","ULISSE COMPACT IP-based (H.264), 24Vac, Kamera 36x",3675]
[null,"UC2PVTA000A","ULISSE COMPACT 24Vac, Kamera 36x PAL, Wischer, IR LED Strahler 10°, I/O alarms",3849]
[null,"UC2PVTAZ00A","ULISSE COMPACT IP-based (H.264), 24Vac, Kamera 36x, Wischer, IR LED Strahler 10°",4388]
[null,"UC2PVUA000A","ULISSE COMPACT 24Vac, Kamera 36x PAL, Wischer, IR LED Strahler 30°, I/O alarms",3849]
[null,"UC2PVUAZ00A","ULISSE COMPACT IP-based (H.264), 24Vac, Kamera 36x, Wischer, IR LED Strahler 30°",4388]
[null,"UC2PVWA000A","ULISSE COMPACT 24Vac, Kamera 36x PAL, Wischer, I/O alarms",3310]
[null,"UC2PVWAZ00A","ULISSE COMPACT IP-based (H.264), 24Vac, Kamera 36x, Wischer",3849]
[null,"UC2PVZA000A","ULISSE COMPACT 24Vac, Tag/Nacht Kamera 36x PAL, Wischer, Weißlicht LED Strahler 30°, I/O alarms",3883]
[null,"UC2PVZAZ00A","ULISSE COMPACT IP-based (H.264), 24Vac, Kamera 36x, Wischer, Weißlicht LED Strahler 30°",4421]
[null,"UC2QVQA000A","ULISSE COMPACT 24Vac, Kamera 28x PAL, IR LED Strahler 30°, I/O alarms",3535]
[null,"UC2QVQAZ00A","ULISSE COMPACT IP-based (H.264), 24Vac, Kamera 28x, IR LED Strahler 30°",4073]
[null,"UC2QVRA000A","ULISSE COMPACT 24Vac, Kamera 28x PAL, IR LED Strahler 10°, I/O alarms",3535]
[null,"UC2QVRAZ00A","ULISSE COMPACT IP-based (H.264), 24Vac, Kamera 28x, IR LED Strahler 10°",4073]
[null,"UC2QVSA000A","ULISSE COMPACT 24Vac, Kamera 28x PAL, I/O alarms",2996]
[null,"UC2QVSAZ00A","ULISSE COMPACT IP-based (H.264), 24Vac, Kamera 28x",3535]
[null,"UC2QVTA000A","ULISSE COMPACT 24Vac, Kamera 28x PAL, Wischer, IR LED Strahler 10°, I/O alarms",3709]
[null,"UC2QVTAZ00A","ULISSE COMPACT IP-based (H.264), 24Vac, Kamera 28x, Wischer, IR LED Strahler 10°",4247]
[null,"UC2QVUA000A","ULISSE COMPACT 24Vac, Kamera 28x PAL, Wischer, IR LED Strahler 30°, I/O alarms",3709]
[null,"UC2QVUAZ00A","ULISSE COMPACT IP-based (H.264), 24Vac, Kamera 28x, Wischer, IR LED Strahler 30°",4247]
[null,"UC2QVWA000A","ULISSE COMPACT 24Vac, Kamera 28x PAL, Wischer, I/O alarms",3170]
[null,"UC2QVWAZ00A","ULISSE COMPACT IP-based (H.264), 24Vac, Kamera 28x, Wischer",3709]
[null,"UC3MVQA000A","ULISSE COMPACT 120Vac, Kamera 28x NTSC, IR LED Strahler 30°, I/O alarms",3535]
[null,"UC3MVRA000A","ULISSE COMPACT 120Vac, Kamera 28x NTSC, IR LED Strahler 10°, I/O alarms",3535]
[null,"UC3MVSA000A","ULISSE COMPACT 120Vac, Kamera 28x NTSC, I/O alarms",2996]
[null,"UC3MVTA000A","ULISSE COMPACT 120Vac, Kamera 28x NTSC, Wischer, IR LED Strahler 10°, I/O alarms",3709]
[null,"UC3MVUA000A","ULISSE COMPACT 120Vac, Kamera 28x NTSC, Wischer, IR LED Strahler 30°, I/O alarms",3709]
[null,"UC3MVWA000A","ULISSE COMPACT 120Vac, Kamera 28x NTSC, Wischer, I/O alarms",3170]
[null,"UC3NVQA000A","ULISSE COMPACT 120Vac, Kamera 36x NTSC, IR LED Strahler 30°, I/O alarms",3675]
[null,"UC3NVRA000A","ULISSE COMPACT 120Vac, Kamera 36x NTSC, IR LED Strahler 10°, I/O alarms",3675]
[null,"UC3NVSA000A","ULISSE COMPACT 120Vac, Kamera 36x NTSC, I/O alarms",3136]
[null,"UC3NVTA000A","ULISSE COMPACT 120Vac, Kamera 36x NTSC, Wischer, IR LED Strahler 10°, I/O alarms",3849]
[null,"UC3NVUA000A","ULISSE COMPACT 120Vac, Kamera 36x NTSC, Wischer, IR LED Strahler 30°, I/O alarms",3849]
[null,"UC3NVWA000A","ULISSE COMPACT 120Vac, Kamera 36x NTSC, Wischer, I/O alarms",3310]
[null,"UC3NVZA000A","ULISSE COMPACT 120Vac, Tag/Nacht Kamera 36x NTSC, Wischer, Weißlicht LED Strahler 30°, I/O alarm card",3883]
[null,"UC3PVQAZ00A","ULISSE COMPACT IP-based (H.264), IP 120Vac, Kamera 36x, IR LED Strahler 30°",4214]
[null,"UC3PVRAZ00A","ULISSE COMPACT IP-based (H.264), 120Vac, Kamera 36x, IR LED Strahler 10°",4214]
[null,"UC3PVSAZ00A","ULISSE COMPACT IP-based (H.264), 120Vac, Kamera 36x",3675]
[null,"UC3PVTAZ00A","ULISSE COMPACT IP-based (H.264), 120Vac, Kamera 36x, Wischer, IR LED Strahler 10°",4388]
[null,"UC3PVUAZ00A","ULISSE COMPACT IP-based (H.264), 120Vac, Kamera 36x, Wischer, IR LED Strahler 30°",4388]
[null,"UC3PVWAZ00A","ULISSE COMPACT IP-based (H.264), 120Vac, Kamera 36x, Wischer",3849]
[null,"UC3PVZAZ00A","ULISSE COMPACT IP-based (H.264), 120Vac, Kamera 36x, Wischer, Weißlicht LED Strahler 30°",4421]
[null,"UC3QVQAZ00A","ULISSE COMPACT IP version, H.264, 120Vac, Kamera 28x, IR LED Strahler 30°",4073]
[null,"UC3QVRAZ00A","ULISSE COMPACT IP-based (H.264), 120Vac, Kamera 28x, IR LED Strahler 10°",4073]
[null,"UC3QVSAZ00A","ULISSE COMPACT IP-based (H.264), 120Vac, Kamera 28x",3535]
[null,"UC3QVTAZ00A","ULISSE COMPACT IP-based (H.264), 120Vac, Kamera 28x, Wischer, IR LED Strahler 10°",4247]
[null,"UC3QVUAZ00A","ULISSE COMPACT IP-based (H.264), 120Vac, Kamera 28x, Wischer, IR LED Strahler 30°",4247]
[null,"UC3QVWAZ00A","ULISSE COMPACT IP-based (H.264), 120Vac, Kamera 28x, Wischer",3709]
[null,"UCCMA","Deckenhalterung mount for upside down working of ULISSE COMPACT",335]
[null,"UCHD1FNAZ00A","ULISSE COMPACT HD 230Vac, Tag/Nacht Kamera FullHD 30x, H.264/AVC, IR LED Strahler 10° 940nm, Wischer",5364]
[null,"UCHD1FTAZ00A","ULISSE COMPACT HD 230Vac, Tag/Nacht Kamera FullHD 30x, H.264/AVC, IR LED Strahler 10° 850nm, Wischer",5364]
[null,"UCHD1FUAZ00A","ULISSE COMPACT HD 230Vac, Tag/Nacht Kamera FullHD 30x, H.264/AVC, IR LED Strahler 30° 850nm, Wischer",5364]
[null,"UCHD1FWAZ00A","ULISSE COMPACT HD 230Vac, Tag/Nacht Kamera FullHD 30x, H.264/AVC, Wischer",5027]
[null,"UCHD1FZAZ00A","ULISSE COMPACT HD 230Vac, Tag/Nacht Kamera FullHD 30x, H.264/AVC, LED Strahler 30° Weißlicht, Wischer",5364]
[null,"UCHD2FNAZ00A","ULISSE COMPACT HD 24Vac, Tag/Nacht Kamera FullHD 30x, H.264/AVC, IR LED Strahler 10° 940nm, Wischer",5364]
[null,"UCHD2FTAZ00A","ULISSE COMPACT HD 24Vac, Tag/Nacht Kamera FullHD 30x, H.264/AVC, IR LED Strahler 10° 850nm, Wischer",5364]
[null,"UCHD2FUAZ00A","ULISSE COMPACT HD 24Vac, Tag/Nacht Kamera FullHD 30x, H.264/AVC, IR LED Strahler 30° 850nm, Wischer",5364]
[null,"UCHD2FWAZ00A","ULISSE COMPACT HD 24Vac, Tag/Nacht Kamera FullHD 30x, H.264/AVC, Wischer",5027]
[null,"UCHD2FZAZ00A","ULISSE COMPACT HD 24Vac, Tag/Nacht Kamera FullHD 30x, H.264/AVC, LED Strahler 30° Weißlicht, Wischer",5364]
[null,"UCHD3FNAZ00A","ULISSE COMPACT HD 120Vac, Tag/Nacht Kamera FullHD 30x, H.264/AVC, IR LED Strahler 10° 940nm, Wischer",5364]
[null,"UCHD3FTAZ00A","ULISSE COMPACT HD 120Vac, Tag/Nacht Kamera FullHD 30x, H.264/AVC, IR LED Strahler 10° 850nm, Wischer",5364]
[null,"UCHD3FUAZ00A","ULISSE COMPACT HD 120Vac, Tag/Nacht Kamera FullHD 30x, H.264/AVC, IR LED Strahler 30° 850nm, Wischer",5364]
[null,"UCHD3FWAZ00A","ULISSE COMPACT HD 120Vac, Tag/Nacht Kamera FullHD 30x, H.264/AVC, Wischer",5027]
[null,"UCHD3FZAZ00A","ULISSE COMPACT HD 120Vac, Tag/Nacht Kamera FullHD 30x, H.264/AVC, LED Strahler 30° Weißlicht, Wischer",5364]
[null,"UCT1PAWA000A","ULISSE COMPACT THERMAL 230Vac, Tag/Nacht Kamera 36x PAL, Thermalkamera 35mm, 320x256, 7.5-8.3Hz, Wischer",12118]
[null,"UCT1PAWA000AH","ULISSE COMPACT THERMAL 230Vac, Tag/Nacht Kamera 36x PAL, Thermalkamera 35mm, 320x256, 25-30Hz, Wischer",12298]
[null,"UCT1PBWA000A","ULISSE COMPACT THERMAL 230Vac, Tag/Nacht Kamera 36x PAL, Thermalkamera 25mm, 320x256, 7.5-8.3Hz, Wischer",12118]
[null,"UCT1PBWA000AH","ULISSE COMPACT THERMAL 230Vac, Tag/Nacht Kamera 36x PAL, Thermalkamera 25mm, 320x256, 25-30Hz, Wischer",12298]
[null,"UCT1PDWA000A","ULISSE COMPACT THERMAL 230Vac, Tag/Nacht Kamera 36x PAL, Thermalkamera 35mm, 640x512, 7.5-8.3Hz, Wischer",19647]
[null,"UCT1PDWA000AH","ULISSE COMPACT THERMAL 230Vac, Tag/Nacht Kamera 36x PAL, Thermalkamera 35mm, 640x512, 25-30Hz, Wischer",20006]
[null,"UCT1PEWA000A","ULISSE COMPACT THERMAL 230Vac, Tag/Nacht Kamera 36x PAL, Thermalkamera 25mm, 640x512, 7.5-8.3Hz, Wischer",19647]
[null,"UCT1PEWA000AH","ULISSE COMPACT THERMAL 230Vac, Tag/Nacht Kamera 36x PAL, Thermalkamera 25mm, 640x512, 25-30Hz, Wischer",20006]
[null,"UCT1QAWA000A","ULISSE COMPACT THERMAL 230Vac, Tag/Nacht Kamera 28x PAL, Thermalkamera 35mm, 320x256, 7.5-8.3Hz, Wischer",11978]
[null,"UCT1QAWA000AH","ULISSE COMPACT THERMAL 230Vac, Tag/Nacht Kamera 28x PAL, Thermalkamera 35mm, 320x256, 25-30Hz, Wischer",12157]
[null,"UCT1QBWA000A","ULISSE COMPACT THERMAL 230Vac, Tag/Nacht Kamera 28x PAL, Thermalkamera 25mm, 320x256, 7.5-8.3Hz, Wischer",11978]
[null,"UCT1QBWA000AH","ULISSE COMPACT THERMAL 230Vac, Tag/Nacht Kamera 28x PAL, Thermalkamera 25mm, 320x256, 25-30Hz, Wischer",12157]
[null,"UCT1QDWA000A","ULISSE COMPACT THERMAL 230Vac, Tag/Nacht Kamera 28x PAL, Thermalkamera 35mm, 640x512, 7.5-8.3Hz, Wischer",19506]
[null,"UCT1QDWA000AH","ULISSE COMPACT THERMAL 230Vac, Tag/Nacht Kamera 28x PAL, Thermalkamera 35mm, 640x512, 25-30Hz, Wischer",19866]
[null,"UCT1QEWA000A","ULISSE COMPACT THERMAL 230Vac, Tag/Nacht Kamera 28x PAL, Thermalkamera 25mm, 640x512, 7.5-8.3Hz, Wischer",19506]
[null,"UCT1QEWA000AH","ULISSE COMPACT THERMAL 230Vac, Tag/Nacht Kamera 28x PAL, Thermalkamera 25mm, 640x512, 25-30Hz, Wischer",19866]
[null,"UCT2MAWA000A","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 28x NTSC, Thermalkamera 35mm, 320x256, 7.5-8.3Hz, Wischer",11978]
[null,"UCT2MAWA000AH","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 28x NTSC, Thermalkamera 35mm, 320x256, 25-30Hz, Wischer",12157]
[null,"UCT2MBWA000A","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 28x NTSC, Thermalkamera 25mm, 320x256, 7.5-8.3Hz, Wischer",11978]
[null,"UCT2MBWA000AH","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 28x NTSC, Thermalkamera 25mm, 320x256, 25-30Hz, Wischer",12157]
[null,"UCT2MDWA000A","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 28x NTSC, Thermalkamera 35mm, 640x512, 7.5-8.3Hz, Wischer",19506]
[null,"UCT2MDWA000AH","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 28x NTSC, Thermalkamera 35mm, 640x512, 25-30Hz, Wischer",19866]
[null,"UCT2MEWA000A","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 28x NTSC, Thermalkamera 25mm, 640x512, 7.5-8.3Hz, Wischer",19506]
[null,"UCT2MEWA000AH","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 28x NTSC, Thermalkamera 25mm, 640x512, 25-30Hz, Wischer",19866]
[null,"UCT2NAWA000A","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 36x NTSC, Thermalkamera 35mm, 320x256, 7.5-8.3Hz, Wischer",12118]
[null,"UCT2NAWA000AH","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 36x NTSC, Thermalkamera 35mm, 320x256, 25-30Hz, Wischer",12298]
[null,"UCT2NBWA000A","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 36x NTSC, Thermalkamera 25mm, 320x256, 7.5-8.3Hz, Wischer",12118]
[null,"UCT2NBWA000AH","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 36x NTSC, Thermalkamera 25mm, 320x256, 25-30Hz, Wischer",12298]
[null,"UCT2NDWA000A","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 36x NTSC, Thermalkamera 35mm, 640x512, 7.5-8.3Hz, Wischer",19647]
[null,"UCT2NDWA000AH","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 36x NTSC, Thermalkamera 35mm, 640x512, 25-30Hz, Wischer",20006]
[null,"UCT2NEWA000A","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 36x NTSC, Thermalkamera 25mm, 640x512, 7.5-8.3Hz, Wischer",19647]
[null,"UCT2NEWA000AH","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 36x NTSC, Thermalkamera 25mm, 640x512, 25-30Hz, Wischer",20006]
[null,"UCT2PAWA000A","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 36x PAL, Thermalkamera 35mm, 320x256, 7.5-8.3Hz, Wischer",12118]
[null,"UCT2PAWA000AH","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 36x PAL, Thermalkamera 35mm, 320x256, 25-30Hz, Wischer",12298]
[null,"UCT2PBWA000A","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 36x PAL, Thermalkamera 25mm, 320x256, 7.5-8.3Hz, Wischer",12118]
[null,"UCT2PBWA000AH","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 36x PAL, Thermalkamera 25mm, 320x256, 25-30Hz, Wischer",12298]
[null,"UCT2PDWA000A","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 36x PAL, Thermalkamera 35mm, 640x512, 7.5-8.3Hz, Wischer",19647]
[null,"UCT2PDWA000AH","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 36x PAL, Thermalkamera 35mm, 640x512, 25-30Hz, Wischer",20006]
[null,"UCT2PEWA000A","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 36x PAL, Thermalkamera 25mm, 640x512, 7.5-8.3Hz, Wischer",19647]
[null,"UCT2PEWA000AH","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 36x PAL, Thermalkamera 25mm, 640x512, 25-30Hz, Wischer",20006]
[null,"UCT2QAWA000A","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 28x PAL, Thermalkamera 35mm, 320x256, 7.5-8.3Hz, Wischer",11978]
[null,"UCT2QAWA000AH","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 28x PAL, Thermalkamera 35mm, 320x256, 25-30Hz, Wischer",12157]
[null,"UCT2QBWA000A","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 28x PAL, Thermalkamera 25mm, 320x256, 7.5-8.3Hz, Wischer",11978]
[null,"UCT2QBWA000AH","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 28x PAL, Thermalkamera 25mm, 320x256, 25-30Hz, Wischer",12157]
[null,"UCT2QDWA000A","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 28x PAL, Thermalkamera 35mm, 640x512, 7.5-8.3Hz, Wischer",19506]
[null,"UCT2QDWA000AH","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 28x PAL, Thermalkamera 35mm, 640x512, 25-30Hz, Wischer",19866]
[null,"UCT2QEWA000A","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 28x PAL, Thermalkamera 25mm, 640x512, 7.5-8.3Hz, Wischer",19506]
[null,"UCT2QEWA000AH","ULISSE COMPACT THERMAL 24Vac, Tag/Nacht Kamera 28x PAL, Thermalkamera 25mm, 640x512, 25-30Hz, Wischer",19866]
[null,"UCT3MAWA000A","ULISSE COMPACT THERMAL 120Vac, Tag/Nacht Kamera 28x NTSC, Thermalkamera 35mm, 320x256, 7.5-8.3Hz, Wischer",11978]
[null,"UCT3MAWA000AH","ULISSE COMPACT THERMAL 120Vac, Tag/Nacht Kamera 28x NTSC, Thermalkamera 35mm, 320x256, 25-30Hz, Wischer",12157]
[null,"UCT3MBWA000A","ULISSE COMPACT THERMAL 120Vac, Tag/Nacht Kamera 28x NTSC, Thermalkamera 25mm, 320x256, 7.5-8.3Hz, Wischer",11978]
[null,"UCT3MBWA000AH","ULISSE COMPACT THERMAL 120Vac, Tag/Nacht Kamera 28x NTSC, Thermalkamera 25mm, 320x256, 25-30Hz, Wischer",12157]
[null,"UCT3MDWA000A","ULISSE COMPACT THERMAL 120Vac, Tag/Nacht Kamera 28x NTSC, Thermalkamera 35mm, 640x512, 7.5-8.3Hz, Wischer",19506]
[null,"UCT3MDWA000AH","ULISSE COMPACT THERMAL 120Vac, Tag/Nacht Kamera 28x NTSC, Thermalkamera 35mm, 640x512, 25-30Hz, Wischer",19866]
[null,"UCT3MEWA000A","ULISSE COMPACT THERMAL 120Vac, Tag/Nacht Kamera 28x NTSC, Thermalkamera 25mm, 640x512, 7.5-8.3Hz, Wischer",19506]
[null,"UCT3MEWA000AH","ULISSE COMPACT THERMAL 120Vac, Tag/Nacht Kamera 28x NTSC, Thermalkamera 25mm, 640x512, 25-30Hz, Wischer",19866]
[null,"UCT3NAWA000A","ULISSE COMPACT THERMAL 120Vac, Tag/Nacht Kamera 36x NTSC, Thermalkamera 35mm, 320x256, 7.5-8.3Hz, Wischer",12118]
[null,"UCT3NAWA000AH","ULISSE COMPACT THERMAL 120Vac, Tag/Nacht Kamera 36x NTSC, Thermalkamera 35mm, 320x256, 25-30Hz, Wischer",12298]
[null,"UCT3NBWA000A","ULISSE COMPACT THERMAL 120Vac, Tag/Nacht Kamera 36x NTSC, Thermalkamera 25mm, 320x256, 7.5-8.3Hz, Wischer",12118]
[null,"UCT3NBWA000AH","ULISSE COMPACT THERMAL 120Vac, Tag/Nacht Kamera 36x NTSC, Thermalkamera 25mm, 320x256, 25-30Hz, Wischer",12298]
[null,"UCT3NDWA000A","ULISSE COMPACT THERMAL 120Vac, Tag/Nacht Kamera 36x NTSC, Thermalkamera 35mm, 640x512, 7.5-8.3Hz, Wischer",19647]
[null,"UCT3NDWA000AH","ULISSE COMPACT THERMAL 120Vac, Tag/Nacht Kamera 36x NTSC, Thermalkamera 35mm, 640x512, 25-30Hz, Wischer",20006]
[null,"UCT3NEWA000A","ULISSE COMPACT THERMAL 120Vac, Tag/Nacht Kamera 36x NTSC, Thermalkamera 25mm, 640x512, 7.5-8.3Hz, Wischer",19647]
[null,"UCT3NEWA000AH","ULISSE COMPACT THERMAL 120Vac, Tag/Nacht Kamera 36x NTSC, Thermalkamera 25mm, 640x512, 25-30Hz, Wischer",20006]
[null,"UPK1QAWAN00A","ULISSE RADICAL PTZ, 230Vac, Kamera 18x, Wischer",13408]
[null,"UPK1QEWAN00A","ULISSE RADICAL PTZ, 230Vac, Kamera 33x, mit Thermal Compensation und Visible Cut Filter, Wischer",25605]
[null,"UPK2QAJAN00A","ULISSE RADICAL PTZ, 24Vac, Kamera 18x, Wischer, Halter für Strahler",13408]
[null,"UPK2QEJAN00A","ULISSE RADICAL PTZ, 24Vac, Kamera 33x, mit Thermal Compensation und Visible Cut Filter, Wischer, Halter für Strahler",25605]
[null,"UPK3QAWAN00A","ULISSE RADICAL PTZ, 120Vac, Kamera 18x, Wischer",13408]
[null,"UPK3QEWAN00A","ULISSE RADICAL PTZ, 120Vac, Kamera 33x, mit Thermal Compensation und Visible Cut Filter, Wischer",25605]
[null,"UPKT1AFSA000A","ULISSE RADICAL THERMAL PTZ 230Vac, Thermalkamera optischer Zoom 3x (digital zoom 8x), 640X512, 7.5-8.3Hz",29172]
[null,"UPKT1AFSA000AH","ULISSE RADICAL THERMAL PTZ 230Vac, Thermalkamera optischer Zoom 3x (digital zoom 8x), 640X512, 25-30Hz",29172]
[null,"UPKT1AFSAN00A","ULISSE RADICAL THERMAL PTZ Full IP, H.264, Onvif-S, 230Vac, Thermalkamera optischer Zoom 3x (digital zoom 8x), 640X512, 7.5-8.3Hz",29846]
[null,"UPKT1AFSAN00AH","ULISSE RADICAL THERMAL PTZ Full IP, H.264, Onvif-S, 230Vac, Thermalkamera optischer Zoom 3x (digital zoom 8x), 640X512, 25-30Hz",29846]
[null,"UPKT1BFSA000A","ULISSE RADICAL THERMAL PTZ 230Vac, Thermalkamera optischer Zoom 3x (digital zoom 4x), 336X256, 7.5-8.3Hz",23562]
[null,"UPKT1BFSA000AH","ULISSE RADICAL THERMAL PTZ 230Vac, Thermalkamera optischer Zoom 3x (digital zoom 4x), 336X256, 25-30Hz",23562]
[null,"UPKT1BFSAN00A","ULISSE RADICAL THERMAL PTZ Full IP, H.264, Onvif-S, 230Vac, Thermalkamera optischer Zoom 3x (digital zoom 4x), 336X256, 7.5-8.3Hz",24236]
[null,"UPKT1BFSAN00AH","ULISSE RADICAL THERMAL PTZ Full IP, H.264, Onvif-S, 230Vac, Thermalkamera optischer Zoom 3x (digital zoom 4x), 336X256, 25-30Hz",24236]
[null,"UPKT2AFSA000A","ULISSE RADICAL THERMAL PTZ 24Vac, Thermalkamera optischer Zoom 3x (digital zoom 8x), 640X512, 7.5-8.3Hz",29172]
[null,"UPKT2AFSA000AH","ULISSE RADICAL THERMAL PTZ 24Vac, Thermalkamera optischer Zoom 3x (digital zoom 8x), 640X512, 25-30Hz",29172]
[null,"UPKT2AFSAN00A","ULISSE RADICAL THERMAL PTZ Full IP, H.264, Onvif-S, 24Vac, Thermalkamera optischer Zoom 3x (digital zoom 8x), 640X512, 7.5-8.3Hz",29846]
[null,"UPKT2AFSAN00AH","ULISSE RADICAL THERMAL PTZ Full IP, H.264, Onvif-S, 24Vac, Thermalkamera optischer Zoom 3x (digital zoom 8x), 640X512, 25-30Hz",29846]
[null,"UPKT2BFSA000A","ULISSE RADICAL THERMAL PTZ 24Vac, Thermalkamera optischer Zoom 3x (digital zoom 4x), 336X256, 7.5-8.3Hz",23562]
[null,"UPKT2BFSA000AH","ULISSE RADICAL THERMAL PTZ 24Vac, Thermalkamera optischer Zoom 3x (digital zoom 4x), 336X256, 25-30Hz",23562]
[null,"UPKT2BFSAN00A","ULISSE RADICAL THERMAL PTZ Full IP, H.264, Onvif-S, 24Vac, Thermalkamera optischer Zoom 3x (digital zoom 4x), 336X256, 7.5-8.3Hz",24236]
[null,"UPKT2BFSAN00AH","ULISSE RADICAL THERMAL PTZ Full IP, H.264, Onvif-S, 24Vac, Thermalkamera optischer Zoom 3x (digital zoom 4x), 336X256, 25-30Hz",24236]
[null,"UPKT3AFSA000A","ULISSE RADICAL THERMAL PTZ 120Vac,  Thermalkamera optischer Zoom 3x (digital zoom 8x), 640X512, 7.5-8.3Hz",29172]
[null,"UPKT3AFSA000AH","ULISSE RADICAL THERMAL PTZ 120Vac,  Thermalkamera optischer Zoom 3x (digital zoom 8x), 640X512, 25-30Hz",29172]
[null,"UPKT3AFSAN00A","ULISSE RADICAL THERMAL PTZ Full IP, H.264, Onvif-S, 120Vac,  Thermalkamera optischer Zoom 3x (digital zoom 8x), 640X512, 7.5-8.3Hz",29846]
[null,"UPKT3AFSAN00AH","ULISSE RADICAL THERMAL PTZ Full IP, H.264, Onvif-S, 120Vac,  Thermalkamera optischer Zoom 3x (digital zoom 8x), 640X512, 25-30Hz",29846]
[null,"UPKT3BFSA000A","ULISSE RADICAL THERMAL PTZ 120Vac,  Thermalkamera optischer Zoom 3x (digital zoom 4x), 336X256, 7.5-8.3Hz",23562]
[null,"UPKT3BFSA000AH","ULISSE RADICAL THERMAL PTZ 120Vac,  Thermalkamera optischer Zoom 3x (digital zoom 4x), 336X256, 25-30Hz",23562]
[null,"UPKT3BFSAN00A","ULISSE RADICAL THERMAL PTZ Full IP, H.264, Onvif-S, 120Vac,  Thermalkamera optischer Zoom 3x (digital zoom 4x), 336X256, 7.5-8.3Hz",24236]
[null,"UPKT3BFSAN00AH","ULISSE RADICAL THERMAL PTZ Full IP, H.264, Onvif-S, 120Vac,  Thermalkamera optischer Zoom 3x (digital zoom 4x), 336X256, 25-30Hz",24236]
[null,"UPT1PVSA000E","ULISSE 230Vac, 36x Tag/Nacht Kamera, PAL",4208]
[null,"UPT1PVWA000E","ULISSE 230Vac, 36x Tag/Nacht Kamera, PAL, Wischer",4556]
[null,"UPT1SLGA000E","ULISSE MAXI for analog Thermalkamera, 230Vac, Wischer",9044]
[null,"UPT1SLGAN00E","ULISSE MAXI for thermal network Kamera 230Vac, Wischer",9549]
[null,"UPT1SLWA000E","ULISSE MAXI for analog Kamera, 230Vac, Wischer",5835]
[null,"UPT1SLWAN00E","ULISSE MAXI for network Kamera 230Vac, Wischer",6340]
[null,"UPT1SMWA000E","ULISSE PLUS for analog Kamera, 230Vac, Wischer",4376]
[null,"UPT1SMWAN00E","ULISSE PLUS for network Kamera 230Vac, Wischer",4881]
[null,"UPT1SVGA000E","ULISSE für analoge Thermal Kamera 230Vac",4595]
[null,"UPT1SVGAN00E","ULISSE für Netzwerk Thermall Kamera 230Vac",5100]
[null,"UPT1SVSA000E","ULISSE für analoge Kamera 230Vac",2862]
[null,"UPT1SVSAN00E","ULISSE für Netzwerk Kamera 230Vac",3366]
[null,"UPT1SVWA000E","ULISSE für analoge Kamera 230Vac, Wischer",3209]
[null,"UPT1SVWAN00E","ULISSE für Netzwerk Kamera 230Vac, Wischer",3714]
[null,"UPT2MVJA000E","ULISSE 24Vac, 28x Tag/Nacht Kamera, NTSC, Wischer, Halter für LED Strahler",4640]
[null,"UPT2MVKA000E","ULISSE 24Vac, 28x Tag/Nacht Kamera, NTSC, Halter für LED Strahler",4292]
[null,"UPT2NVJA000E","ULISSE 24Vac, 36x Tag/Nacht Kamera, NTSC, Wischer, Halter für LED Strahler",4780]
[null,"UPT2NVKA000E","ULISSE 24Vac, 36x Tag/Nacht Kamera, NTSC, Halter für LED Strahler",4432]
[null,"UPT2NVSA000E","ULISSE 24Vac, 36x Tag/Nacht Kamera, NTSC",4208]
[null,"UPT2NVWA000E","ULISSE 24Vac, 36x Tag/Nacht Kamera, NTSC, Wischer",4556]
[null,"UPT2PVJA000E","ULISSE 24Vac, 36x Tag/Nacht Kamera, PAL, Wischer, Halter für LED Strahler",4780]
[null,"UPT2PVKA000E","ULISSE 24Vac, 36x Tag/Nacht Kamera, PAL, Halter für LED Strahler",4432]
[null,"UPT2PVSA000E","ULISSE 24Vac, 36x Tag/Nacht Kamera, PAL",4208]
[null,"UPT2PVWA000E","ULISSE 24Vac, 36x Tag/Nacht Kamera, PAL, Wischer",4556]
[null,"UPT2QVJA000E","ULISSE 24Vac, 28x Tag/Nacht Kamera, PAL, Wischer, Halter für LED Strahler",4640]
[null,"UPT2QVKA000E","ULISSE 24Vac, 28x Tag/Nacht Kamera, PAL, Halter für LED Strahler",4292]
[null,"UPT2SLGA000E","ULISSE MAXI for analog Thermalkamera, 24Vac, Wischer",9044]
[null,"UPT2SLGAN00E","ULISSE MAXI for network Thermalkamera, 24Vac, Wischer",9549]
[null,"UPT2SLJA000E","ULISSE MAXI for analog Kamera, 24Vac, Wischer, Halter für LED Strahler",5835]
[null,"UPT2SLJAN00E","ULISSE MAXI for network Kamera, 24Vac, Wischer, Halter für LED Strahler",6340]
[null,"UPT2SMJA000E","ULISSE PLUS for analog Kamera, 24Vac, Wischer, Halter für LED Strahler",4679]
[null,"UPT2SMJAN00E","ULISSE PLUS for network Kamera 24Vac, Wischer, Halter für LED Strahler",5184]
[null,"UPT2SMWA000E","ULISSE PLUS for analog Kamera, 24Vac, Wischer",4376]
[null,"UPT2SMWAN00E","ULISSE PLUS for network Kamera 24Vac, Wischer",4881]
[null,"UPT2SVGA000E","ULISSE for analog Thermalkamera, 24Vac",4595]
[null,"UPT2SVGAN00E","ULISSE for thermal network Kamera, 24Vac",5100]
[null,"UPT2SVJA000E","ULISSE for analog Kamera, 24Vac, Wischer, Halter für LED Strahler",3434]
[null,"UPT2SVJAN00E","ULISSE for network Kamera, 24Vac, Wischer, Halter für LED Strahler",4017]
[null,"UPT2SVKA000E","ULISSE for analog Kamera, 24Vac, Halter für LED Strahler",3086]
[null,"UPT2SVKAN00E","ULISSE for network Kamera, 24Vac, Halter für LED Strahler",3669]
[null,"UPT2SVSA000E","ULISSE for analog Kamera, 24Vac",2862]
[null,"UPT2SVSAN00E","ULISSE for network Kamera, 24Vac",3366]
[null,"UPT2SVWA000E","ULISSE for analog Kamera, 24Vac, Wischer",3209]
[null,"UPT2SVWAN00E","ULISSE for network Kamera 24Vac, Wischer",3714]
[null,"UPT3NVSA000E","ULISSE 120Vac, 36x Tag/Nacht Kamera, NTSC",4208]
[null,"UPT3NVWA000E","ULISSE 120Vac, 36x Tag/Nacht Kamera, NTSC, Wischer",4556]
[null,"UPT3SLGA000E","ULISSE MAXI for analog Thermalkamera, 120Vac, Wischer",9044]
[null,"UPT3SLGAN00E","ULISSE MAXI for network Thermalkamera, 120Vac, Wischer",9549]
[null,"UPT3SLWA000E","ULISSE MAXI for analog Kamera, 120Vac, Wischer",5835]
[null,"UPT3SLWAN00E","ULISSE MAXI for network Kamera 120Vac, Wischer",6340]
[null,"UPT3SMWA000E","ULISSE PLUS for analog Kamera, 120Vac, Wischer",4376]
[null,"UPT3SMWAN00E","ULISSE PLUS for network Kamera 120Vac, Wischer",4881]
[null,"UPT3SVGA000E","ULISSE for analog Thermalkamera, 120Vac",4595]
[null,"UPT3SVGAN00E","ULISSE for thermal network Kamera, 120Vac",5100]
[null,"UPT3SVSA000E","ULISSE 120Vac",2862]
[null,"UPT3SVSAN00E","ULISSE for network Kamera, 120Vac",3366]
[null,"UPT3SVWA000E","ULISSE 120Vac, Wischer",3209]
[null,"UPT3SVWAN00E","ULISSE for network Kamera 120Vac, Wischer",3714]
[null,"UPTHT1","Reinforced Heizung für ULISSE mit generic lens/Kameras",139]
[null,"UPTHT2","Reinforced Heizung für ULISSE mit integrated block Kamera",139]
[null,"UPTIRN108A00","LED Strahler for ULISSE 10° 850nm, 24Vac - 12/24Vdc",509]
[null,"UPTIRN109A00","LED Strahler for ULISSE 10°, 940nm, 24Vac - 12/24Vdc",821]
[null,"UPTIRN10WA00","LED Strahler for ULISSE, Weißlicht 10°, 24Vac-12/24Vdc",509]
[null,"UPTIRN308A00","LED Strahler for ULISSE 30° 850nm, 24Vac - 12/24Vdc",509]
[null,"UPTIRN309A00","LED Strahler for ULISSE 30°, 940nm, 24Vac - 12/24Vdc",821]
[null,"UPTIRN30WA00","LED Strahler for ULISSE, Weißlicht 30°, 24Vac-12/24Vdc",509]
[null,"UPTIRN608A00","LED Strahler for ULISSE 60° 850nm, 24Vac - 12/24Vdc",509]
[null,"UPTIRN60WA00","LED Strahler for ULISSE, Weißlicht 60°, 24Vac-12/24Vdc",509]
[null,"UPTIRPS100N","Sensor und  Netzteil for ULISSE mit Strahler, IN 100Vac in waterproof metal box",405]
[null,"UPTIRPS120UL","Sensor und  Netzteil for ULISSE mit Strahler, IN 120Vac in waterproof metal box (UL certified)",509]
[null,"UPTIRPS230N","Sensor und  Netzteil for ULISSE mit Strahler, IN 230Vac in waterproof metal box",405]
[null,"UPTJBUL","UL junction weatherproof box",226]
[null,"UPTWBA","Wandhalterung mit internal cable channel",104]
[null,"UPTWBTAB","Parapet bracket mit internal cable channel",104]
[null,"USB485","USB-RS485 converter for PC connection of control keyboard DCJ und DCT",47]
[null,"VA01002","ALBERT digital encoder for intelligent video content analysis, 1 video channel H264, bidirectional audio, bidirectional RS485/RS422, alarm inputs/outputs, SD slot",1502]
[null,"VA03002","ALBERT digital encoder for intelligent video content analysis, 1 video channel, H264, bidirectional audio, bidirectional RS485/RS422, alarm inputs/outputs, SD slot und 40GB Industrial Hard Disk for H264 recording",1964]
[null,"VD18T1","Video distributor 1 input / 8 outputs",163]
[null,"VD48P1","Programmable video distributor 4 inputs / 8 outputs",203]
[null,"VD816PR1","Programmable video distributor 8 inputs / 16 outputs, rack version",382]
[null,"VIP6A1","Wischer kit 230Vac",426]
[null,"VIP6A2","Wischer kit 24Vac",426]
[null,"VIPNX1C","Edelstahl- Wischer 230Vac",789]
[null,"VIPNX2C","Edelstahl- Wischer 24Vac",789]
[null,"VIPNXL1C","Edelstahl- Wischer 230Vac",789]
[null,"VIPNXL2C","Edelstahl- Wischer 24Vac",789]
[null,"WAS0V23L11M00","Tank 23l (6gal), IN 230Vac-24Vac-120Vac washer pump, delivery up to 11m (36ft)",636]
[null,"WAS0V23L5M00","Tank 23l (6gal), IN 230Vac-24Vac-120Vac Wischerpumpe für bis zu 5m (16ft)",439]
[null,"WAS0V5L5M00","Tank 5l (1.3gal), IN 230Vac-24Vac-120Vac Wischerpumpe für bis zu 5m (16ft)",393]
[null,"WAS1V23L30M00","Tank 23l (6gal), IN 230Vac Wischerpumpe für bis zu 30m (98ft) mit water float",1202]
[null,"WAS3V23L30M00","Tank 23l (6gal), IN 120Vac Wischerpumpe für bis zu 30m (98ft) mit water float",1202]
[null,"WASPT0V23L11M00","Tank 23l (6gal), IN 230Vac-24Vac-120Vac washer pump, delivery up to 11m (36ft), mit water float",855]
[null,"WASPT0V23L5M00","Tank 23l (6gal), IN 230Vac-24Vac-120Vac Wischerpumpe für bis zu 5m (16ft)",555]
[null,"WASPT0V5L5M00","Tank 5l (1.3gal), IN 230Vac-24Vac-120Vac Wischerpumpe für bis zu 5m (16ft)",520]
[null,"WASPT1V23L30M00","Tank 23l (6gal), IN 230Vac Wischerpumpe für bis zu 30m (98ft) mit water float",1479]
[null,"WASPT3V23L30M00","Tank 23l (6gal), IN 120Vac Wischerpumpe für bis zu 30m (98ft) mit water float",1479]
[null,"WBCLA","Technopolymer wall/ceiling Kamera bracket, RAL9002",7]
[null,"WBJA","Gehäuse Wandhalterung mit ball joint",19]
[null,"WBLA","Wandhalterung for HGV Gehäuse mit ball joint in non-corrosive sturdy anticorodal aluminium alloy",590]
[null,"WBMA","Gehäuse Wandhalterung mit ball joint",19]
[null,"WBOV3A2","WBOVA2 Wandhalterung mit support plate und integrated junction box mit internal cable channel",152]
[null,"WBOVA2","Wandhalterung mit interner Kabelführung (HOT, HOV, HEB, HEK, VERSO, VERSO Compact)",28]
[null,"WCM3A","Deckenhalterung mit ball joint",62]
[null,"WCM4A2","Deckenhalterung mit internal cable channel",88]
[null,"WCM5A","Deckenhalterung mit ball joint",99]
[null,"WCMPA","Extension for WCM4A2 und WCM5A brackets, 500mm (20in)",27]
[null,"WCPA","Wandhalterung adaptor plate",31]
[null,"WCWA","Corner mount adaptor",48]
[null,"WCWGC","Corner adaptor",79]
[null,"WFWBTA","Column Halter für PTH P&T series",52]
[null,"WFWCA","Column mount mit ball joint for Gehäuse",81]
[null,"WSFPA","Pole mount adaptor Ø from 65mm to 110mm (2.5in - 4.3in)",55]

{"sheet":"NVT","index":8,"n_rows":103,"n_cols":4,"rows_kept":103,"cut":false,"hidden":false,"merged":[]}
["NVT / Übertragung"]
[]
[]
[null,"Modell","Beschreibung","EURO"]
["EoC System "]
[null,"NV-EC1701","Single Channel EoC Transceiver (power supply not included)",370]
["EoC System Kits"]
[null,"NV-EC1701-KIT1","1 - Camera EoC Transmission System; (2) NV-EC1701 & (1) NV-PS48-60W, (1) NV-PC4PR, (1) NV-PC2PR",825]
[null,"NV-EC1701-KIT2","2 - Camera EoC Transmission System; (3) NV-EC1701 & (1) NV-PS48-60W & (1) NV-BNCT, (2) NV-PC4PR, (1) NV-PC2PR",1202.5]
[null,"NV-EC1701-KIT3","3 - Camera EoC Transmission System; (4) NV-EC1701 & (1) NV-PS48-60W & (1) NV-EC4BNC, (3) NV-PC4PR, (1) NV-PC2PR ",1582.5]
[null,"NV-EC1701-KIT4","4 - Camera EoC Transmission System; (5) NV-EC1701 & (1) NV-PS48-60W & (1) NV-EC4BNC, (4) NV-PC4PR, (1) NV-PC2PR  ",1962.5]
["Eo2 Transceiver"]
[null,"NV-EC1701U","Single Channel Eo2 Transceiver (power supply not included)",370]
["Eo2 System Kits"]
[null,"NV-EC1701U-KIT1","1 - Camera Eo2 Transmission System; (2) NV-EC1701U & (1) NV-PS48-60W, (1) NV-PC4PR, (1) NV-PC2PR",825]
[null,"NV-EC1701U-KIT2","2 - Camera Eo2Transmission System; (3) NV-EC1701U & (1) NV-PS48-60W &  (2) NV-PC4PR, (1) NV-PC2PR",1202.5]
[null,"NV-EC1701U-KIT3","3 - Camera Eo2 Transmission System; (4) NV-EC1701U & (1) NV-PS48-60W &  (3) NV-PC4PR, (1) NV-PC2PR ",1582.5]
[null,"NV-EC1701U-KIT4","4 - Camera Eo2 Transmission System; (5) NV-EC1701U & (1) NV-PS48-60W &  (4) NV-PC4PR, (1) NV-PC2PR  ",1962.5]
["Accessories"]
[null,"NV-PS48-60W","48VDC power supply, 60 watts with IEC line cord",77.5]
[null,"NV-PS56-60W","56VDC Power Supply, 60 watts with IEC line cord",100]
[null,"NV-PS56-90W","56VDC Power Supply, 90 watts with IEC line cord",120]
[null,"NV-PC4PR","RJ45 Patch Cord, 4-pair 3' (1m) Grey",7.5]
[null,"NV-PC2PR","RJ45 Patch Cord, 2-pair 3' (1m) Red",7.5]
[null,"NV-BNCT","BNC \"T\" Adaptor",7.5]
[null,"NV-RM8/10","Rack mount kit, 19\" X 2U, holds up to (4) NV-EC1701 transceivers",57.5]
[null,"NV-RMEC16","EoC Rack Mount Tray Kit - up to (4) NV-EC1701 Transceivers w/Power Supplies (not included)",195]
[null,"NV-RMEC16U","Eo2 Rack Mount Tray Kit - up to (4) NV-EC1701U Transceivers w/Power Supplies (not included)",195]
[null,"NV-DPSC4","Detachable Power Supply Cord Splitter 1:4 x 2ft",20]
[null,"NV-EC4BNC","BNC Coax Splitter 1:4",20]
[]
[]
["Passive Transceiver"]
[null,"NV-213A (&A-M)","Passive Video Transceiver",160]
[null,"NV-208A-M","Passive Video Transceiver",65]
[null,"NV-214A-M","Passive Video Transceiver",65]
[null,"NV-215J-M","Passive Video Transceiver with RJ45",65]
[null,"NV-217J-M","Passive Video Transceiver with RJ45",65]
["Active Receiver/Transmitter",null,""]
[null,"NV-652R","Active Video Receiver *",280]
[null,"NV-653T","Active Video Transmitter *",275]
[null,null,""]
[null,"NV-413A","4-Ch Passive Video Transceiver",485]
[null,"NV-452R","4-Ch Active Video Receiver *",975]
["Passive Hub",null,""]
[null,"NV-813","8-Channel Passive Hub ▲",1135]
[null,"NV-813S","8-Channel  Passive Stub Hub ►",635]
[null,"NV-1613","16-Channel Passive Hub ▲",2198]
[null,"NV-1613S","16-Channel  Passive Stub Hub ►",1223]
[null,"NV-3213","32-Channel Passive Hub ▲",4030]
[null,"NV-3213S","32-Channel  Passive Stub Hub ►",2358]
["Active Hub",null,""]
[null,"NV-442","4-Channel Active StubEQ Receiver Hub †",990]
[null,"NV-842","8-Channel DigitalEQ Stub Hub † ►",1250]
[null,"NV-1642","16-Channel DigitalEQ Stub Hub † ►",2418]
[null,"NV-3242","32-Channel DigitalEQ Stub Hub † ►",4438]
[null,"NV-872","8-Channel DigitalEQ Hub †▲",1933]
[null,"NV-1672","16-Channel DigitalEQ Hub †▲",3730]
[null,"NV-3272","32-Channel DigitalEQ Hub †▲",6845]
["Power, Video, Data",null,""]
[null,"NV-216A-PV","Power-Video Transceiver ",80]
[null,"NV-218A-PVD","Power-Video-Data Transceiver ",127.5]
[null,"NV-226J-PV","Video Transmitter & 12VDC Converter †",155]
[null,"NV-4PS10- PVD","Power Supply Cable Integrator Hub †",408]
[null,"NV-16PS10-PVD","Power Supply Cable Integrator Hub †",1233]
[null,"NV-4PS13-PVD","Power Supply Passive Receiver Hub †►",865]
[null,"NV-8PS13-PVD","Power Supply Passive Receiver Hub †▲",1733]
[null,"NV-16PS13-PVD","Power Supply Passive Receiver Hub †▲",3465]
[null,"NV-8PS42-PVD","8-Channel Power Supply StubEQ Active Receiver Hub †",1818]
[null,"NV-16PS42-PVD","16-Channel Power Supply StubEQ Active Receiver Hub †",35963]
[null,"NV-32PS42-PVD","32-Channel Power Supply StubEQ Active Receiver Hub †",6968]
[null,"NV-704J-PVD","4-Ch PVD Cable Integrator *",185]
[null,"NV-716J-PVD","16-Ch PVD Cable Integrator *",340]
["Multimedia",null,""]
[null,"NV-314A","Passive Video & Audio Transceiver",250]
[null,"NV-418A","Dual Passive AV Transceiver",322]
[null,"NV-418AR","Dual Passive AV Transceiver, Rackmt",322]
[null,"NV-518A ","Dual AV Transceiver *",588]
[null,"NV-518AR","Dual AV Transceiver, Rackmt ",588]
[null,"NV-RM-15","Rackmount Chassis †",933]
["Accessories",null,""]
[null,"NV-4PSRMBK","Rack Panel Kit for 4 Port Power Supply Product",65]
[null,"NV-BKT214-8","Mounting Bracket for 8 NV-214AM's",15]
[null,"NV-BNC-8","Coax Jumper Cables 2ft (8-pack)",65]
[null,"NV-RJ45A","RJ45/Screw Terminal Block Adapter (2 each)",10]
[null,"NV-RM8/10","Rack Panel Kit",65]
[null,"NV-RMBK","Rear Mounting Bracket Kit",65]
[null,"NV-WMBK","Wall Mounting Bracket Kit",65]
[]
["Transmission IP - Other"]
[null,"IP01","IP Extender over Coax - Passive type (2 pieces/one set package)",61]
[null,"IP01H","4 port Ethernet Switch Kit (over coax, BNC interface)  (power adapter included)",182]
[null,"IP01K","4 x IP01+1 x IP01H 5 port Ethernet Switch Kit (over coax, BNC interface)",279]
[null,"IP01P","POE Extender over Coax 300M  (Package without POE switch/injector)",182]
[null,"IP02P","IP Extender with Power over Coax 180M, including TX x1, RX x 1 (power adapter included)",291]
[null,"IP02","Active IP Extender over Coax,  including TX x1, RX x1 (power adapter included)",412]
[null,"IP03","Active IP Extender over CAT5,  including TX x1, RX x1 (power adapter included)",412]
[null,"IP03P","Internet and POE or UTP, Coax, telefone, bell, alarm / power Cabels",460]
[null,"IP04","POE Repeater 300Meters",121]
[null,"IP07M","Chainable IP Extender with Power over Coax/Two Wire IP07M x 1 unit",158]
[null,"IP07MK-DC24V","Chainable IP Extender IP07M x 2 units with 1 x DC24V power adapter",339]
[null,"IP07MK-DC48V","Chainable IP Extender IP07M x 2 units with 1 x DC48V power adapter",351]
[null,"IP07MK-DC56V","Chainable IP Extender IP07M x 2 units with 1 x DC56V power adapter",400]